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SECTION 1: Identification of the substance/mixture and of the company/undertaking
1.1. Product identifier
	Product form
	:
	Mixture

	Product name
	:
	MILK & HONEY #EU24302F 25% in DPG

	Product code
	:
	EU24302F_25%

	Type of product
	:
	Perfumes, fragrances


1.2. Relevant identified uses of the substance or mixture and uses advised against
1.2.1. Relevant identified uses
	Industrial/Professional use spec
	:
	Industrial
For professional use only

	Use of the substance/mixture
	:
	Perfumes, fragrances

	Function or use category
	:
	Odour agents


1.2.2. Uses advised against
No additional information available
1.3. Details of the supplier of the safety data sheet
No additional information available
1.4. Emergency telephone number
No additional information available
SECTION 2: Hazards identification
2.1. Classification of the substance or mixture
Classification according to Regulation (EC) No. 1272/2008 [CLP]
	Skin sensitisation, Category 1
	H317 
	
	

	Hazardous to the aquatic environment – Chronic Hazard, Category 3
	H412 
	
	


Full text of H- and EUH-statements: see section 16
Adverse physicochemical, human health and environmental effects
No additional information available
2.2. Label elements
Labelling according to Regulation (EC) No. 1272/2008 [CLP]
	Hazard pictograms (CLP)
	:
	[image: ]
	
	
	
	
	

	
	
	GHS07
	
	
	
	
	

	Signal word (CLP)
	:
	Warning

	Contains
	:
	Benzyl salicylate; 3-(2,2-dimethyl-3-hydroxypropyl)toluene; (alt.): 2,2-dimethyl-3-(3-methylphenyl)propanol; isoeugenol

	Hazard statements (CLP)
	:
	H317 - May cause an allergic skin reaction.
H412 - Harmful to aquatic life with long lasting effects.

	Precautionary statements (CLP)
	:
	P261 - Avoid breathing dust/fume/gas/mist/vapours/spray.
P272 - Contaminated work clothing should not be allowed out of the workplace.
P273 - Avoid release to the environment.
P280 - Wear protective gloves/protective clothing/eye protection/face protection/hearing protection.
P302+P352 - IF ON SKIN: Wash with plenty of water.
P321 - Specific treatment (see supplemental first aid instruction on this label).

	Extra phrases
	:
	Restricted to professional users.
For professional users only.


2.3. Other hazards
	Contains no PBT and/or vPvB substances ≥ 0.1% assessed in accordance with REACH Annex XIII



	The mixture does not contain substance(s) included in the list established in accordance with Article 59(1) of REACH for having endocrine disrupting properties, or substance(s) are not identified as having endocrine disrupting properties in accordance with the criteria set out in Commission Delegated Regulation (EU) 2017/2100 or Commission Regulation (EU) 2018/605 at a concentration equal to or greater than 0,1 %



SECTION 3: Composition/information on ingredients
3.1. Substances
Not applicable
3.2. Mixtures
	Name
	Product identifier
	%
	Classification according to Regulation (EC) No. 1272/2008 [CLP]

	benzyl benzoate
	CAS-No.: 120-51-4
EC-No.: 204-402-9
EC Index-No.: 607-085-00-9
REACH-no: 01-2119976371-33
	8.125 – 16.225
	Acute Tox. 4 (Oral), H302
Aquatic Acute 1, H400
Aquatic Chronic 2, H411

	Verdox
	CAS-No.: 88-41-5
EC-No.: 201-828-7
REACH-no: 01-2119970713-33
	1 – 2
	Aquatic Chronic 2, H411

	Benzyl salicylate
	CAS-No.: 118-58-1
EC-No.: 204-262-9
EC Index-No.: 607-754-00-5
REACH-no: 01-2119969442-31
	1 – 2
	Eye Irrit. 2, H319
Skin Sens. 1B, H317
Aquatic Chronic 3, H412

	3-(2,2-dimethyl-3-hydroxypropyl)toluene; (alt.): 2,2-dimethyl-3-(3-methylphenyl)propanol
	CAS-No.: 103694-68-4
EC-No.: 403-140-4
EC Index-No.: 603-138-00-5
	0.00575 – 1.15
	Skin Sens. 1, H317
Aquatic Chronic 3, H412

	Carbitol
substance with national workplace exposure limit(s) (AT, DE, EE, SE, SI, CH)
	CAS-No.: 111-90-0
EC-No.: 203-919-7
REACH-no: 01-2119475105-42
	0.4158975 – 0.831795
	Not classified

	benzaldehyde
substance with national workplace exposure limit(s) (BG, FI, HU, LT, LV, PL)
	CAS-No.: 100-52-7
EC-No.: 202-860-4
EC Index-No.: 605-012-00-5
REACH-no: 01-2119455540-44
	0.2 – 0.375
	Acute Tox. 4 (Oral), H302

	Sandal Mysore Core
	CAS-No.: 28219-60-5
EC-No.: 248-907-2
	0.075 – 0.125
	Skin Irrit. 2, H315
Eye Irrit. 2, H319
Aquatic Acute 1, H400
Aquatic Chronic 1, H410

	isoeugenol
	CAS-No.: 97-54-1
EC-No.: 202-590-7
EC Index-No.: 604-094-00-X; 202-590-1
REACH-no: 17-2119417630-49
	0.025 – 0.05
	Acute Tox. 4 (Oral), H302
Acute Tox. 4 (Dermal), H312
Acute Tox. 4 (Inhalation), H332
Skin Irrit. 2, H315
Eye Irrit. 2, H319
Skin Sens. 1A, H317
Carc. 2, H351
STOT SE 3, H335

	Ethyl benzoate
substance with national workplace exposure limit(s) (RO)
	CAS-No.: 93-89-0
EC-No.: 202-284-3
	0.025 – 0.025
	Not classified

	ethanol; ethyl alcohol
substance with national workplace exposure limit(s) (AT, BE, BG, CZ, DE, DK, EE, ES, FI, FR, GB, GR, HR, HU, IE, LT, LV, NL, PL, PT, RO, SE, SI, SK, NO, CH, TR)
	CAS-No.: 64-17-5
EC-No.: 200-578-6
EC Index-No.: 603-002-00-5
	0.025 – 0.025
	Flam. Liq. 2, H225

	acetaldehyde; ethanal
substance with national workplace exposure limit(s) (AT, BE, BG, CZ, DE, DK, EE, ES, FI, FR, GB, GR, HR, HU, IE, LT, LV, NL, PL, PT, RO, SE, SI, SK, NO, CH)
	CAS-No.: 75-07-0
EC-No.: 200-836-8
EC Index-No.: 605-003-00-6
	0.025 – 0.025
	Flam. Liq. 1, H224
Acute Tox. 4 (Oral), H302
Eye Irrit. 2, H319
Muta. 2, H341
Carc. 1B, H350
STOT SE 3, H335

	.alpha.-Pinene
substance with national workplace exposure limit(s) (BE, EE, ES, LT, PT, SE, NO)
	CAS-No.: 80-56-8
EC-No.: 201-291-9
	0.0025 – 0.00625
	Flam. Liq. 3, H226
Acute Tox. 4 (Oral), H302
Skin Irrit. 2, H315
Skin Sens. 1B, H317
Asp. Tox. 1, H304
Aquatic Acute 1, H400
Aquatic Chronic 1, H410

	.beta.-Pinene
substance with national workplace exposure limit(s) (BE, EE, ES, LT, PT, SE, NO)
	CAS-No.: 127-91-3
EC-No.: 204-872-5
	0.0025 – 0.00625
	Flam. Liq. 3, H226

	(R)-p-mentha-1,8-diene; d-limonene
substance with national workplace exposure limit(s) (DE, ES, FI, SI, NO, CH)
	CAS-No.: 5989-27-5
EC-No.: 205-341-0
EC Index-No.: 601-096-00-2
REACH-no: 01-2119493353-35
	0.00125 – 0.0025
	Flam. Liq. 3, H226
Skin Irrit. 2, H315
Skin Sens. 1B, H317
Asp. Tox. 1, H304
Aquatic Acute 1, H400
Aquatic Chronic 3, H412

	p-Cymene
substance with national workplace exposure limit(s) (DK, EE, LT, LV, SE)
	CAS-No.: 99-87-6
EC-No.: 202-796-7
EC Index-No.: 601-094-00-1
	0.00025 – 0.00125
	Flam. Liq. 3, H226
Acute Tox. 3 (Inhalation), H331
Acute Tox. 3 (Inhalation:dust,mist), H331
Repr. 2, H361
Asp. Tox. 1, H304
Aquatic Chronic 2, H411



	Specific concentration limits:

	Name
	Product identifier
	Specific concentration limits (%)

	isoeugenol
	CAS-No.: 97-54-1
EC-No.: 202-590-7
EC Index-No.: 604-094-00-X; 202-590-1
REACH-no: 17-2119417630-49
	(0.01 ≤ C ≤ 100) Skin Sens. 1A, H317


Full text of H- and EUH-statements: see section 16
SECTION 4: First aid measures
4.1. Description of first aid measures
	First-aid measures general
	:
	Never give anything by mouth to an unconscious person. If you feel unwell, seek medical advice (show the label where possible).

	First-aid measures after inhalation
	:
	Allow affected person to breathe fresh air. Allow the victim to rest.

	First-aid measures after skin contact
	:
	Remove affected clothing and wash all exposed skin area with mild soap and water, followed by warm water rinse.

	First-aid measures after eye contact
	:
	Rinse immediately with plenty of water. Obtain medical attention if pain, blinking or redness persists.

	First-aid measures after ingestion
	:
	Rinse mouth. Do NOT induce vomiting. Obtain emergency medical attention.


4.2. Most important symptoms and effects, both acute and delayed
	Symptoms/effects
	:
	Not expected to present a significant hazard under anticipated conditions of normal use.


4.3. Indication of any immediate medical attention and special treatment needed
No additional information available
SECTION 5: Firefighting measures
5.1. Extinguishing media
	Suitable extinguishing media
	:
	Foam. Dry powder. Carbon dioxide. Water spray. Sand.

	Unsuitable extinguishing media
	:
	Do not use a heavy water stream.


5.2. Special hazards arising from the substance or mixture
No additional information available
5.3. Advice for firefighters
	Firefighting instructions
	:
	Use water spray or fog for cooling exposed containers. Exercise caution when fighting any chemical fire. Prevent fire fighting water from entering the environment.

	Protection during firefighting
	:
	Do not enter fire area without proper protective equipment, including respiratory protection.


SECTION 6: Accidental release measures
6.1. Personal precautions, protective equipment and emergency procedures
6.1.1. For non-emergency personnel
	Emergency procedures
	:
	Evacuate unnecessary personnel.


6.1.2. For emergency responders
	Protective equipment
	:
	Equip cleanup crew with proper protection.

	Emergency procedures
	:
	Ventilate area.


6.2. Environmental precautions
Prevent entry to sewers and public waters. Notify authorities if liquid enters sewers or public waters.
6.3. Methods and material for containment and cleaning up
	Methods for cleaning up
	:
	Soak up spills with inert solids, such as clay or diatomaceous earth as soon as possible. Collect spillage. Store away from other materials.


6.4. Reference to other sections
See Section 8. Exposure controls and personal protection.
SECTION 7: Handling and storage
7.1. Precautions for safe handling
	Precautions for safe handling
	:
	Wash hands and other exposed areas with mild soap and water before eating, drinking or smoking and when leaving work. Provide good ventilation in process area to prevent formation of vapour.


7.2. Conditions for safe storage, including any incompatibilities
	Storage conditions
	:
	Keep only in the original container in a cool, well ventilated place away from : Keep container closed when not in use.

	Incompatible products
	:
	Strong bases. Strong acids.

	Incompatible materials
	:
	Sources of ignition. Direct sunlight.

	Germany

	Storage class (LGK, TRGS 510)
	:
	LGK 12 - Non-combustible liquids

	Joint storage table
	:
	[image: ]

	Joint storage not permitted for
	:
	LGK 1, LGK 6.2, LGK 7

	Joint storage with restrictions permitted for
	:
	LGK 4.1A, LGK 4.3, LGK 5.1C

	Joint storage permitted for
	:
	LGK 2A, LGK 2B, LGK 3, LGK 4.1B, LGK 4.2, LGK 5.1A, LGK 5.1B, LGK 5.2, LGK 6.1A, LGK 6.1B, LGK 6.1C, LGK 6.1D, LGK 8A, LGK 8B, LGK 10, LGK 11, LGK 12, LGK 13, LGK 10-13

	Switzerland

	Storage class (LK)
	:
	LK 10/12 - Liquids


7.3. Specific end use(s)
No additional information available
SECTION 8: Exposure controls/personal protection
8.1. Control parameters
[bookmark: _Hlk54076387]8.1.1 National occupational exposure and biological limit values

	Carbitol (111-90-0)

	Austria - Occupational Exposure Limits

	MAK (OEL TWA)
	35 mg/m³

	MAK (OEL TWA)
	6 ppm

	MAK (OEL STEL)
	140 mg/m³

	MAK (OEL STEL)
	24 ppm

	Estonia - Occupational Exposure Limits

	OEL TWA
	50.1 mg/m³

	OEL TWA
	10 ppm

	OEL chemical category
	Skin notation

	Germany - Occupational Exposure Limits (TRGS 900)

	AGW (OEL TWA)
	35 mg/m³ (the risk of damage to the embryo or fetus can be excluded when AGW and BGW values are observed)

	AGW (OEL TWA)
	6 ppm (the risk of damage to the embryo or fetus can be excluded when AGW and BGW values are observed)

	Slovenia - Occupational Exposure Limits

	OEL TWA
	35 mg/m³

	OEL TWA
	6 ppm

	OEL STEL
	70 mg/m³

	OEL STEL
	12 ppm

	Sweden - Occupational Exposure Limits

	NGV (OEL TWA)
	80 mg/m³

	NGV (OEL TWA)
	15 ppm

	KGV (OEL STEL)
	170 mg/m³

	KGV (OEL STEL)
	30 ppm

	OEL chemical category
	Skin notation

	Switzerland - Occupational Exposure Limits

	MAK (OEL TWA)
	50 mg/m³ (aerosol, inhalable dust, vapour)

	KZGW (OEL STEL)
	100 mg/m³ (aerosol, inhalable dust, vapour)



	benzaldehyde (100-52-7)

	Bulgaria - Occupational Exposure Limits

	OEL TWA
	5 mg/m³

	Finland - Occupational Exposure Limits

	HTP (OEL TWA)
	4.4 mg/m³

	HTP (OEL TWA)
	1 ppm

	HTP (OEL C)
	17.4 mg/m³

	HTP (OEL C)
	4 ppm

	Hungary - Occupational Exposure Limits

	AK (OEL TWA)
	5 mg/m³

	CK (OEL STEL)
	10 mg/m³

	Latvia - Occupational Exposure Limits

	OEL TWA
	5 mg/m³

	Lithuania - Occupational Exposure Limits

	IPRV (OEL TWA)
	5 mg/m³

	Poland - Occupational Exposure Limits

	NDS (OEL TWA)
	10 mg/m³

	NDSCh (OEL STEL)
	40 mg/m³



	.alpha.-Pinene (80-56-8)

	Belgium - Occupational Exposure Limits

	OEL TWA
	20 ppm

	Estonia - Occupational Exposure Limits

	OEL TWA
	150 mg/m³ (Turpentine produced from Nordic conifers has an irritating effect on the skin, monoterpenes, with the exception of 3-Carene, have a lesser effect)

	OEL TWA
	25 ppm (Turpentine produced from Nordic conifers has an irritating effect on the skin, monoterpenes, with the exception of 3-Carene, have a lesser effect)

	OEL STEL
	300 mg/m³ (Turpentine produced from Nordic conifers has an irritating effect on the skin, monoterpenes, with the exception of 3-Carene, have a lesser effect)

	OEL STEL
	50 ppm (Turpentine produced from Nordic conifers has an irritating effect on the skin, monoterpenes, with the exception of 3-Carene, have a lesser effect)

	Lithuania - Occupational Exposure Limits

	IPRV (OEL TWA)
	150 mg/m³

	IPRV (OEL TWA)
	25 ppm

	TPRV (OEL STEL)
	300 mg/m³

	TPRV (OEL STEL)
	50 ppm

	Portugal - Occupational Exposure Limits

	OEL TWA
	20 ppm (Turpentine and selected Monoterpenes)

	OEL chemical category
	Sensitizer dermal, A4 - Not Classifiable as a Human Carcinogen

	Spain - Occupational Exposure Limits

	VLA-ED (OEL TWA)
	113 mg/m³

	VLA-ED (OEL TWA)
	20 ppm

	OEL chemical category
	Sensitizer

	Sweden - Occupational Exposure Limits

	NGV (OEL TWA)
	150 mg/m³

	NGV (OEL TWA)
	25 ppm

	KGV (OEL STEL)
	300 mg/m³

	KGV (OEL STEL)
	50 ppm

	OEL chemical category
	Sensitizer

	Norway - Occupational Exposure Limits

	Grenseverdi (OEL TWA)
	140 mg/m³

	Grenseverdi (OEL TWA)
	25 ppm

	Korttidsverdi (OEL STEL)
	175 mg/m³ (value calculated)

	Korttidsverdi (OEL STEL)
	37.5 ppm (value calculated)

	OEL chemical category
	Skin notation

	USA - ACGIH - Occupational Exposure Limits

	ACGIH OEL TWA
	20 ppm (Turpentine and selected Monoterpenes)

	ACGIH chemical category
	Not Classifiable as a Human Carcinogen, dermal sensitizer



	(R)-p-mentha-1,8-diene; d-limonene (5989-27-5)

	Finland - Occupational Exposure Limits

	HTP (OEL TWA)
	140 mg/m³

	HTP (OEL TWA)
	25 ppm

	HTP (OEL STEL)
	280 mg/m³

	HTP (OEL STEL)
	50 ppm

	Germany - Occupational Exposure Limits (TRGS 900)

	AGW (OEL TWA)
	28 mg/m³ (the risk of damage to the embryo or fetus can be excluded when AGW and BGW values are observed)

	AGW (OEL TWA)
	5 ppm (the risk of damage to the embryo or fetus can be excluded when AGW and BGW values are observed)

	Chemical category
	Skin notation, Skin sensitization

	Slovenia - Occupational Exposure Limits

	OEL TWA
	28 mg/m³

	OEL TWA
	5 ppm

	OEL STEL
	112 mg/m³

	OEL STEL
	20 ppm

	OEL chemical category
	Potential for cutaneous absorption

	Spain - Occupational Exposure Limits

	VLA-ED (OEL TWA)
	168 mg/m³

	VLA-ED (OEL TWA)
	30 ppm

	OEL chemical category
	Sensitizer, skin - potential for cutaneous absorption

	Norway - Occupational Exposure Limits

	Grenseverdi (OEL TWA)
	140 mg/m³

	Grenseverdi (OEL TWA)
	25 ppm

	Korttidsverdi (OEL STEL)
	175 mg/m³ (value calculated)

	Korttidsverdi (OEL STEL)
	37.5 ppm (value calculated)

	OEL chemical category
	Allergenic substance

	Switzerland - Occupational Exposure Limits

	MAK (OEL TWA)
	40 mg/m³

	MAK (OEL TWA)
	7 ppm

	KZGW (OEL STEL)
	80 mg/m³

	KZGW (OEL STEL)
	14 ppm

	OEL chemical category
	Sensitizer



	.beta.-Pinene (127-91-3)

	Belgium - Occupational Exposure Limits

	OEL TWA
	20 ppm

	Estonia - Occupational Exposure Limits

	OEL TWA
	150 mg/m³ (Turpentine produced from Nordic conifers has an irritating effect on the skin, monoterpenes, with the exception of 3-Carene, have a lesser effect)

	OEL TWA
	25 ppm (Turpentine produced from Nordic conifers has an irritating effect on the skin, monoterpenes, with the exception of 3-Carene, have a lesser effect)

	OEL STEL
	300 mg/m³ (Turpentine produced from Nordic conifers has an irritating effect on the skin, monoterpenes, with the exception of 3-Carene, have a lesser effect)

	OEL STEL
	50 ppm (Turpentine produced from Nordic conifers has an irritating effect on the skin, monoterpenes, with the exception of 3-Carene, have a lesser effect)

	Lithuania - Occupational Exposure Limits

	IPRV (OEL TWA)
	150 mg/m³

	IPRV (OEL TWA)
	25 ppm

	TPRV (OEL STEL)
	300 mg/m³

	TPRV (OEL STEL)
	50 ppm

	Portugal - Occupational Exposure Limits

	OEL TWA
	20 ppm (Turpentine and selected Monoterpenes)

	OEL chemical category
	Sensitizer dermal, A4 - Not Classifiable as a Human Carcinogen

	Spain - Occupational Exposure Limits

	VLA-ED (OEL TWA)
	113 mg/m³

	VLA-ED (OEL TWA)
	20 ppm

	OEL chemical category
	Sensitizer

	Sweden - Occupational Exposure Limits

	NGV (OEL TWA)
	150 mg/m³

	NGV (OEL TWA)
	25 ppm

	KGV (OEL STEL)
	300 mg/m³

	KGV (OEL STEL)
	50 ppm

	OEL chemical category
	Sensitizer

	Norway - Occupational Exposure Limits

	Grenseverdi (OEL TWA)
	140 mg/m³

	Grenseverdi (OEL TWA)
	25 ppm

	Korttidsverdi (OEL STEL)
	175 mg/m³ (value calculated)

	Korttidsverdi (OEL STEL)
	37.5 ppm (value calculated)

	USA - ACGIH - Occupational Exposure Limits

	ACGIH OEL TWA
	20 ppm (Turpentine and selected Monoterpenes)

	ACGIH chemical category
	Not Classifiable as a Human Carcinogen, dermal sensitizer



	p-Cymene (99-87-6)

	Denmark - Occupational Exposure Limits

	OEL TWA
	135 mg/m³ (Methylisopropylbenzenes)

	OEL TWA
	25 ppm (Methylisopropylbenzenes)

	OEL STEL
	270 mg/m³ (Methylisopropylbenzenes)

	OEL STEL
	50 ppm (Methylisopropylbenzenes)

	Estonia - Occupational Exposure Limits

	OEL TWA
	140 mg/m³

	OEL TWA
	25 ppm

	OEL STEL
	190 mg/m³

	OEL STEL
	35 ppm

	Latvia - Occupational Exposure Limits

	OEL TWA
	10 mg/m³ (Cymene (2, 3, 4-isomers mixture))

	Lithuania - Occupational Exposure Limits

	IPRV (OEL TWA)
	140 mg/m³

	IPRV (OEL TWA)
	25 ppm

	TPRV (OEL STEL)
	190 mg/m³

	TPRV (OEL STEL)
	35 ppm

	Sweden - Occupational Exposure Limits

	NGV (OEL TWA)
	140 mg/m³

	NGV (OEL TWA)
	25 ppm

	KGV (OEL STEL)
	190 mg/m³

	KGV (OEL STEL)
	35 ppm



	Ethyl benzoate (93-89-0)

	Romania - Occupational Exposure Limits

	OEL TWA
	200 mg/m³

	OEL TWA
	33 ppm

	OEL STEL
	300 mg/m³

	OEL STEL
	49 ppm



	ethanol; ethyl alcohol (64-17-5)

	Austria - Occupational Exposure Limits

	MAK (OEL TWA)
	1900 mg/m³

	MAK (OEL TWA)
	1000 ppm

	MAK (OEL STEL)
	3800 mg/m³

	MAK (OEL STEL)
	2000 ppm

	Belgium - Occupational Exposure Limits

	OEL TWA
	1907 mg/m³

	OEL TWA
	1000 ppm

	Bulgaria - Occupational Exposure Limits

	OEL TWA
	1000 mg/m³

	Croatia - Occupational Exposure Limits

	GVI (OEL TWA)
	1900 mg/m³

	GVI (OEL TWA)
	1000 ppm

	Czech Republic - Occupational Exposure Limits

	PEL (OEL TWA)
	1000 mg/m³

	Denmark - Occupational Exposure Limits

	OEL TWA
	1900 mg/m³

	OEL TWA
	1000 ppm

	OEL STEL
	3800 mg/m³

	OEL STEL
	2000 ppm

	Estonia - Occupational Exposure Limits

	OEL TWA
	1000 mg/m³

	OEL TWA
	500 ppm

	OEL STEL
	1900 mg/m³

	OEL STEL
	1000 ppm

	Finland - Occupational Exposure Limits

	HTP (OEL TWA)
	1900 mg/m³

	HTP (OEL TWA)
	1000 ppm

	HTP (OEL STEL)
	2500 mg/m³

	HTP (OEL STEL)
	1300 ppm

	France - Occupational Exposure Limits

	VME (OEL TWA)
	1900 mg/m³

	VME (OEL TWA)
	1000 ppm

	VLE (OEL C/STEL)
	9500 mg/m³

	VLE (OEL C/STEL)
	5000 ppm

	Germany - Occupational Exposure Limits (TRGS 900)

	AGW (OEL TWA)
	380 mg/m³ (the risk of damage to the embryo or fetus can be excluded when AGW and BGW values are observed)

	AGW (OEL TWA)
	200 ppm (the risk of damage to the embryo or fetus can be excluded when AGW and BGW values are observed)

	Greece - Occupational Exposure Limits

	OEL TWA
	1900 mg/m³

	OEL TWA
	1000 ppm

	Hungary - Occupational Exposure Limits

	AK (OEL TWA)
	1900 mg/m³

	CK (OEL STEL)
	3800 mg/m³

	Ireland - Occupational Exposure Limits

	OEL STEL
	1000 ppm

	Latvia - Occupational Exposure Limits

	OEL TWA
	1000 mg/m³

	Lithuania - Occupational Exposure Limits

	IPRV (OEL TWA)
	1000 mg/m³

	IPRV (OEL TWA)
	500 ppm

	TPRV (OEL STEL)
	1900 mg/m³

	TPRV (OEL STEL)
	1000 ppm

	Netherlands - Occupational Exposure Limits

	TGG-8u (OEL TWA)
	260 mg/m³

	TGG-8u (OEL TWA)
	137 ppm

	TGG-15min (OEL STEL)
	1900 mg/m³

	TGG-15min (OEL STEL)
	1000 ppm

	MAC chemical category
	Skin notation

	Poland - Occupational Exposure Limits

	NDS (OEL TWA)
	1900 mg/m³

	Portugal - Occupational Exposure Limits

	OEL STEL
	1000 ppm

	OEL chemical category
	A3 - Confirmed Animal Carcinogen with Unknown Relevance to Humans

	Romania - Occupational Exposure Limits

	OEL TWA
	1900 mg/m³

	OEL TWA
	1000 ppm

	OEL STEL
	9500 mg/m³

	OEL STEL
	5000 ppm

	Slovakia - Occupational Exposure Limits

	NPHV (OEL TWA)
	960 mg/m³

	NPHV (OEL TWA)
	500 ppm

	NPHV (OEL C)
	1920 mg/m³

	Slovenia - Occupational Exposure Limits

	OEL TWA
	960 mg/m³

	OEL TWA
	500 ppm

	OEL STEL
	1920 mg/m³

	OEL STEL
	1000 ppm

	Spain - Occupational Exposure Limits

	VLA-EC (OEL STEL)
	1910 mg/m³

	VLA-EC (OEL STEL)
	1000 ppm

	Sweden - Occupational Exposure Limits

	NGV (OEL TWA)
	1000 mg/m³

	NGV (OEL TWA)
	500 ppm

	KGV (OEL STEL)
	1900 mg/m³

	KGV (OEL STEL)
	1000 ppm

	United Kingdom - Occupational Exposure Limits

	WEL TWA (OEL TWA)
	1920 mg/m³

	WEL TWA (OEL TWA)
	1000 ppm

	WEL STEL (OEL STEL)
	5760 mg/m³ (calculated)

	WEL STEL (OEL STEL)
	3000 ppm (calculated)

	Norway - Occupational Exposure Limits

	Grenseverdi (OEL TWA)
	950 mg/m³

	Grenseverdi (OEL TWA)
	500 ppm

	Korttidsverdi (OEL STEL)
	1187.5 mg/m³ (value calculated)

	Korttidsverdi (OEL STEL)
	625 ppm (value calculated)

	Switzerland - Occupational Exposure Limits

	MAK (OEL TWA)
	960 mg/m³

	MAK (OEL TWA)
	500 ppm

	KZGW (OEL STEL)
	1920 mg/m³

	KZGW (OEL STEL)
	1000 ppm

	USA - ACGIH - Occupational Exposure Limits

	ACGIH OEL STEL
	1000 ppm

	ACGIH chemical category
	Confirmed Animal Carcinogen with Unknown Relevance to Humans



	acetaldehyde; ethanal (75-07-0)

	Austria - Occupational Exposure Limits

	MAK (OEL TWA)
	90 mg/m³

	MAK (OEL TWA)
	50 ppm

	MAK (OEL STEL)
	90 mg/m³

	MAK (OEL STEL)
	50 ppm

	OEL C
	90 mg/m³

	OEL C
	50 ppm

	OEL chemical category
	Group B Carcinogen

	Belgium - Occupational Exposure Limits

	OEL TWA
	46 mg/m³

	OEL TWA
	25 ppm

	Bulgaria - Occupational Exposure Limits

	OEL TWA
	30 mg/m³

	OEL STEL
	200 mg/m³

	Croatia - Occupational Exposure Limits

	GVI (OEL TWA)
	37 mg/m³

	GVI (OEL TWA)
	20 ppm

	KGVI (OEL STEL)
	92 mg/m³

	KGVI (OEL STEL)
	50 ppm

	Czech Republic - Occupational Exposure Limits

	PEL (OEL TWA)
	50 mg/m³

	Denmark - Occupational Exposure Limits

	OEL C
	45 mg/m³

	OEL C
	25 ppm

	Estonia - Occupational Exposure Limits

	OEL TWA
	45 mg/m³

	OEL TWA
	25 ppm

	OEL STEL
	90 mg/m³

	OEL STEL
	50 ppm

	OEL chemical category
	Carcinogenic substance

	Finland - Occupational Exposure Limits

	HTP (OEL STEL)
	46 mg/m³

	HTP (OEL STEL)
	25 ppm

	France - Occupational Exposure Limits

	VME (OEL TWA)
	180 mg/m³

	VME (OEL TWA)
	100 ppm

	OEL chemical category
	Carcinogen category 1B, Mutagen category 2

	Germany - Occupational Exposure Limits (TRGS 900)

	AGW (OEL TWA)
	91 mg/m³ (the risk of damage to the embryo or fetus can be excluded when AGW and BGW values are observed)

	AGW (OEL TWA)
	50 ppm (the risk of damage to the embryo or fetus can be excluded when AGW and BGW values are observed)

	Greece - Occupational Exposure Limits

	OEL TWA
	180 mg/m³

	OEL TWA
	100 ppm

	OEL STEL
	270 mg/m³

	OEL STEL
	150 ppm

	Hungary - Occupational Exposure Limits

	AK (OEL TWA)
	45 mg/m³

	CK (OEL STEL)
	45 mg/m³

	Ireland - Occupational Exposure Limits

	OEL STEL
	45 mg/m³

	OEL STEL
	25 ppm

	Latvia - Occupational Exposure Limits

	OEL TWA
	5 mg/m³

	Lithuania - Occupational Exposure Limits

	IPRV (OEL TWA)
	45 mg/m³

	IPRV (OEL TWA)
	25 ppm

	TPRV (OEL STEL)
	90 mg/m³

	TPRV (OEL STEL)
	50 ppm

	OEL chemical category
	Carcinogen

	Netherlands - Occupational Exposure Limits

	TGG-8u (OEL TWA)
	37 mg/m³

	TGG-8u (OEL TWA)
	20 ppm

	TGG-15min (OEL STEL)
	92 mg/m³

	TGG-15min (OEL STEL)
	50 ppm

	Poland - Occupational Exposure Limits

	NDSP (OEL C)
	45 mg/m³

	Portugal - Occupational Exposure Limits

	OEL C
	25 ppm

	OEL chemical category
	A2 - Suspected Human Carcinogen

	Romania - Occupational Exposure Limits

	OEL TWA
	90 mg/m³

	OEL TWA
	50 ppm

	OEL STEL
	180 mg/m³

	OEL STEL
	100 ppm

	Slovakia - Occupational Exposure Limits

	NPHV (OEL TWA)
	91 mg/m³

	NPHV (OEL TWA)
	50 ppm

	Slovenia - Occupational Exposure Limits

	OEL TWA
	91 mg/m³

	OEL TWA
	50 ppm

	OEL STEL
	91 mg/m³

	OEL STEL
	50 ppm

	OEL chemical category
	Category 2

	Spain - Occupational Exposure Limits

	VLA-EC (OEL STEL)
	46 mg/m³

	VLA-EC (OEL STEL)
	25 ppm

	OEL chemical category
	C1B

	Sweden - Occupational Exposure Limits

	NGV (OEL TWA)
	45 mg/m³

	NGV (OEL TWA)
	25 ppm

	KGV (OEL STEL)
	90 mg/m³

	KGV (OEL STEL)
	50 ppm

	OEL chemical category
	Carcinogen

	United Kingdom - Occupational Exposure Limits

	WEL TWA (OEL TWA)
	37 mg/m³

	WEL TWA (OEL TWA)
	20 ppm

	WEL STEL (OEL STEL)
	92 mg/m³

	WEL STEL (OEL STEL)
	50 ppm

	WEL chemical category
	Capable of causing cancer and/or heritable genetic damage

	Norway - Occupational Exposure Limits

	Grenseverdi (OEL TWA)
	45 mg/m³

	Grenseverdi (OEL TWA)
	25 ppm

	Korttidsverdi (OEL STEL)
	67.5 mg/m³ (value calculated)

	Korttidsverdi (OEL STEL)
	37.5 ppm (value calculated)

	OEL chemical category
	Carcinogen

	Switzerland - Occupational Exposure Limits

	MAK (OEL TWA)
	90 ppm
50 ppm

	KZGW (OEL STEL)
	90 mg/m³

	KZGW (OEL STEL)
	50 ppm

	OEL chemical category
	Category C2 carcinogen

	USA - ACGIH - Occupational Exposure Limits

	ACGIH OEL C
	25 ppm

	ACGIH chemical category
	Suspected Human Carcinogen


[bookmark: _Hlk54076527]8.1.2. Recommended monitoring procedures
No additional information available
[bookmark: _Hlk54076613]8.1.3. Air contaminants formed
No additional information available
[bookmark: _Hlk54076910]8.1.4. DNEL and PNEC
No additional information available
[bookmark: _Hlk54076968]8.1.5. Control banding
No additional information available
8.2. Exposure controls
8.2.1. Appropriate engineering controls
No additional information available

8.2.2. Personal protection equipment
	Personal protective equipment:

	Avoid all unnecessary exposure.

	Personal protective equipment symbol(s):

	[image: ]



8.2.2.1. Eye and face protection
	Eye protection:

	Chemical goggles or safety glasses



8.2.2.2. Skin protection
	Hand protection:

	Wear protective gloves.



8.2.2.3. Respiratory protection
	Respiratory protection:

	Wear appropriate mask



8.2.2.4. Thermal hazards
No additional information available

8.2.3. Environmental exposure controls
	Other information:

	Do not eat, drink or smoke during use.


SECTION 9: Physical and chemical properties
9.1. Information on basic physical and chemical properties
	Physical state
	:
	Liquid

	Colour
	:
	Conforms to standard.

	Odour
	:
	characteristic.

	Odour threshold
	:
	Not available

	Melting point
	:
	Not available

	Freezing point
	:
	Not available

	Boiling point
	:
	Not available

	Flammability
	:
	Non flammable.

	Lower explosion limit
	:
	Not available

	Upper explosion limit
	:
	Not available

	Flash point
	:
	> 93 °C

	Auto-ignition temperature
	:
	Not available

	Decomposition temperature
	:
	Not available

	pH
	:
	Not available

	Viscosity, kinematic
	:
	Not available

	Solubility
	:
	Not available

	Partition coefficient n-octanol/water (Log Kow)
	:
	Not available

	Vapour pressure
	:
	Not available

	Vapour pressure at 50°C
	:
	Not available

	Density
	:
	Not available

	Relative density
	:
	Not available

	Relative vapour density at 20°C
	:
	Not available

	Particle characteristics
	:
	Not applicable


9.2. Other information
[bookmark: _Hlk54084650]9.2.1. Information with regard to physical hazard classes
No additional information available
9.2.2. Other safety characteristics
No additional information available
SECTION 10: Stability and reactivity
10.1. Reactivity
No additional information available
10.2. Chemical stability
Not established.
10.3. Possibility of hazardous reactions
Not established.
10.4. Conditions to avoid
Direct sunlight. Extremely high or low temperatures.
10.5. Incompatible materials
Strong acids. Strong bases.
10.6. Hazardous decomposition products
fume. Carbon monoxide. Carbon dioxide.
SECTION 11: Toxicological information
11.1. Information on hazard classes as defined in Regulation (EC) No 1272/2008
	Acute toxicity (oral)
	:
	Not classified

	Acute toxicity (dermal)
	:
	Not classified

	Acute toxicity (inhalation)
	:
	Not classified



	benzyl benzoate (120-51-4)

	LD50 oral rat
	> 2000 mg/kg (Source: ECHA_API)

	LD50 oral
	1160 mg/kg bodyweight

	LD50 dermal rabbit
	4000 mg/kg (Source: NLM_CIP)



	Verdox (88-41-5)

	LD50 oral rat
	4600 mg/kg (Source: NLM_CIP)

	LD50 oral
	4600 mg/kg



	Benzyl salicylate (118-58-1)

	LD50 oral rat
	2227 mg/kg (Source: NLM_CIP)

	LD50 oral
	2200 mg/kg bodyweight

	LD50 dermal rabbit
	> 5000 mg/kg (Source: CHEMVIEW)



	3-(2,2-dimethyl-3-hydroxypropyl)toluene; (alt.): 2,2-dimethyl-3-(3-methylphenyl)propanol (103694-68-4)

	LD50 oral
	3440 mg/kg bodyweight

	LD50 dermal rabbit
	> 5 ml/kg (Source: ECHA_API)



	Carbitol (111-90-0)

	LD50 oral rat
	10502 mg/kg (Source: OECD_SIDS)

	LD50 dermal rabbit
	9143 mg/kg (Source: OECD_SIDS)

	LC50 Inhalation - Rat
	> 5240 mg/m³ (Exposure time: 4 h Source: NLM_CIP)



	benzaldehyde (100-52-7)

	LD50 oral rat
	1292 mg/kg (Source: JAPAN_GHS)

	LD50 dermal rabbit
	> 1250 mg/kg (Source: JAPAN_GHS)

	LC50 Inhalation - Rat
	< 5 mg/l/4h



	isoeugenol (97-54-1)

	LD50 oral rat
	1560 mg/kg (Source: NLM_CIP)

	LD50 oral
	1500 mg/kg bodyweight

	LD50 dermal
	1912 mg/kg bodyweight



	.alpha.-Pinene (80-56-8)

	LD50 oral rat
	3700 mg/kg (Source: NLM_CIP)

	LD50 dermal rat
	> 5000 mg/kg (Source: CHEMVIEW)



	(R)-p-mentha-1,8-diene; d-limonene (5989-27-5)

	LD50 oral rat
	4400 mg/kg (Source: CHEMVIEW)

	LD50 dermal rabbit
	> 5 g/kg (Source: CHEMVIEW)



	.beta.-Pinene (127-91-3)

	LD50 oral rat
	> 5000 mg/kg (Source: EPA_HPV)

	LD50 dermal rabbit
	> 5000 mg/kg (Source: CHEMVIEW)



	p-Cymene (99-87-6)

	LD50 oral rat
	4750 mg/kg (Source: NLM_CIP)

	LD50 oral
	4750 mg/kg bodyweight

	LD50 dermal rabbit
	> 5000 mg/kg (Source: CHEMVIEW)

	LC50 Inhalation - Rat
	> 9.7 mg/l (Exposure time: 5 h Source: EU_CLH)

	LC50 Inhalation - Rat (Vapours)
	9.7 mg/l/4h



	Ethyl benzoate (93-89-0)

	LD50 oral rat
	2100 mg/kg (Source: NLM_CIP)



	ethanol; ethyl alcohol (64-17-5)

	LD50 oral rat
	7060 mg/kg (Source: NLM_CIP)

	LC50 Inhalation - Rat
	133.8 mg/l/4h



	acetaldehyde; ethanal (75-07-0)

	LD50 oral rat
	660 mg/kg (Source: JAPAN_GHS)

	LD50 oral
	700 mg/kg

	LD50 dermal rabbit
	3540 mg/kg (Source: NLM_HSDB)

	LD50 dermal
	3540 mg/kg

	LC50 Inhalation - Rat [ppm]
	13000 ppm/4h



	Skin corrosion/irritation
	:
	Not classified

	Additional information
	:
	Based on available data, the classification criteria are not met



	Serious eye damage/irritation
	:
	Not classified

	Additional information
	:
	Based on available data, the classification criteria are not met



	Respiratory or skin sensitisation
	:
	May cause an allergic skin reaction.

	Additional information
	:
	Based on available data, the classification criteria are not met



	Germ cell mutagenicity
	:
	Not classified

	Additional information
	:
	Based on available data, the classification criteria are not met



	Carcinogenicity
	:
	Not classified

	Additional information
	:
	Based on available data, the classification criteria are not met 



	isoeugenol (97-54-1)

	IARC group
	2B - Possibly carcinogenic to humans



	(R)-p-mentha-1,8-diene; d-limonene (5989-27-5)

	IARC group
	3 - Not classifiable



	acetaldehyde; ethanal (75-07-0)

	IARC group
	1 - Carcinogenic to humans,2B - Possibly carcinogenic to humans



	Reproductive toxicity
	:
	Not classified

	Additional information
	:
	Based on available data, the classification criteria are not met



	STOT-single exposure
	:
	Not classified

	Additional information
	:
	Based on available data, the classification criteria are not met



	isoeugenol (97-54-1)

	STOT-single exposure
	May cause respiratory irritation. 



	acetaldehyde; ethanal (75-07-0)

	STOT-single exposure
	May cause respiratory irritation. 



	STOT-repeated exposure
	:
	Not classified

	Additional information
	:
	Based on available data, the classification criteria are not met



	Aspiration hazard
	:
	Not classified

	Additional information
	:
	Based on available data, the classification criteria are not met



	benzyl benzoate (120-51-4)

	Viscosity, kinematic
	7.456 mm²/s



	.alpha.-Pinene (80-56-8)

	Hydrocarbon
	Yes



	(R)-p-mentha-1,8-diene; d-limonene (5989-27-5)

	Hydrocarbon
	Yes



	.beta.-Pinene (127-91-3)

	Hydrocarbon
	Yes



	p-Cymene (99-87-6)

	Hydrocarbon
	Yes


[bookmark: _Hlk54089399]11.2. Information on other hazards
11.2.1. Endocrine disrupting properties
No additional information available
[bookmark: _Hlk54089489][bookmark: _Hlk54089553]11.2.2. Other information
	Potential adverse human health effects and symptoms
	:
	Based on available data, the classification criteria are not met


SECTION 12: Ecological information
12.1. Toxicity
	Hazardous to the aquatic environment, short–term (acute)
	:
	Not classified

	Hazardous to the aquatic environment, long–term (chronic)
	:
	Harmful to aquatic life with long lasting effects.



	benzyl benzoate (120-51-4)

	LC50 - Fish [1]
	2.32 mg/l (Exposure time: 96 h - Species: Danio rerio [semi-static] Source: ECHA)

	NOEC (chronic)
	0.168 mg/l



	Benzyl salicylate (118-58-1)

	LC50 - Fish [1]
	1.03 mg/l (Exposure time: 96 h - Species: Danio rerio [semi-static] Source: ECHA)



	Carbitol (111-90-0)

	LC50 - Fish [1]
	10000 mg/l (Exposure time: 96 h - Species: Lepomis macrochirus [static] Source: EPA)

	LC50 - Fish [2]
	19100 – 23900 mg/l (Exposure time: 96 h - Species: Lepomis macrochirus [flow-through] Source: EPA)

	EC50 - Crustacea [1]
	3940 – 4670 mg/l (Exposure time: 48 h - Species: Daphnia magna)



	benzaldehyde (100-52-7)

	LC50 - Fish [1]
	10.6 – 11.8 mg/l (Exposure time: 96 h - Species: Oncorhynchus mykiss [flow-through] Source: EPA)

	LC50 - Fish [2]
	12.69 mg/l (Exposure time: 96 h - Species: Oncorhynchus mykiss [static] Source: IUCLID)



	.alpha.-Pinene (80-56-8)

	LC50 - Fish [1]
	0.28 mg/l (Exposure time: 96 h - Species: Pimephales promelas [static] Source: IUCLID)

	EC50 - Crustacea [1]
	41 mg/l (Exposure time: 48 h - Species: Daphnia magna)



	(R)-p-mentha-1,8-diene; d-limonene (5989-27-5)

	LC50 - Fish [1]
	0.619 – 0.796 mg/l (Exposure time: 96 h - Species: Pimephales promelas [flow-through] Source: EPA)

	LC50 - Fish [2]
	35 mg/l (Exposure time: 96 h - Species: Oncorhynchus mykiss Source: EPA)



	Ethyl benzoate (93-89-0)

	LC50 - Fish [1]
	6.7 mg/l (Exposure time: 96 h - Species: Pimephales promelas [flow-through] Source: EPA)



	ethanol; ethyl alcohol (64-17-5)

	LC50 - Fish [2]
	> 100 mg/l (Exposure time: 96 h - Species: Pimephales promelas [static] Source: EPA)

	EC50 - Crustacea [1]
	9268 – 14221 mg/l (Exposure time: 48 h - Species: Daphnia magna)

	EC50 - Crustacea [2]
	2 mg/l (Exposure time: 48 h - Species: Daphnia magna [Static])



	acetaldehyde; ethanal (75-07-0)

	LC50 - Fish [1]
	28 – 34 mg/l (Exposure time: 96 h - Species: Pimephales promelas [flow-through] Source: EPA)

	LC50 - Fish [2]
	53 mg/l (Exposure time: 96 h - Species: Lepomis macrochirus [static] Source: EPA)

	EC50 - Crustacea [1]
	3.64 – 6.15 mg/l (Exposure time: 48 h - Species: Daphnia magna [Static])

	EC50 - Crustacea [2]
	48.3 mg/l (Exposure time: 48 h - Species: Daphnia magna)


12.2. Persistence and degradability
	MILK & HONEY #EU24302F 25% in DPG 

	Persistence and degradability
	Not established.



	benzyl benzoate (120-51-4)

	Persistence and degradability
	May cause long-term adverse effects in the environment.



	Verdox (88-41-5)

	Persistence and degradability
	Rapidly degradable



	Benzyl salicylate (118-58-1)

	Persistence and degradability
	Rapidly degradable



	3-(2,2-dimethyl-3-hydroxypropyl)toluene; (alt.): 2,2-dimethyl-3-(3-methylphenyl)propanol (103694-68-4)

	Persistence and degradability
	Rapidly degradable



	Carbitol (111-90-0)

	Persistence and degradability
	Rapidly degradable



	benzaldehyde (100-52-7)

	Persistence and degradability
	Rapidly degradable



	Sandal Mysore Core (28219-60-5)

	Persistence and degradability
	Rapidly degradable



	isoeugenol (97-54-1)

	Persistence and degradability
	Rapidly degradable



	.alpha.-Pinene (80-56-8)

	Persistence and degradability
	Rapidly degradable



	(R)-p-mentha-1,8-diene; d-limonene (5989-27-5)

	Persistence and degradability
	Rapidly degradable



	.beta.-Pinene (127-91-3)

	Persistence and degradability
	Rapidly degradable



	p-Cymene (99-87-6)

	Persistence and degradability
	Rapidly degradable



	Ethyl benzoate (93-89-0)

	Persistence and degradability
	Rapidly degradable



	ethanol; ethyl alcohol (64-17-5)

	Persistence and degradability
	Rapidly degradable



	acetaldehyde; ethanal (75-07-0)

	Persistence and degradability
	Rapidly degradable


12.3. Bioaccumulative potential
	MILK & HONEY #EU24302F 25% in DPG 

	Bioaccumulative potential
	Not established.



	benzyl benzoate (120-51-4)

	Partition coefficient n-octanol/water (Log Pow)
	3.97 (at 25 °C)

	Bioaccumulative potential
	Not established.



	Benzyl salicylate (118-58-1)

	Partition coefficient n-octanol/water (Log Pow)
	4



	3-(2,2-dimethyl-3-hydroxypropyl)toluene; (alt.): 2,2-dimethyl-3-(3-methylphenyl)propanol (103694-68-4)

	Partition coefficient n-octanol/water (Log Pow)
	3.07 (at 20 °C)



	Carbitol (111-90-0)

	Partition coefficient n-octanol/water (Log Pow)
	-0.8



	benzaldehyde (100-52-7)

	BCF - Fish [1]
	(no significant bioaccumulation)

	Partition coefficient n-octanol/water (Log Pow)
	1.4 (at 25 °C)



	.alpha.-Pinene (80-56-8)

	Partition coefficient n-octanol/water (Log Pow)
	4.1



	(R)-p-mentha-1,8-diene; d-limonene (5989-27-5)

	Partition coefficient n-octanol/water (Log Pow)
	4.38 (at 37 °C (at pH 7.2)



	p-Cymene (99-87-6)

	Partition coefficient n-octanol/water (Log Pow)
	4.8 (at 20 °C (at pH 7)

	Partition coefficient n-octanol/water (Log Kow)
	0



	Ethyl benzoate (93-89-0)

	Partition coefficient n-octanol/water (Log Pow)
	2.59 (at 22.8 °C (at pH 6-7)



	ethanol; ethyl alcohol (64-17-5)

	Partition coefficient n-octanol/water (Log Pow)
	-0.35 (at 24 °C (at pH 7.4)



	acetaldehyde; ethanal (75-07-0)

	Partition coefficient n-octanol/water (Log Pow)
	0.45 – 0.63 (at 25 °C (at pH 7)


12.4. Mobility in soil
No additional information available
12.5. Results of PBT and vPvB assessment
No additional information available
12.6. Endocrine disrupting properties
[bookmark: _Hlk54090163]No additional information available
12.7. Other adverse effects
	Additional information
	:
	Avoid release to the environment.


SECTION 13: Disposal considerations
13.1. Waste treatment methods
	Product/Packaging disposal recommendations
	:
	Dispose in a safe manner in accordance with local/national regulations.

	Ecological information
	:
	Avoid release to the environment.

	HP Code
	:
	HP4 - “Irritant – skin irritation and eye damage:” waste which on application can cause skin irritation or damage to the eye.
HP14 - “Ecotoxic:” waste which presents or may present immediate or delayed risks for one or more sectors of the environment


SECTION 14: Transport information
In accordance with ADR / IMDG / IATA / ADN / RID
	ADR
	IMDG
	IATA
	ADN
	RID

	14.1. UN number or ID number

	Not applicable
	Not applicable
	Not applicable
	Not applicable
	Not applicable

	14.2. UN proper shipping name

	Not applicable
	Not applicable
	Not applicable
	Not applicable
	Not applicable

	14.3. Transport hazard class(es)

	Not applicable
	Not applicable
	Not applicable
	Not applicable
	Not applicable

	14.4. Packing group

	Not applicable
	Not applicable
	Not applicable
	Not applicable
	Not applicable

	14.5. Environmental hazards

	Not applicable
	Not applicable
	Not applicable
	Not applicable
	Not applicable

	No supplementary information available


14.6. Special precautions for user
	Overland transport

	Not applicable



	Transport by sea

	Not applicable



	Air transport

	Not applicable



	Inland waterway transport

	Not applicable



	Rail transport

	Not applicable


14.7. Maritime transport in bulk according to IMO instruments
Not applicable
SECTION 15: Regulatory information
15.1. Safety, health and environmental regulations/legislation specific for the substance or mixture
15.1.1. EU-Regulations
REACH Annex XVII (Restriction List)
	EU restriction list (REACH Annex XVII)

	Reference code
	Applicable on
	Entry title or description

	28.
	acetaldehyde; ethanal
	Substances which are classified as carcinogen category 1A or 1B in Part 3 of Annex VI to Regulation (EC) No 1272/2008 and are listed in Appendix 1 or Appendix 2, respectively.

	3(a)
	.alpha.-Pinene ; (R)-p-mentha-1,8-diene; d-limonene ; .beta.-Pinene ; p-Cymene ; ethanol; ethyl alcohol ; acetaldehyde; ethanal
	Substances or mixtures fulfilling the criteria for any of the following hazard classes or categories set out in Annex I to Regulation (EC) No 1272/2008: Hazard classes 2.1 to 2.4, 2.6 and 2.7, 2.8 types A and B, 2.9, 2.10, 2.12, 2.13 categories 1 and 2, 2.14 categories 1 and 2, 2.15 types A to F

	3(b)
	MILK & HONEY #EU24302F 25% in DPG ; benzyl benzoate ; Benzyl salicylate ; 3-(2,2-dimethyl-3-hydroxypropyl)toluene; (alt.): 2,2-dimethyl-3-(3-methylphenyl)propanol ; benzaldehyde ; Sandal Mysore Core ; isoeugenol ; .alpha.-Pinene ; (R)-p-mentha-1,8-diene; d-limonene ; p-Cymene ; acetaldehyde; ethanal
	Substances or mixtures fulfilling the criteria for any of the following hazard classes or categories set out in Annex I to Regulation (EC) No 1272/2008: Hazard classes 3.1 to 3.6, 3.7 adverse effects on sexual function and fertility or on development, 3.8 effects other than narcotic effects, 3.9 and 3.10

	3(c)
	MILK & HONEY #EU24302F 25% in DPG ; benzyl benzoate ; Verdox ; Benzyl salicylate ; 3-(2,2-dimethyl-3-hydroxypropyl)toluene; (alt.): 2,2-dimethyl-3-(3-methylphenyl)propanol ; Sandal Mysore Core ; .alpha.-Pinene ; (R)-p-mentha-1,8-diene; d-limonene ; p-Cymene
	Substances or mixtures fulfilling the criteria for any of the following hazard classes or categories set out in Annex I to Regulation (EC) No 1272/2008: Hazard class 4.1

	40.
	.alpha.-Pinene ; (R)-p-mentha-1,8-diene; d-limonene ; .beta.-Pinene ; p-Cymene ; ethanol; ethyl alcohol ; acetaldehyde; ethanal
	Substances classified as flammable gases category 1 or 2, flammable liquids categories 1, 2 or 3, flammable solids category 1 or 2, substances and mixtures which, in contact with water, emit flammable gases, category 1, 2 or 3, pyrophoric liquids category 1 or pyrophoric solids category 1, regardless of whether they appear in Part 3 of Annex VI to Regulation (EC) No 1272/2008 or not.


REACH Annex XIV (Authorisation List)
Contains no substance(s) listed on REACH Annex XIV (Authorisation List)
REACH Candidate List (SVHC)
Contains no substance(s) listed on the REACH Candidate List
PIC Regulation (Prior Informed Consent)
Contains no substance(s) listed on the PIC list (Regulation EU 649/2012 concerning the export and import of hazardous chemicals)
POP Regulation (Persistent Organic Pollutants)
Contains no substance(s) listed on the POP list (Regulation EU 2019/1021 on persistent organic pollutants)
Ozone Regulation (1005/2009)
Contains no substance(s) listed on the Ozone Depletion list (Regulation EU 1005/2009 on substances that deplete the ozone layer)
Council Regulation (EC) for the control of dual-use items
Contains no substance subject to the COUNCIL REGULATION (EC) for the control of dual-use items
Explosives Precursors Regulation (2019/1148)
Contains no substance(s) listed on the Explosives Precursors list (Regulation EU 2019/1148 on the marketing and use of explosives precursors)
Drug Precursors Regulation (273/2004)
Contains no substance(s) listed on the Drug Precursors list (Regulation EC 273/2004 on the manufacture and the placing on market of certain substances used in the illicit manufacture of narcotic drugs and psychotropic substances)
15.1.2. National regulations
	France

		Occupational diseases

	Code
	Description

	RG 84
	Conditions caused by liquid organic solvents for professional use: saturated or unsaturated aliphatic or cyclic liquid hydrocarbons and mixtures thereof; liquid halogenated hydrocarbons; nitrated derivatives of aliphatic hydrocarbons; alcohols; glycols, glycol ethers; ketones; aldehydes; aliphatic and cyclic ethers, including tetrahydrofuran; esters; dimethylformamide and dimethylacetamine; acetonitrile and propionitrile; pyridine; dimethylsulfone and dimethylsulfoxide




	Germany

	Water hazard class (WGK)
	:
	WGK 2, Significantly hazardous to water (Classification according to AwSV, Annex 1).

	Hazardous Incident Ordinance (12. BImSchV)
	:
	 Is not subject to the Hazardous Incident Ordinance (12. BImSchV)

	Netherlands

	ABM category
	:
	A(2) - toxic for aquatic organisms, may have longterm hazardous effects in aquatic environment

	SZW-lijst van kankerverwekkende stoffen
	:
	Ethyl alcohol,Acetaldehyde are listed

	SZW-lijst van mutagene stoffen
	:
	None of the components are listed

	SZW-lijst van reprotoxische stoffen – Borstvoeding
	:
	Ethyl alcohol is listed

	SZW-lijst van reprotoxische stoffen – Vruchtbaarheid
	:
	Ethyl alcohol is listed

	SZW-lijst van reprotoxische stoffen – Ontwikkeling
	:
	Ethyl alcohol is listed

	Denmark

	Classification remarks
	:
	Emergency management guidelines for the storage of flammable liquids must be followed

	Danish National Regulations
	:
	Young people below the age of 18 years are not allowed to use the product
Pregnant/breastfeeding women working with the product must not be in direct contact with the product


15.2. Chemical safety assessment
No chemical safety assessment has been carried out
SECTION 16: Other information
	Data sources
	:
	REGULATION (EC) No 1272/2008 OF THE EUROPEAN PARLIAMENT AND OF THE COUNCIL of 16 December 2008 on classification, labelling and packaging of substances and mixtures, amending and repealing Directives 67/548/EEC and 1999/45/EC, and amending Regulation (EC) No 1907/2006.

	Other information
	:
	None.



	Full text of H- and EUH-statements:

	Acute Tox. 3 (Inhalation)
	Acute toxicity (inhal.), Category 3

	Acute Tox. 3 (Inhalation:dust,mist)
	Acute toxicity (inhalation:dust,mist) Category 3

	Acute Tox. 4 (Dermal)
	Acute toxicity (dermal), Category 4

	Acute Tox. 4 (Inhalation)
	Acute toxicity (inhal.), Category 4

	Acute Tox. 4 (Oral)
	Acute toxicity (oral), Category 4

	Aquatic Acute 1
	Hazardous to the aquatic environment – Acute Hazard, Category 1

	Aquatic Chronic 1
	Hazardous to the aquatic environment – Chronic Hazard, Category 1

	Aquatic Chronic 2
	Hazardous to the aquatic environment – Chronic Hazard, Category 2

	Aquatic Chronic 3
	Hazardous to the aquatic environment – Chronic Hazard, Category 3

	Asp. Tox. 1
	Aspiration hazard, Category 1

	Carc. 1B
	Carcinogenicity, Category 1B

	Carc. 2
	Carcinogenicity, Category 2

	Eye Irrit. 2
	Serious eye damage/eye irritation, Category 2

	Flam. Liq. 1
	Flammable liquids, Category 1

	Flam. Liq. 2
	Flammable liquids, Category 2

	Flam. Liq. 3
	Flammable liquids, Category 3

	H224
	Extremely flammable liquid and vapour.

	H225
	Highly flammable liquid and vapour.

	H226
	Flammable liquid and vapour.

	H302
	Harmful if swallowed.

	H304
	May be fatal if swallowed and enters airways.

	H312
	Harmful in contact with skin.

	H315
	Causes skin irritation.

	H317
	May cause an allergic skin reaction.

	H319
	Causes serious eye irritation.

	H331
	Toxic if inhaled.

	H332
	Harmful if inhaled.

	H335
	May cause respiratory irritation.

	H341
	Suspected of causing genetic defects.

	H350
	May cause cancer.

	H351
	Suspected of causing cancer.

	H361
	Suspected of damaging fertility or the unborn child.

	H400
	Very toxic to aquatic life.

	H410
	Very toxic to aquatic life with long lasting effects.

	H411
	Toxic to aquatic life with long lasting effects.

	H412
	Harmful to aquatic life with long lasting effects.

	Muta. 2
	Germ cell mutagenicity, Category 2

	Repr. 2
	Reproductive toxicity, Category 2

	Skin Irrit. 2
	Skin corrosion/irritation, Category 2

	Skin Sens. 1
	Skin sensitisation, Category 1

	Skin Sens. 1A
	Skin sensitisation, category 1A

	Skin Sens. 1B
	Skin sensitisation, category 1B

	STOT SE 3
	Specific target organ toxicity – Single exposure, Category 3, Respiratory tract irritation



	The classification complies with
	:
	ATP 12


Safety Data Sheet (SDS), EU
This information is based on our current knowledge and is intended to describe the product for the purposes of health, safety and environmental requirements only. It should not therefore be construed as guaranteeing any specific property of the product.
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