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SECTION 1: Identification of the substance/mixture and of the company/undertaking
1.1. Product identifier
	Product form
	:
	Mixture

	Product name
	:
	J'Adore Type #EU30835F 25% in DPG

	Product code
	:
	EU30835F_25%

	Type of product
	:
	Perfumes, fragrances


1.2. Relevant identified uses of the substance or mixture and uses advised against
1.2.1. Relevant identified uses
	Industrial/Professional use spec
	:
	Industrial
For professional use only

	Use of the substance/mixture
	:
	Perfumes, fragrances

	Function or use category
	:
	Odour agents


1.2.2. Uses advised against
No additional information available
1.3. Details of the supplier of the safety data sheet
No additional information available
1.4. Emergency telephone number
No additional information available
SECTION 2: Hazards identification
2.1. Classification of the substance or mixture
Classification according to Regulation (EC) No. 1272/2008 [CLP]
	Hazardous to the aquatic environment – Chronic Hazard, Category 3
	H412 
	


Full text of H- and EUH-statements: see section 16
Adverse physicochemical, human health and environmental effects
No additional information available
2.2. Label elements
Labelling according to Regulation (EC) No. 1272/2008 [CLP]
	Signal word (CLP)
	:
	-

	Hazard statements (CLP)
	:
	H412 - Harmful to aquatic life with long lasting effects.

	Precautionary statements (CLP)
	:
	P273 - Avoid release to the environment.
P501 - Dispose of contents/container to hazardous or special waste collection point, in accordance with local, regional, national and/or international regulation.

	EUH-statements
	:
	EUH208 - Contains Ethyl linalool, Hexyl salicylate, Hexyl cinnamic aldehyde, Helional, Benzyl salicylate, Citronellol Pure, Linalyl acetate. May produce an allergic reaction.

	Extra phrases
	:
	For professional users only.


2.3. Other hazards
	Contains no PBT and/or vPvB substances ≥ 0.1% assessed in accordance with REACH Annex XIII


SECTION 3: Composition/information on ingredients
3.1. Substances
Not applicable
3.2. Mixtures
	Name
	Product identifier
	%
	Classification according to Regulation (EC) No. 1272/2008 [CLP]

	benzyl benzoate
	CAS-No.: 120-51-4
EC-No.: 204-402-9
EC Index-No.: 607-085-00-9
REACH-no: 01-2119976371-33
	9.4 – 18.818
	Acute Tox. 4 (Oral), H302
Aquatic Acute 1, H400
Aquatic Chronic 2, H411

	Ethyl linalool
	CAS-No.: 10339-55-6
EC-No.: 233-732-6
REACH-no: 01-2119969272-32
	0.275 – 0.525
	Eye Irrit. 2, H319
Skin Sens. 1B, H317

	Hexyl cinnamic aldehyde
	CAS-No.: 101-86-0
EC-No.: 202-983-3
REACH-no: 01-2119533092-50
	0.175 – 0.325
	Skin Sens. 1, H317
Aquatic Chronic 2, H411

	2-phenoxyethanol
substance with national workplace exposure limit(s) (AT, DE, FI, PL, SI, CH)
	CAS-No.: 122-99-6
EC-No.: 204-589-7
EC Index-No.: 603-098-00-9
REACH-no: 01-2119488943-21
	0.125 – 0.2625
	Acute Tox. 4 (Oral), H302
STOT SE 3, H335
Eye Dam. 1, H318

	Helional
	CAS-No.: 1205-17-0
EC-No.: 214-881-6
REACH-no: 01-2120740119-58
	0.125 – 0.2625
	Skin Sens. 1B, H317
Repr. 2, H361
Aquatic Chronic 2, H411

	Hexyl salicylate
	CAS-No.: 6259-76-3
EC-No.: 228-408-6
	0.1025 – 0.260775
	Skin Irrit. 2, H315
Skin Sens. 1, H317
Aquatic Acute 1, H400
Aquatic Chronic 1, H410

	Benzyl salicylate
	CAS-No.: 118-58-1
EC-No.: 204-262-9
EC Index-No.: 607-754-00-5
REACH-no: 01-2119969442-31
	0.125 – 0.250075
	Eye Irrit. 2, H319
Skin Sens. 1B, H317
Aquatic Chronic 3, H412

	ACETYL HEXAMETHYL TETRALIN
	CAS-No.: 21145-77-7
EC-No.: 244-240-6
	0.125 – 0.2375
	Acute Tox. 4 (Oral), H302
Aquatic Acute 1, H400
Aquatic Chronic 1, H410

	Citronellol Pure
	CAS-No.: 106-22-9
EC-No.: 203-375-0
REACH-no: 01-2119453995-23
	0.075 – 0.1625
	Skin Irrit. 2, H315
Eye Irrit. 2, H319
Skin Sens. 1B, H317

	Linalyl acetate
	CAS-No.: 115-95-7
EC-No.: 204-116-4
REACH-no: 01-2119454789-19
	0.075 – 0.15
	Skin Irrit. 2, H315
Eye Irrit. 2, H319
Skin Sens. 1, H317

	Benzyl acetate
substance with national workplace exposure limit(s) (BE, DK, ES, IE, LT, LV, PT, RO)
	CAS-No.: 140-11-4
EC-No.: 205-399-7
REACH-no: 01-2119638272-42
	0.075 – 0.1375
	Aquatic Chronic 3, H412

	Carbitol
substance with national workplace exposure limit(s) (AT, DE, EE, SE, SI, CH)
	CAS-No.: 111-90-0
EC-No.: 203-919-7
REACH-no: 01-2119475105-42
	0.0180825 – 0.036165
	Not classified

	ethyl acetate
substance with national workplace exposure limit(s) (AT, BE, BG, CY, CZ, DE, DK, EE, ES, FI, FR, GB, GI, GR, HR, HU, IE, IT, LT, LU, LV, MT, NL, PL, PT, RO, SE, SI, SK, NO, CH); substance with a Community workplace exposure limit
	CAS-No.: 141-78-6
EC-No.: 205-500-4
EC Index-No.: 607-022-00-5
REACH-no: 01-2119475103-46
	0 – 0.0125
	Flam. Liq. 1, H224
Eye Irrit. 2, H319
STOT SE 3, H336

	Alcohol C-10
substance with national workplace exposure limit(s) (BG, DE, LT, LV, RO, CH)
	CAS-No.: 112-30-1
EC-No.: 203-956-9
	0 – 0.00035
	Aquatic Chronic 3, H412

	Aldehyde C-6
substance with national workplace exposure limit(s) (FI, PL)
	CAS-No.: 66-25-1
EC-No.: 200-624-5
	0 – 0.0001
	Flam. Liq. 3, H226


Full text of H- and EUH-statements: see section 16

SECTION 4: First aid measures
4.1. Description of first aid measures
	First-aid measures general
	:
	Never give anything by mouth to an unconscious person. If you feel unwell, seek medical advice (show the label where possible).

	First-aid measures after inhalation
	:
	Allow affected person to breathe fresh air. Allow the victim to rest.

	First-aid measures after skin contact
	:
	Remove affected clothing and wash all exposed skin area with mild soap and water, followed by warm water rinse.

	First-aid measures after eye contact
	:
	Rinse immediately with plenty of water. Obtain medical attention if pain, blinking or redness persists.

	First-aid measures after ingestion
	:
	Rinse mouth. Do NOT induce vomiting. Obtain emergency medical attention.


4.2. Most important symptoms and effects, both acute and delayed
	Symptoms/effects
	:
	Not expected to present a significant hazard under anticipated conditions of normal use.


4.3. Indication of any immediate medical attention and special treatment needed
No additional information available
SECTION 5: Firefighting measures
5.1. Extinguishing media
	Suitable extinguishing media
	:
	Foam. Dry powder. Carbon dioxide. Water spray. Sand.

	Unsuitable extinguishing media
	:
	Do not use a heavy water stream.


5.2. Special hazards arising from the substance or mixture
No additional information available
5.3. Advice for firefighters
	Firefighting instructions
	:
	Use water spray or fog for cooling exposed containers. Exercise caution when fighting any chemical fire. Prevent fire fighting water from entering the environment.

	Protection during firefighting
	:
	Do not enter fire area without proper protective equipment, including respiratory protection.


SECTION 6: Accidental release measures
6.1. Personal precautions, protective equipment and emergency procedures
6.1.1. For non-emergency personnel
	Emergency procedures
	:
	Evacuate unnecessary personnel.


6.1.2. For emergency responders
	Protective equipment
	:
	Equip cleanup crew with proper protection.

	Emergency procedures
	:
	Ventilate area.


6.2. Environmental precautions
Prevent entry to sewers and public waters. Notify authorities if liquid enters sewers or public waters.
6.3. Methods and material for containment and cleaning up
	Methods for cleaning up
	:
	Soak up spills with inert solids, such as clay or diatomaceous earth as soon as possible. Collect spillage. Store away from other materials.


6.4. Reference to other sections
See Section 8. Exposure controls and personal protection.
SECTION 7: Handling and storage
7.1. Precautions for safe handling
	Precautions for safe handling
	:
	Wash hands and other exposed areas with mild soap and water before eating, drinking or smoking and when leaving work. Provide good ventilation in process area to prevent formation of vapour.


7.2. Conditions for safe storage, including any incompatibilities
	Storage conditions
	:
	Keep only in the original container in a cool, well ventilated place away from : Keep container closed when not in use.

	Incompatible products
	:
	Strong bases. Strong acids.

	Incompatible materials
	:
	Sources of ignition. Direct sunlight.


7.3. Specific end use(s)
No additional information available
SECTION 8: Exposure controls/personal protection
8.1. Control parameters
[bookmark: _Hlk54076387]8.1.1 National occupational exposure and biological limit values

	2-phenoxyethanol (122-99-6)

	Austria - Occupational Exposure Limits

	MAK (OEL TWA)
	110 mg/m³

	MAK (OEL TWA) [ppm]
	20 ppm

	MAK (OEL STEL)
	110 mg/m³

	MAK (OEL STEL) [ppm]
	20 ppm

	OEL C
	110 mg/m³

	OEL C
	20 ppm

	Finland - Occupational Exposure Limits

	HTP (OEL TWA) [1]
	110 mg/m³

	HTP (OEL TWA) [2]
	20 ppm

	HTP (OEL STEL)
	290 mg/m³

	HTP (OEL STEL) [ppm]
	50 ppm

	OEL chemical category
	Potential for cutaneous absorption

	Germany - Occupational Exposure Limits (TRGS 900)

	AGW (OEL TWA) [1]
	5.7 mg/m³ (the risk of damage to the embryo or fetus can be excluded when AGW and BGW values are observed)

	AGW (OEL TWA) [2]
	1 ppm (the risk of damage to the embryo or fetus can be excluded when AGW and BGW values are observed)

	Poland - Occupational Exposure Limits

	NDS (OEL TWA)
	230 mg/m³

	Slovenia - Occupational Exposure Limits

	OEL TWA
	5.7 mg/m³

	OEL TWA
	1 ppm

	OEL STEL
	5.7 mg/m³

	OEL STEL
	1 ppm

	Switzerland - Occupational Exposure Limits

	MAK (OEL TWA) [1]
	110 mg/m³ (aerosol, vapour)

	MAK (OEL TWA) [2]
	20 ppm (aerosol, vapour)

	KZGW (OEL STEL)
	110 mg/m³ (aerosol, vapour)

	KZGW (OEL STEL) [ppm]
	20 ppm (aerosol, vapour)



	Benzyl acetate (140-11-4)

	Belgium - Occupational Exposure Limits

	OEL TWA
	62 mg/m³

	OEL TWA
	10 ppm

	Denmark - Occupational Exposure Limits

	OEL TWA [1]
	61 mg/m³

	OEL TWA [2]
	10 ppm

	OEL STEL
	122 mg/m³

	OEL STEL
	20 ppm

	Ireland - Occupational Exposure Limits

	OEL TWA [2]
	10 ppm

	OEL STEL
	30 ppm (calculated)

	Latvia - Occupational Exposure Limits

	OEL TWA
	5 mg/m³

	Lithuania - Occupational Exposure Limits

	IPRV (OEL TWA)
	5 mg/m³

	Portugal - Occupational Exposure Limits

	OEL TWA
	10 ppm

	OEL chemical category
	A4 - Not Classifiable as a Human Carcinogen

	Romania - Occupational Exposure Limits

	OEL TWA
	50 mg/m³

	OEL TWA
	8 ppm

	OEL STEL
	80 mg/m³

	OEL STEL
	13 ppm

	Spain - Occupational Exposure Limits

	VLA-ED (OEL TWA) [1]
	62 mg/m³

	VLA-ED (OEL TWA) [2]
	10 ppm

	USA - ACGIH - Occupational Exposure Limits

	ACGIH OEL TWA [ppm]
	10 ppm

	ACGIH chemical category
	Not Classifiable as a Human Carcinogen



	Carbitol (111-90-0)

	Austria - Occupational Exposure Limits

	MAK (OEL TWA)
	35 mg/m³

	MAK (OEL TWA) [ppm]
	6 ppm

	MAK (OEL STEL)
	140 mg/m³

	MAK (OEL STEL) [ppm]
	24 ppm

	Estonia - Occupational Exposure Limits

	OEL TWA
	50.1 mg/m³

	OEL TWA
	10 ppm

	OEL chemical category
	Skin notation

	Germany - Occupational Exposure Limits (TRGS 900)

	AGW (OEL TWA) [1]
	35 mg/m³ (the risk of damage to the embryo or fetus can be excluded when AGW and BGW values are observed)

	AGW (OEL TWA) [2]
	6 ppm (the risk of damage to the embryo or fetus can be excluded when AGW and BGW values are observed)

	Slovenia - Occupational Exposure Limits

	OEL TWA
	35 mg/m³

	OEL TWA
	6 ppm

	OEL STEL
	70 mg/m³

	OEL STEL
	12 ppm

	Sweden - Occupational Exposure Limits

	NGV (OEL TWA)
	80 mg/m³

	NGV (OEL TWA) [ppm]
	15 ppm

	KTV (OEL STEL)
	170 mg/m³

	KTV (OEL STEL) [ppm]
	30 ppm

	OEL chemical category
	Skin notation

	Switzerland - Occupational Exposure Limits

	MAK (OEL TWA) [1]
	50 mg/m³ (aerosol, inhalable dust, vapour)

	KZGW (OEL STEL)
	100 mg/m³ (aerosol, inhalable dust, vapour)



	ethyl acetate (141-78-6)

	EU - Indicative Occupational Exposure Limit (IOEL)

	IOEL TWA
	734 mg/m³

	IOEL TWA [ppm]
	200 ppm

	IOEL STEL
	1468 mg/m³

	IOEL STEL [ppm]
	400 ppm

	Austria - Occupational Exposure Limits

	MAK (OEL TWA)
	734 mg/m³

	MAK (OEL TWA) [ppm]
	200 ppm

	MAK (OEL STEL)
	1468 mg/m³

	MAK (OEL STEL) [ppm]
	400 ppm

	Belgium - Occupational Exposure Limits

	OEL TWA
	734 mg/m³

	OEL TWA
	200 ppm

	OEL STEL
	1468 mg/m³

	OEL STEL
	400 ppm

	Bulgaria - Occupational Exposure Limits

	OEL TWA
	734 mg/m³

	OEL TWA
	200 ppm

	OEL STEL
	1468 mg/m³

	OEL STEL
	400 ppm

	Croatia - Occupational Exposure Limits

	GVI (OEL TWA) [1]
	734 mg/m³

	GVI (OEL TWA) [2]
	200 ppm

	KGVI (OEL STEL)
	1468 mg/m³

	KGVI (OEL STEL) [ppm]
	400 ppm

	Cyprus - Occupational Exposure Limits

	OEL TWA
	734 mg/m³

	OEL TWA
	200 ppm

	OEL STEL
	1468 mg/m³

	OEL STEL
	400 ppm

	Czech Republic - Occupational Exposure Limits

	PEL (OEL TWA)
	700 mg/m³

	Denmark - Occupational Exposure Limits

	OEL TWA [1]
	540 mg/m³

	OEL TWA [2]
	150 ppm

	OEL STEL
	1468 mg/m³

	OEL STEL
	400 ppm

	Estonia - Occupational Exposure Limits

	OEL TWA
	500 mg/m³

	OEL TWA
	150 ppm

	OEL STEL
	1100 mg/m³

	OEL STEL
	300 ppm

	Finland - Occupational Exposure Limits

	HTP (OEL TWA) [1]
	730 mg/m³

	HTP (OEL TWA) [2]
	200 ppm

	HTP (OEL STEL)
	1470 mg/m³

	HTP (OEL STEL) [ppm]
	400 ppm

	France - Occupational Exposure Limits

	VME (OEL TWA)
	734 mg/m³

	VME (OEL TWA) [ppm]
	200 ppm

	VLE (OEL C/STEL)
	1468 mg/m³ (restrictive limit)

	VLE (OEL C/STEL) [ppm]
	400 ppm (restrictive limit)

	Germany - Occupational Exposure Limits (TRGS 900)

	AGW (OEL TWA) [1]
	730 mg/m³ (the risk of damage to the embryo or fetus can be excluded when AGW and BGW values are observed)

	AGW (OEL TWA) [2]
	200 ppm (the risk of damage to the embryo or fetus can be excluded when AGW and BGW values are observed)

	Gibraltar - Occupational Exposure Limits

	OEL TWA
	200 mg/m³

	OEL TWA
	734 ppm

	OEL STEL
	400 mg/m³

	OEL STEL
	1468 ppm

	Greece - Occupational Exposure Limits

	OEL TWA
	734 mg/m³

	OEL TWA
	200 ppm

	OEL STEL
	1468 mg/m³

	OEL STEL
	400 ppm

	Hungary - Occupational Exposure Limits

	AK (OEL TWA)
	734 mg/m³

	CK (OEL STEL)
	1468 mg/m³

	OEL chemical category
	Sensitizer

	Ireland - Occupational Exposure Limits

	OEL TWA [1]
	734 mg/m³

	OEL TWA [2]
	200 ppm

	OEL STEL
	1468 mg/m³

	OEL STEL
	400 ppm

	Italy - Occupational Exposure Limits

	OEL TWA
	734 mg/m³

	OEL TWA
	200 ppm

	OEL STEL
	1468 mg/m³

	OEL STEL
	400 ppm

	Latvia - Occupational Exposure Limits

	OEL TWA
	200 mg/m³

	OEL TWA
	54 ppm

	Lithuania - Occupational Exposure Limits

	IPRV (OEL TWA)
	500 mg/m³

	IPRV (OEL TWA) [ppm]
	150 ppm

	NRV (OEL C)
	1100 mg/m³

	NRV (OEL C) [ppm]
	300 ppm

	Luxembourg - Occupational Exposure Limits

	OEL TWA
	734 mg/m³

	OEL TWA
	200 ppm

	OEL STEL
	1468 mg/m³

	OEL STEL
	400 ppm

	Malta - Occupational Exposure Limits

	OEL TWA
	734 mg/m³

	OEL TWA
	200 ppm

	OEL STEL
	1468 mg/m³

	OEL STEL
	400 ppm

	Netherlands - Occupational Exposure Limits

	TGG-8u (OEL TWA)
	734 mg/m³

	TGG-8u (OEL TWA) [ppm]
	200 ppm

	TGG-15min (OEL STEL)
	1468 mg/m³

	TGG-15min (OEL STEL) [ppm]
	400 ppm

	Poland - Occupational Exposure Limits

	NDS (OEL TWA)
	734 mg/m³

	NDSCh (OEL STEL)
	1468 mg/m³

	Portugal - Occupational Exposure Limits

	OEL TWA
	734 mg/m³ (indicative limit value)

	OEL TWA
	200 ppm (indicative limit value)

	OEL STEL
	1468 mg/m³ (indicative limit value)

	OEL STEL
	400 ppm (indicative limit value)

	Romania - Occupational Exposure Limits

	OEL TWA
	734 mg/m³

	OEL TWA
	200 ppm

	OEL STEL
	1468 mg/m³

	OEL STEL
	400 ppm

	Slovakia - Occupational Exposure Limits

	NPHV (OEL TWA) [1]
	734 mg/m³

	NPHV (OEL TWA) [2]
	200 ppm

	NPHV (OEL C)
	1100 mg/m³

	Slovenia - Occupational Exposure Limits

	OEL TWA
	734 mg/m³

	OEL TWA
	200 ppm

	OEL STEL
	1468 mg/m³

	OEL STEL
	400 ppm

	Spain - Occupational Exposure Limits

	VLA-ED (OEL TWA) [1]
	734 mg/m³

	VLA-ED (OEL TWA) [2]
	200 ppm

	VLA-EC (OEL STEL)
	1468 mg/m³

	VLA-EC (OEL STEL) [ppm]
	400 ppm

	Sweden - Occupational Exposure Limits

	NGV (OEL TWA)
	550 mg/m³

	NGV (OEL TWA) [ppm]
	150 ppm

	KTV (OEL STEL)
	1100 mg/m³

	KTV (OEL STEL) [ppm]
	300 ppm

	United Kingdom - Occupational Exposure Limits

	WEL TWA (OEL TWA) [1]
	734 mg/m³

	WEL TWA (OEL TWA) [2]
	200 ppm

	WEL STEL (OEL STEL)
	1468 mg/m³

	WEL STEL (OEL STEL) [ppm]
	400 ppm

	Norway - Occupational Exposure Limits

	Grenseverdi (OEL TWA) [1]
	734 mg/m³

	Grenseverdi (OEL TWA) [2]
	200 ppm

	Korttidsverdi (OEL STEL)
	1468 mg/m³ (value from the regulation)

	Korttidsverdi (OEL STEL) [ppm]
	400 ppm (value from the regulation)

	Switzerland - Occupational Exposure Limits

	MAK (OEL TWA) [1]
	730 mg/m³

	MAK (OEL TWA) [2]
	200 ppm

	KZGW (OEL STEL)
	1460 mg/m³

	KZGW (OEL STEL) [ppm]
	400 ppm

	USA - ACGIH - Occupational Exposure Limits

	ACGIH OEL TWA [ppm]
	400 ppm



	Alcohol C-10 (112-30-1)

	Bulgaria - Occupational Exposure Limits

	OEL TWA
	10 mg/m³

	Germany - Occupational Exposure Limits (TRGS 900)

	AGW (OEL TWA) [1]
	66 mg/m³ (the risk of damage to the embryo or fetus can be excluded when AGW and BGW values are observed)

	AGW (OEL TWA) [2]
	10 ppm (the risk of damage to the embryo or fetus can be excluded when AGW and BGW values are observed)

	Latvia - Occupational Exposure Limits

	OEL TWA
	10 mg/m³

	Lithuania - Occupational Exposure Limits

	IPRV (OEL TWA)
	10 mg/m³

	Romania - Occupational Exposure Limits

	OEL TWA
	100 mg/m³

	OEL TWA
	15 ppm

	OEL STEL
	200 mg/m³

	OEL STEL
	30 ppm

	Switzerland - Occupational Exposure Limits

	MAK (OEL TWA) [1]
	66 mg/m³ (aerosol, vapour)

	MAK (OEL TWA) [2]
	10 ppm (aerosol, vapour)

	KZGW (OEL STEL)
	66 mg/m³ (aerosol, vapour)

	KZGW (OEL STEL) [ppm]
	10 ppm (aerosol, vapour)



	Aldehyde C-6 (66-25-1)

	Finland - Occupational Exposure Limits

	HTP (OEL STEL)
	42 mg/m³

	HTP (OEL STEL) [ppm]
	10 ppm

	Poland - Occupational Exposure Limits

	NDS (OEL TWA)
	40 mg/m³

	NDSCh (OEL STEL)
	80 mg/m³


[bookmark: _Hlk54076527]8.1.2. Recommended monitoring procedures
No additional information available
[bookmark: _Hlk54076613]8.1.3. Air contaminants formed
No additional information available
[bookmark: _Hlk54076910]8.1.4. DNEL and PNEC
No additional information available
[bookmark: _Hlk54076968]8.1.5. Control banding
No additional information available
8.2. Exposure controls
8.2.1. Appropriate engineering controls
No additional information available
8.2.2. Personal protection equipment
	Personal protective equipment:

	Avoid all unnecessary exposure.

	Personal protective equipment symbol(s):

	[image: ]


8.2.2.1. Eye and face protection
	Eye protection:

	Chemical goggles or safety glasses


8.2.2.2. Skin protection
	Hand protection:

	Wear protective gloves.


8.2.2.3. Respiratory protection
	Respiratory protection:

	Wear appropriate mask


8.2.2.4. Thermal hazards
No additional information available
8.2.3. Environmental exposure controls
	Other information:

	Do not eat, drink or smoke during use.


SECTION 9: Physical and chemical properties
9.1. Information on basic physical and chemical properties
	Physical state
	:
	Liquid

	Colour
	:
	Standard.

	Odour
	:
	characteristic.

	Odour threshold
	:
	No data available

	pH
	:
	No data available

	Relative evaporation rate (butylacetate=1)
	:
	No data available

	Melting point
	:
	No data available

	Freezing point
	:
	No data available

	Boiling point
	:
	No data available

	Flash point
	:
	> 93 °C

	Auto-ignition temperature
	:
	No data available

	Decomposition temperature
	:
	No data available

	Flammability (solid, gas)
	:
	Non flammable.

	Vapour pressure
	:
	No data available

	Relative vapour density at 20°C
	:
	No data available

	Relative density
	:
	No data available

	Solubility
	:
	No data available

	Partition coefficient n-octanol/water (Log Pow)
	:
	No data available

	Viscosity, kinematic
	:
	No data available

	Viscosity, dynamic
	:
	No data available

	Explosive properties
	:
	No data available

	Oxidising properties
	:
	No data available

	Explosive limits
	:
	No data available


9.2. Other information
No additional information available
SECTION 10: Stability and reactivity
10.1. Reactivity
No additional information available
10.2. Chemical stability
Not established.
10.3. Possibility of hazardous reactions
Not established.
10.4. Conditions to avoid
Direct sunlight. Extremely high or low temperatures.
10.5. Incompatible materials
Strong acids. Strong bases.
10.6. Hazardous decomposition products
fume. Carbon monoxide. Carbon dioxide.
SECTION 11: Toxicological information
11.1 Information on toxicological effects
	Acute toxicity (oral)
	:
	Not classified

	Acute toxicity (dermal)
	:
	Not classified

	Acute toxicity (inhalation)
	:
	Not classified



	benzyl benzoate (120-51-4)

	LD50 oral rat
	500 mg/kg (Source: NLM_CIP)

	LD50 oral
	1160 mg/kg bodyweight

	LD50 dermal rabbit
	4000 mg/kg (Source: NLM_CIP)



	Ethyl linalool (10339-55-6)

	LD50 oral
	5000 mg/kg bodyweight

	LD50 dermal rabbit
	> 5000 mg/kg (Source: ECHA_API)



	Hexyl salicylate (6259-76-3)

	LD50 oral rat
	> 5 g/kg (Source: NLM_CIP)

	LD50 dermal rabbit
	> 5000 mg/kg (Source: ECHA_API)



	Hexyl cinnamic aldehyde (101-86-0)

	LD50 oral rat
	3100 mg/kg (Source: NLM_CIP)

	LD50 oral
	3100 mg/kg bodyweight

	LD50 dermal rabbit
	> 3000 mg/kg (Source: EPA_HPV)

	LC50 Inhalation - Rat
	> 5 mg/l/4h



	2-phenoxyethanol (122-99-6)

	LD50 oral rat
	1850 mg/kg (Source: EU_CLH)

	LD50 oral
	1394 mg/kg bodyweight

	LD50 dermal rabbit
	5 ml/kg (Source: NLM_CIP)

	LC50 Inhalation - Rat
	> 0.057 mg/l (Exposure time: 8 h Source: EU_CLH)



	Helional (1205-17-0)

	LD50 dermal rabbit
	> 2000 mg/kg (Source: ECHA_API)



	Benzyl salicylate (118-58-1)

	LD50 oral rat
	2227 mg/kg (Source: NLM_CIP)

	LD50 oral
	2200 mg/kg bodyweight

	LD50 dermal rabbit
	> 5000 mg/kg (Source: CHEMVIEW)



	ACETYL HEXAMETHYL TETRALIN (21145-77-7)

	LD50 oral rat
	570 mg/kg (Source: NLM_CIP)

	LD50 oral
	1000 mg/kg bodyweight

	LD50 dermal rabbit
	> 5 g/kg (Source: NLM_HSDB)



	Citronellol Pure (106-22-9)

	LD50 oral rat
	3450 mg/kg (Source: NLM_CIP)

	LD50 oral
	3450 mg/kg bodyweight

	LD50 dermal rabbit
	2650 mg/kg (Source: EPA_HPV)

	LD50 dermal
	2650 mg/kg bodyweight



	Linalyl acetate (115-95-7)

	LD50 oral rat
	14550 mg/kg (Source: EPA_HPV)

	LD50 dermal rabbit
	> 5000 mg/kg (Source: EPA_HPV)



	Benzyl acetate (140-11-4)

	LD50 oral rat
	2490 mg/kg (Source: JAPAN_GHS)

	LD50 oral
	2490 mg/kg bodyweight

	LD50 dermal rabbit
	> 5000 mg/kg (Source: JAPAN_GHS)



	Carbitol (111-90-0)

	LD50 oral rat
	10502 mg/kg (Source: OECD_SIDS)

	LD50 dermal rabbit
	9143 mg/kg (Source: OECD_SIDS)

	LC50 Inhalation - Rat
	> 5240 mg/m³ (Exposure time: 4 h Source: NLM_CIP)



	ethyl acetate (141-78-6)

	LD50 oral rat
	5620 mg/kg (Source: NLM_CIP)

	LD50 dermal rabbit
	> 18000 mg/kg (Source: JAPAN_GHS)

	LC50 Inhalation - Rat [ppm]
	4000 ppm/4h



	Alcohol C-10 (112-30-1)

	LD50 oral rat
	4720 mg/kg (Source: NZ_CCID)

	LD50 dermal rabbit
	3560 mg/kg (Source: NLM_CIP)



	Aldehyde C-6 (66-25-1)

	LD50 oral rat
	4890 mg/kg (Source: NLM_CIP)

	LD50 dermal rabbit
	> 8100 mg/kg (Source: ECHA_API)



	Skin corrosion/irritation
	:
	Not classified

	Additional information
	:
	Based on available data, the classification criteria are not met



	Serious eye damage/irritation
	:
	Not classified

	Additional information
	:
	Based on available data, the classification criteria are not met



	Respiratory or skin sensitisation
	:
	Not classified

	Additional information
	:
	Based on available data, the classification criteria are not met



	Germ cell mutagenicity
	:
	Not classified

	Additional information
	:
	Based on available data, the classification criteria are not met



	Carcinogenicity
	:
	Not classified

	Additional information
	:
	Based on available data, the classification criteria are not met 



	Benzyl acetate (140-11-4)

	IARC group
	3 - Not classifiable



	Reproductive toxicity
	:
	Not classified

	Additional information
	:
	Based on available data, the classification criteria are not met



	STOT-single exposure
	:
	Not classified

	Additional information
	:
	Based on available data, the classification criteria are not met



	2-phenoxyethanol (122-99-6)

	STOT-single exposure
	May cause respiratory irritation. 



	ethyl acetate (141-78-6)

	STOT-single exposure
	May cause drowsiness or dizziness. 



	STOT-repeated exposure
	:
	Not classified

	Additional information
	:
	Based on available data, the classification criteria are not met



	Aspiration hazard
	:
	Not classified

	Additional information
	:
	Based on available data, the classification criteria are not met



	benzyl benzoate (120-51-4)

	Viscosity, kinematic
	7.456 mm²/s



	Potential adverse human health effects and symptoms
	:
	Based on available data, the classification criteria are not met


SECTION 12: Ecological information
12.1. Toxicity
	Hazardous to the aquatic environment, short–term (acute)
	:
	Not classified

	Hazardous to the aquatic environment, long–term (chronic)
	:
	Harmful to aquatic life with long lasting effects.



	benzyl benzoate (120-51-4)

	LC50 - Fish [1]
	2.32 mg/l (Exposure time: 96 h - Species: Danio rerio [semi-static] Source: ECHA)

	NOEC (chronic)
	0.168 mg/l



	Ethyl linalool (10339-55-6)

	LC50 - Fish [1]
	24 mg/l (Exposure time: 96 h - Species: Danio rerio [semi-static] Source: ECHA)



	2-phenoxyethanol (122-99-6)

	LC50 - Fish [1]
	337 – 352 mg/l (Exposure time: 96 h - Species: Pimephales promelas [flow-through] Source: EPA)

	LC50 - Fish [2]
	366 mg/l (Exposure time: 96 h - Species: Pimephales promelas [static] Source: IUCLID)

	EC50 - Crustacea [1]
	> 500 mg/l (Exposure time: 48 h - Species: Daphnia magna)

	EC50 72h - Algae [1]
	> 500 mg/l (Species: Desmodesmus subspicatus)



	Benzyl salicylate (118-58-1)

	LC50 - Fish [1]
	1.03 mg/l (Exposure time: 96 h - Species: Danio rerio [semi-static] Source: ECHA)



	Linalyl acetate (115-95-7)

	LC50 - Fish [1]
	11 mg/l (Exposure time: 96 h - Species: Cyprinus carpio [flow-through] Source: ECHA)



	Carbitol (111-90-0)

	LC50 - Fish [1]
	10000 mg/l (Exposure time: 96 h - Species: Lepomis macrochirus [static] Source: EPA)

	LC50 - Fish [2]
	19100 – 23900 mg/l (Exposure time: 96 h - Species: Lepomis macrochirus [flow-through] Source: EPA)

	EC50 - Crustacea [1]
	3940 – 4670 mg/l (Exposure time: 48 h - Species: Daphnia magna)



	ethyl acetate (141-78-6)

	LC50 - Fish [1]
	220 – 250 mg/l (Exposure time: 96 h - Species: Pimephales promelas [flow-through] Source: EPA)

	LC50 - Fish [2]
	484 mg/l (Exposure time: 96 h - Species: Oncorhynchus mykiss [flow-through] Source: IUCLID)

	EC50 - Crustacea [1]
	560 mg/l (Exposure time: 48 h - Species: Daphnia magna [Static])



	Alcohol C-10 (112-30-1)

	LC50 - Fish [1]
	2.2 – 2.5 mg/l (Exposure time: 96 h - Species: Pimephales promelas [flow-through] Source: EPA)

	LC50 - Fish [2]
	4.12 – 6.2 mg/l (Exposure time: 96 h - Species: Lepomis macrochirus [static] Source: EPA)

	EC50 - Crustacea [1]
	3 mg/l (Exposure time: 48 h - Species: Daphnia magna)



	Aldehyde C-6 (66-25-1)

	LC50 - Fish [1]
	12 – 16.5 mg/l (Exposure time: 96 h - Species: Pimephales promelas [flow-through] Source: EPA)


12.2. Persistence and degradability
	J'Adore Type #EU30835F 25% in DPG 

	Persistence and degradability
	Not established.



	benzyl benzoate (120-51-4)

	Persistence and degradability
	May cause long-term adverse effects in the environment.


12.3. Bioaccumulative potential
	J'Adore Type #EU30835F 25% in DPG 

	Bioaccumulative potential
	Not established.



	benzyl benzoate (120-51-4)

	Partition coefficient n-octanol/water (Log Pow)
	3.97 (at 25 °C)

	Bioaccumulative potential
	Not established.



	Ethyl linalool (10339-55-6)

	Partition coefficient n-octanol/water (Log Pow)
	3.3 (at 20 °C)



	Hexyl salicylate (6259-76-3)

	Partition coefficient n-octanol/water (Log Pow)
	5.5 (at 30 °C (at pH 7)



	2-phenoxyethanol (122-99-6)

	Partition coefficient n-octanol/water (Log Pow)
	1.107



	Helional (1205-17-0)

	Partition coefficient n-octanol/water (Log Pow)
	2.4 (at 25 °C)



	Benzyl salicylate (118-58-1)

	Partition coefficient n-octanol/water (Log Pow)
	4



	ACETYL HEXAMETHYL TETRALIN (21145-77-7)

	Partition coefficient n-octanol/water (Log Pow)
	5.7 (at 24 °C)



	Citronellol Pure (106-22-9)

	Partition coefficient n-octanol/water (Log Pow)
	3.41 (at 25 °C)



	Linalyl acetate (115-95-7)

	Partition coefficient n-octanol/water (Log Pow)
	3.9 (at 25 °C)



	Benzyl acetate (140-11-4)

	Partition coefficient n-octanol/water (Log Pow)
	1.96 (at 25 °C (at pH 7)



	Carbitol (111-90-0)

	Partition coefficient n-octanol/water (Log Pow)
	-0.8



	ethyl acetate (141-78-6)

	BCF - Fish [1]
	(30 dimensionless)

	Partition coefficient n-octanol/water (Log Pow)
	0.73 (at 20 °C (at pH 7)



	Alcohol C-10 (112-30-1)

	Partition coefficient n-octanol/water (Log Pow)
	4.5 (at 25 °C (at pH 6)



	Aldehyde C-6 (66-25-1)

	Partition coefficient n-octanol/water (Log Pow)
	2.3 (at 25 °C (at pH 5)


12.4. Mobility in soil
No additional information available
12.5. Results of PBT and vPvB assessment
No additional information available
12.6. Other adverse effects
	Additional information
	:
	Avoid release to the environment.


SECTION 13: Disposal considerations
13.1. Waste treatment methods
	Product/Packaging disposal recommendations
	:
	Dispose in a safe manner in accordance with local/national regulations.

	Ecology - waste materials
	:
	Avoid release to the environment.

	HP Code
	:
	HP3 - “Flammable:” 
– flammable liquid waste: liquid waste having a flash point below 60 °C or waste gas oil, diesel and light heating oils having a flash point > 55 °C and ≤ 75 °C; 
– flammable pyrophoric liquid and solid waste: solid or liquid waste which, even in small quantities, is liable to ignite within five minutes after coming into contact with air; 
– flammable solid waste: solid waste which is readily combustible or may cause or contribute to fire through friction; 
– flammable gaseous waste: gaseous waste which is flammable in air at 20 °C and a standard pressure of 101.3 kPa; 
– water reactive waste: waste which, in contact with water, emits flammable gases in dangerous quantities; 
– other flammable waste: flammable aerosols, flammable self-heating waste, flammable organic peroxides and flammable self-reactive waste.
HP14 - “Ecotoxic:” waste which presents or may present immediate or delayed risks for one or more sectors of the environment


SECTION 14: Transport information
In accordance with ADR / IMDG / IATA / ADN / RID
	ADR
	IMDG
	IATA
	ADN
	RID

	14.1. UN number

	Not applicable
	Not applicable
	Not applicable
	Not applicable
	Not applicable

	14.2. UN proper shipping name

	Not applicable
	Not applicable
	Not applicable
	Not applicable
	Not applicable

	14.3. Transport hazard class(es)

	Not applicable
	Not applicable
	Not applicable
	Not applicable
	Not applicable

	14.4. Packing group

	Not applicable
	Not applicable
	Not applicable
	Not applicable
	Not applicable

	14.5. Environmental hazards

	Not applicable
	Not applicable
	Not applicable
	Not applicable
	Not applicable

	No supplementary information available


14.6. Special precautions for user
	Overland transport

	Not applicable



	Transport by sea

	Not applicable



	Air transport

	Not applicable



	Inland waterway transport

	Not applicable



	Rail transport

	Not applicable


14.7. Transport in bulk according to Annex II of Marpol and the IBC Code
Not applicable
SECTION 15: Regulatory information
15.1. Safety, health and environmental regulations/legislation specific for the substance or mixture
15.1.1. EU-Regulations
REACH Annex XVII (Restriction List)
	EU restriction list (REACH Annex XVII)

	Reference code
	Applicable on
	Entry title or description

	3(a)
	ethyl acetate ; Aldehyde C-6
	Substances or mixtures fulfilling the criteria for any of the following hazard classes or categories set out in Annex I to Regulation (EC) No 1272/2008: Hazard classes 2.1 to 2.4, 2.6 and 2.7, 2.8 types A and B, 2.9, 2.10, 2.12, 2.13 categories 1 and 2, 2.14 categories 1 and 2, 2.15 types A to F

	3(b)
	benzyl benzoate ; Ethyl linalool ; Hexyl salicylate ; Hexyl cinnamic aldehyde ; 2-phenoxyethanol ; Helional ; Benzyl salicylate ; Citronellol Pure ; Linalyl acetate ; ethyl acetate
	Substances or mixtures fulfilling the criteria for any of the following hazard classes or categories set out in Annex I to Regulation (EC) No 1272/2008: Hazard classes 3.1 to 3.6, 3.7 adverse effects on sexual function and fertility or on development, 3.8 effects other than narcotic effects, 3.9 and 3.10

	3(c)
	J'Adore Type #EU30835F 25% in DPG ; benzyl benzoate ; Hexyl salicylate ; Hexyl cinnamic aldehyde ; Helional ; Benzyl salicylate ; Benzyl acetate ; Alcohol C-10
	Substances or mixtures fulfilling the criteria for any of the following hazard classes or categories set out in Annex I to Regulation (EC) No 1272/2008: Hazard class 4.1

	40.
	ethyl acetate ; Aldehyde C-6
	Substances classified as flammable gases category 1 or 2, flammable liquids categories 1, 2 or 3, flammable solids category 1 or 2, substances and mixtures which, in contact with water, emit flammable gases, category 1, 2 or 3, pyrophoric liquids category 1 or pyrophoric solids category 1, regardless of whether they appear in Part 3 of Annex VI to Regulation (EC) No 1272/2008 or not.


REACH Annex XIV (Authorisation List)
Contains no substance(s) listed on REACH Annex XIV (Authorisation List)
REACH Candidate List (SVHC)
Contains no substance(s) listed on the REACH Candidate List
PIC Regulation (Prior Informed Consent)
Contains no substance(s) listed on the PIC list (Regulation EU 649/2012 concerning the export and import of hazardous chemicals)
POP Regulation (Persistent Organic Pollutants)
Contains no substance(s) listed on the POP list (Regulation EU 2019/1021 on persistent organic pollutants)
Ozone Regulation (1005/2009)
Contains no substance(s) listed on the Ozone Depletion list (Regulation EU 1005/2009 on substances that deplete the ozone layer)
Explosives Precursors Regulation (2019/1148)
Contains no substance(s) listed on the Explosives Precursors list (Regulation EU 2019/1148 on the marketing and use of explosives precursors)
Drug Precursors Regulation (273/2004)
Contains substance(s) listed on the Drug Precursors list (Regulation EC 273/2004 on the manufacture and the placing on market of certain substances used in the illicit manufacture of narcotic drugs and psychotropic substances)
15.1.2. National regulations
	France

		Occupational diseases

	Code
	Description

	RG 84
	Conditions caused by liquid organic solvents for professional use: saturated or unsaturated aliphatic or cyclic liquid hydrocarbons and mixtures thereof; liquid halogenated hydrocarbons; nitrated derivatives of aliphatic hydrocarbons; alcohols; glycols, glycol ethers; ketones; aldehydes; aliphatic and cyclic ethers, including tetrahydrofuran; esters; dimethylformamide and dimethylacetamine; acetonitrile and propionitrile; pyridine; dimethylsulfone and dimethylsulfoxide




	Germany

	Water hazard class (WGK)
	:
	WGK 2, Significantly hazardous to water (Classification according to AwSV, Annex 1).

	Storage class (LGK, TRGS 510)
	:
	LGK 12 - Non-combustible liquids.

	Joint storage table
	:
	[image: ]

	Joint storage not permitted for
	:
	LGK 1, LGK 6.2, LGK 7.

	Joint storage with restrictions permitted for
	:
	LGK 4.1A, LGK 4.3, LGK 5.1C.

	Joint storage permitted for
	:
	LGK 2A, LGK 2B, LGK 3, LGK 4.1B, LGK 4.2, LGK 5.1A, LGK 5.1B, LGK 5.2, LGK 6.1A, LGK 6.1B, LGK 6.1C, LGK 6.1D, LGK 8A, LGK 8B, LGK 10, LGK 11, LGK 12, LGK 13, LGK 10-13.

	Hazardous Incident Ordinance (12. BImSchV)
	:
	 Is not subject of the Hazardous Incident Ordinance (12. BImSchV)

	Netherlands

	ABM category
	:
	A(2) - toxic for aquatic organisms, may have longterm hazardous effects in aquatic environment

	SZW-lijst van kankerverwekkende stoffen
	:
	None of the components are listed

	SZW-lijst van mutagene stoffen
	:
	None of the components are listed

	SZW-lijst van reprotoxische stoffen – Borstvoeding
	:
	None of the components are listed

	SZW-lijst van reprotoxische stoffen – Vruchtbaarheid
	:
	None of the components are listed

	SZW-lijst van reprotoxische stoffen – Ontwikkeling
	:
	None of the components are listed

	Denmark

	Classification remarks
	:
	Emergency management guidelines for the storage of flammable liquids must be followed

	Danish National Regulations
	:
	Pregnant/breastfeeding women working with the product must not be in direct contact with the product

	Switzerland

	Storage class (LK)
	:
	LK 10/12 - Liquids


15.2. Chemical safety assessment
No chemical safety assessment has been carried out
SECTION 16: Other information
	Data sources
	:
	REGULATION (EC) No 1272/2008 OF THE EUROPEAN PARLIAMENT AND OF THE COUNCIL of 16 December 2008 on classification, labelling and packaging of substances and mixtures, amending and repealing Directives 67/548/EEC and 1999/45/EC, and amending Regulation (EC) No 1907/2006.

	Other information
	:
	None.



	Full text of H- and EUH-statements:

	Acute Tox. 4 (Oral)
	Acute toxicity (oral), Category 4

	Aquatic Acute 1
	Hazardous to the aquatic environment – Acute Hazard, Category 1

	Aquatic Chronic 1
	Hazardous to the aquatic environment – Chronic Hazard, Category 1

	Aquatic Chronic 2
	Hazardous to the aquatic environment – Chronic Hazard, Category 2

	Aquatic Chronic 3
	Hazardous to the aquatic environment – Chronic Hazard, Category 3

	EUH208
	Contains Ethyl linalool, Hexyl salicylate, Hexyl cinnamic aldehyde, Helional, Benzyl salicylate, Citronellol Pure, Linalyl acetate. May produce an allergic reaction.

	Eye Dam. 1
	Serious eye damage/eye irritation, Category 1

	Eye Irrit. 2
	Serious eye damage/eye irritation, Category 2

	Flam. Liq. 1
	Flammable liquids, Category 1

	Flam. Liq. 3
	Flammable liquids, Category 3

	H224
	Extremely flammable liquid and vapour.

	H226
	Flammable liquid and vapour.

	H302
	Harmful if swallowed.

	H315
	Causes skin irritation.

	H317
	May cause an allergic skin reaction.

	H318
	Causes serious eye damage.

	H319
	Causes serious eye irritation.

	H335
	May cause respiratory irritation.

	H336
	May cause drowsiness or dizziness.

	H361
	Suspected of damaging fertility or the unborn child.

	H400
	Very toxic to aquatic life.

	H410
	Very toxic to aquatic life with long lasting effects.

	H411
	Toxic to aquatic life with long lasting effects.

	H412
	Harmful to aquatic life with long lasting effects.

	Repr. 2
	Reproductive toxicity, Category 2

	Skin Irrit. 2
	Skin corrosion/irritation, Category 2

	Skin Sens. 1
	Skin sensitisation, Category 1

	Skin Sens. 1B
	Skin sensitisation, category 1B

	STOT SE 3
	Specific target organ toxicity – Single exposure, Category 3, Respiratory tract irritation



	The classification complies with
	:
	ATP 12


Safety Data Sheet (SDS), EU
This information is based on our current knowledge and is intended to describe the product for the purposes of health, safety and environmental requirements only. It should not therefore be construed as guaranteeing any specific property of the product.
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