	JAPANESE BAMBOO #EU47242F 5% in DPG

	Safety Data Sheet
	

	according to Regulation (EC) No. 1907/2006 (REACH) with its amendment Regulation (EU) 2020/878
Issue date: 6/25/2024   
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	Safety Data Sheet
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SECTION 1: Identification of the substance/mixture and of the company/undertaking
1.1. Product identifier
	Product form
	:
	Mixture

	Product name
	:
	JAPANESE BAMBOO #EU47242F 5% in DPG

	Product code
	:
	EU47242F_5%

	Type of product
	:
	Perfumes, Fragrances


1.2. Relevant identified uses of the substance or mixture and uses advised against
1.2.1. Relevant identified uses
	Industrial/Professional use spec
	:
	Industrial
For professional use only

	Use of the substance/mixture
	:
	Perfumes, Fragrances

	Function or use category
	:
	Odour agents


1.2.2. Uses advised against
No additional information available
1.3. Details of the supplier of the safety data sheet
No additional information available
1.4. Emergency telephone number
No additional information available
SECTION 2: Hazards identification
2.1. Classification of the substance or mixture
Classification according to Regulation (EC) No. 1272/2008 [CLP]
	Skin sensitization, Category 1
	H317 
	
	


Full text of H- and EUH-statements: see section 16
Adverse physicochemical, human health and environmental effects
No additional information available
2.2. Label elements
Labeling according to Regulation (EC) No. 1272/2008 [CLP]
	Hazard pictograms (CLP)
	:
	[image: ]
	
	
	
	
	

	
	
	GHS07
	
	
	
	
	

	Signal word (CLP)
	:
	Warning

	Contains
	:
	Hexyl cinnamic aldehyde; Hydroxy; Helional; Amyl cinnamic aldehyde; isoeugenol; Citronellol Pure; Linalool

	Hazard statements (CLP)
	:
	H317 - May cause an allergic skin reaction.

	Precautionary statements (CLP)
	:
	P261 - Avoid breathing dust/fume/gas/mist/vapors/spray.
P272 - Contaminated work clothing should not be allowed out of the workplace.
P280 - Wear protective gloves/protective clothing/eye protection/face protection/hearing protection.
P302+P352 - IF ON SKIN: Wash with plenty of water.
P321 - Specific treatment (see supplemental first aid instruction on this label).
P333+P313 - If skin irritation or rash occurs: Get medical advice/attention.

	Extra phrases
	:
	Restricted to professional users.


2.3. Other hazards
	Contains no PBT and/or vPvB substances ≥ 0.1% assessed in accordance with REACH Annex XIII



	The mixture does not contain substance(s) included in the list established in accordance with Article 59(1) of REACH for having endocrine disrupting properties, or substance(s) are not identified as having endocrine disrupting properties in accordance with the criteria set out in Commission Delegated Regulation (EU) 2017/2100 or Commission Regulation (EU) 2018/605 at a concentration equal to or greater than 0,1 %



SECTION 3: Composition/Information on ingredients
3.1. Substances
Not applicable
3.2. Mixtures
	Name
	Product identifier
	%
	Classification according to Regulation (EC) No. 1272/2008 [CLP]

	Linalool
	CAS-No.: 78-70-6
EC-No.: 201-134-4
EC Index-No.: 603-235-00-2
REACH-no: 01-2119474016-42
	0.185 – 0.365
	Skin Irrit. 2, H315
Eye Irrit. 2, H319
Skin Sens. 1B, H317

	benzyl benzoate
	CAS-No.: 120-51-4
EC-No.: 204-402-9
EC Index-No.: 607-085-00-9
REACH-no: 01-2119976371-33
	0.16 – 0.3235
	Acute Tox. 4 (Oral), H302
Aquatic Acute 1, H400
Aquatic Chronic 2, H411

	Undecavertol
	CAS-No.: 81782-77-6
EC-No.: 279-815-0
	0.115 – 0.23
	Aquatic Acute 1, H400
Aquatic Chronic 2, H411

	Hexyl cinnamic aldehyde
	CAS-No.: 101-86-0
EC-No.: 202-983-3
REACH-no: 01-2119533092-50
	0.1 – 0.2
	Skin Sens. 1, H317
Aquatic Chronic 2, H411

	Citronellol Pure
	CAS-No.: 106-22-9
EC-No.: 203-375-0
REACH-no: 01-2119453995-23
	0.09 – 0.18
	Skin Irrit. 2, H315
Eye Irrit. 2, H319
Skin Sens. 1B, H317

	Amyl cinnamic aldehyde
	CAS-No.: 122-40-7
EC-No.: 204-541-5
	0.09 – 0.1775
	Skin Sens. 1B, H317
Aquatic Chronic 2, H411

	Helional
	CAS-No.: 1205-17-0
EC-No.: 214-881-6
REACH-no: 01-2120740119-58
	0.085 – 0.171
	Skin Sens. 1B, H317
Repr. 2, H361
Aquatic Chronic 2, H411

	Benzyl acetate
substance with national workplace exposure limit(s) (BE, DK, ES, IE, LT, LV, PT, RO)
	CAS-No.: 140-11-4
EC-No.: 205-399-7
REACH-no: 01-2119638272-42
	0.07 – 0.1425
	Aquatic Chronic 3, H412

	Carbitol
substance with national workplace exposure limit(s) (AT, DE, EE, SE, SI, CH)
	CAS-No.: 111-90-0
EC-No.: 203-919-7
REACH-no: 01-2119475105-42
	0.0542475 – 0.108495
	Not classified

	Hydroxy
	CAS-No.: 107-75-5
EC-No.: 203-518-7
REACH-no: 01-2119973482-31
	0.055805 – 0.10661
	Eye Irrit. 2, H319
Skin Sens. 1B, H317

	Bacdanol
	CAS-No.: 28219-61-6
EC-No.: 248-908-8
REACH-no: 01-2119529224-45
	0.05 – 0.1
	Skin Irrit. 2, H315
Eye Irrit. 2, H319
Aquatic Chronic 1, H410

	ethanol, ethyl alcohol
substance with national workplace exposure limit(s) (AT, BE, BG, CZ, DE, DK, EE, ES, FI, FR, GB, GR, HR, HU, IE, LT, LV, NL, PL, PT, RO, SE, SI, SK, NO, CH)
	CAS-No.: 64-17-5
EC-No.: 200-578-6
EC Index-No.: 603-002-00-5
	0.025 – 0.0475
	Flam. Liq. 2, H225

	isoeugenol
	CAS-No.: 97-54-1
EC-No.: 202-590-7
EC Index-No.: 604-094-00-X; 202-590-1
REACH-no: 17-2119417630-49
	0.005 – 0.0125
	Acute Tox. 4 (Oral), H302
Acute Tox. 4 (Dermal), H312
Acute Tox. 4 (Inhalation), H332
Skin Irrit. 2, H315
Eye Irrit. 2, H319
Skin Sens. 1A, H317
Carc. 2, H351
STOT SE 3, H335

	Diphenyl oxide
substance with national workplace exposure limit(s) (AT, BE, BG, CY, CZ, DE, DK, EE, ES, FI, FR, GB, GI, GR, HR, HU, IE, IT, LT, LU, LV, MT, NL, PL, PT, RO, SE, SI, SK, NO, CH); substance with a Community workplace exposure limit
	CAS-No.: 101-84-8
EC-No.: 202-981-2
REACH-no: 01-2119472545-33
	0 – 0.0025
	Eye Irrit. 2, H319
Aquatic Acute 1, H400
Aquatic Chronic 1, H410

	Alcohol C-10
substance with national workplace exposure limit(s) (BG, DE, LT, LV, RO, CH)
	CAS-No.: 112-30-1
EC-No.: 203-956-9
	0 – 0.00035
	Aquatic Chronic 3, H412

	Aldehyde C-6
substance with national workplace exposure limit(s) (FI, PL)
	CAS-No.: 66-25-1
EC-No.: 200-624-5
	0 – 0.00009
	Flam. Liq. 3, H226

	Caproic acid
substance with national workplace exposure limit(s) (BG, LT, LV)
	CAS-No.: 142-62-1
EC-No.: 205-550-7
	0 – 0.000005
	Eye Dam. 1, H318
Skin Corr. 1C, H314



	Specific concentration limits:

	Name
	Product identifier
	Specific concentration limits (%)

	isoeugenol
	CAS-No.: 97-54-1
EC-No.: 202-590-7
EC Index-No.: 604-094-00-X; 202-590-1
REACH-no: 17-2119417630-49
	(0.01 ≤ C ≤ 100) Skin Sens. 1A, H317


Full text of H- and EUH-statements: see section 16
SECTION 4: First aid measures
4.1. Description of first aid measures
	First-aid measures general
	:
	Never give anything by mouth to an unconscious person. If you feel unwell, seek medical advice (show the label where possible).

	First-aid measures after inhalation
	:
	Allow affected person to breathe fresh air. Allow the victim to rest.

	First-aid measures after skin contact
	:
	Remove affected clothing and wash all exposed skin area with mild soap and water, followed by warm water rinse.

	First-aid measures after eye contact
	:
	Rinse immediately with plenty of water. Obtain medical attention if pain, blinking or redness persists.

	First-aid measures after ingestion
	:
	Rinse mouth. Do NOT induce vomiting. Obtain emergency medical attention.


4.2. Most important symptoms and effects, both acute and delayed
	Symptoms/effects
	:
	Not expected to present a significant hazard under anticipated conditions of normal use.


4.3. Indication of any immediate medical attention and special treatment needed
No additional information available
SECTION 5: Firefighting measures
5.1. Extinguishing media
	Suitable extinguishing media
	:
	Foam. Dry powder. Carbon dioxide. Water spray. Sand.

	Unsuitable extinguishing media
	:
	Do not use a heavy water stream.


5.2. Special hazards arising from the substance or mixture
No additional information available
5.3. Advice for firefighters
	Firefighting instructions
	:
	Use water spray or fog for cooling exposed containers. Exercise caution when fighting any chemical fire. Prevent fire-fighting water from entering environment.

	Protection during firefighting
	:
	Do not enter fire area without proper protective equipment, including respiratory protection.


SECTION 6: Accidental release measures
6.1. Personal precautions, protective equipment and emergency procedures
6.1.1. For non-emergency personnel
	Emergency procedures
	:
	Evacuate unnecessary personnel.


6.1.2. For emergency responders
	Protective equipment
	:
	Equip cleanup crew with proper protection.

	Emergency procedures
	:
	Ventilate area.


6.2. Environmental precautions
Prevent entry to sewers and public waters. Notify authorities if liquid enters sewers or public waters.
6.3. Methods and material for containment and cleaning up
	Methods for cleaning up
	:
	Soak up spills with inert solids, such as clay or diatomaceous earth as soon as possible. Collect spillage. Store away from other materials.


6.4. Reference to other sections
See Heading 8. Exposure controls and personal protection.
SECTION 7: Handling and storage
7.1. Precautions for safe handling
	Precautions for safe handling
	:
	Wash hands and other exposed areas with mild soap and water before eating, drinking or smoking and when leaving work. Provide good ventilation in process area to prevent formation of vapor.


7.2. Conditions for safe storage, including any incompatibilities
	Storage conditions
	:
	Keep only in the original container in a cool, well ventilated place away from : Keep container closed when not in use.

	Incompatible products
	:
	Strong bases. Strong acids.

	Incompatible materials
	:
	Sources of ignition. Direct sunlight.

	Germany

	Storage class (LGK, TRGS 510)
	:
	LGK 12 - Non-combustible liquids

	Joint storage table
	:
	[image: ]

	Joint storage not permitted for
	:
	LGK 1, LGK 6.2, LGK 7

	Joint storage with restrictions permitted for
	:
	LGK 4.1A, LGK 4.3, LGK 5.1C

	Joint storage permitted for
	:
	LGK 2A, LGK 2B, LGK 3, LGK 4.1B, LGK 4.2, LGK 5.1A, LGK 5.1B, LGK 5.2, LGK 6.1A, LGK 6.1B, LGK 6.1C, LGK 6.1D, LGK 8A, LGK 8B, LGK 10, LGK 11, LGK 12, LGK 13, LGK 10-13

	Switzerland

	Storage class (LK)
	:
	LK 10/12 - Liquids


7.3. Specific end use(s)
No additional information available
SECTION 8: Exposure controls/personal protection
8.1. Control parameters
[bookmark: _Hlk54076387]8.1.1 National occupational exposure and biological limit values

	Diphenyl oxide (101-84-8)

	EU - Indicative Occupational Exposure Limit (IOEL)

	IOEL TWA
	7 mg/m³

	IOEL TWA
	1 ppm

	IOEL STEL
	14 mg/m³

	IOEL STEL
	2 ppm

	Austria - Occupational Exposure Limits

	MAK (OEL TWA)
	7 mg/m³

	MAK (OEL TWA)
	1 ppm

	MAK (OEL STEL)
	14 mg/m³

	MAK (OEL STEL)
	2 ppm

	Belgium - Occupational Exposure Limits

	OEL TWA
	7 mg/m³ (vapor)

	OEL TWA
	1 ppm (vapor)

	OEL STEL
	14 mg/m³ (vapor)

	OEL STEL
	2 ppm (vapor)

	Bulgaria - Occupational Exposure Limits

	OEL TWA
	7 mg/m³

	OEL TWA
	1 ppm

	OEL STEL
	14 mg/m³

	OEL STEL
	2 ppm

	Croatia - Occupational Exposure Limits

	GVI (OEL TWA)
	7 mg/m³

	GVI (OEL TWA)
	1 ppm

	KGVI (OEL STEL)
	14 mg/m³

	KGVI (OEL STEL)
	2 ppm

	Cyprus - Occupational Exposure Limits

	OEL TWA
	7 mg/m³

	OEL TWA
	1 ppm

	OEL STEL
	14 mg/m³

	OEL STEL
	2 ppm

	Czech Republic - Occupational Exposure Limits

	PEL (OEL TWA)
	5 mg/m³

	Denmark - Occupational Exposure Limits

	OEL TWA
	7 mg/m³

	OEL TWA
	1 ppm

	OEL STEL
	14 mg/m³

	OEL STEL
	2 ppm

	Estonia - Occupational Exposure Limits

	OEL TWA
	7 mg/m³

	OEL TWA
	1 ppm

	OEL STEL
	14 mg/m³

	OEL STEL
	2 ppm

	Finland - Occupational Exposure Limits

	HTP (OEL TWA)
	7 mg/m³

	HTP (OEL TWA)
	1 ppm

	HTP (OEL STEL)
	14 mg/m³

	HTP (OEL STEL)
	2 ppm

	France - Occupational Exposure Limits

	VME (OEL TWA)
	7 mg/m³ (indicative limit)

	VME (OEL TWA)
	1 ppm (indicative limit)

	VLE (OEL C/STEL)
	14 mg/m³ (indicative limit)

	VLE (OEL C/STEL)
	2 ppm (indicative limit)

	Germany - Occupational Exposure Limits (TRGS 900)

	AGW (OEL TWA)
	7.1 mg/m³ (the risk of damage to the embryo or fetus can be excluded when AGW and BGW values are observed-vapor)

	AGW (OEL TWA)
	1 ppm (the risk of damage to the embryo or fetus can be excluded when AGW and BGW values are observed-vapor)

	Gibraltar - Occupational Exposure Limits

	OEL TWA
	7 mg/m³

	OEL TWA
	1 ppm

	OEL STEL
	14 mg/m³

	OEL STEL
	200 ppm

	Greece - Occupational Exposure Limits

	OEL TWA
	7 mg/m³

	OEL TWA
	1 ppm

	OEL STEL
	14 mg/m³

	OEL STEL
	2 ppm

	Hungary - Occupational Exposure Limits

	AK (OEL TWA)
	7 mg/m³

	CK (OEL STEL)
	14 mg/m³

	Ireland - Occupational Exposure Limits

	OEL TWA
	7 mg/m³ (vapour)

	OEL TWA
	1 ppm (vapour)

	OEL STEL
	14 mg/m³ (vapour)

	OEL STEL
	2 ppm (vapour)

	Italy - Occupational Exposure Limits

	OEL TWA
	7 mg/m³

	OEL TWA
	1 ppm

	Latvia - Occupational Exposure Limits

	OEL TWA
	7 mg/m³

	OEL TWA
	1 ppm

	Lithuania - Occupational Exposure Limits

	IPRV (OEL TWA)
	7 mg/m³

	IPRV (OEL TWA)
	1 ppm

	TPRV (OEL STEL)
	14 mg/m³

	TPRV (OEL STEL)
	2 ppm

	Luxembourg - Occupational Exposure Limits

	OEL TWA
	7 mg/m³

	OEL TWA
	1 ppm

	OEL STEL
	14 mg/m³

	OEL STEL
	2 ppm

	Malta - Occupational Exposure Limits

	OEL TWA
	7 mg/m³

	OEL TWA
	1 ppm

	OEL STEL
	14 mg/m³

	OEL STEL
	2 ppm

	Netherlands - Occupational Exposure Limits

	TGG-8u (OEL TWA)
	7 mg/m³

	TGG-8u (OEL TWA)
	1 ppm

	TGG-15min (OEL STEL)
	14 mg/m³

	TGG-15min (OEL STEL)
	2 ppm

	Poland - Occupational Exposure Limits

	NDS (OEL TWA)
	7 mg/m³

	NDSCh (OEL STEL)
	14 mg/m³

	Portugal - Occupational Exposure Limits

	OEL TWA
	7 mg/m³

	OEL TWA
	1 ppm (vapor)

	OEL STEL
	14 mg/m³ (indicative limit value)

	OEL STEL
	2 ppm (indicative limit value-vapor)

	Romania - Occupational Exposure Limits

	OEL TWA
	7 mg/m³

	OEL TWA
	1 ppm

	OEL STEL
	14 mg/m³

	OEL STEL
	2 ppm

	Slovakia - Occupational Exposure Limits

	NPHV (OEL TWA)
	7 mg/m³

	NPHV (OEL TWA)
	1 ppm

	NPHV (OEL C)
	7.1 mg/m³

	Slovenia - Occupational Exposure Limits

	OEL TWA
	7 mg/m³

	OEL TWA
	1 ppm

	OEL STEL
	14 mg/m³

	OEL STEL
	2 ppm

	Spain - Occupational Exposure Limits

	VLA-ED (OEL TWA)
	7.1 mg/m³ (vapor)

	VLA-ED (OEL TWA)
	1 ppm (vapor)

	VLA-EC (OEL STEL)
	14.2 mg/m³ (vapor)

	VLA-EC (OEL STEL)
	2 ppm (vapor)

	Sweden - Occupational Exposure Limits

	NGV (OEL TWA)
	7 mg/m³

	NGV (OEL TWA)
	1 ppm

	KGV (OEL STEL)
	14 mg/m³

	KGV (OEL STEL)
	2 ppm

	United Kingdom - Occupational Exposure Limits

	WEL TWA (OEL TWA)
	7 mg/m³

	WEL TWA (OEL TWA)
	1 ppm

	WEL STEL (OEL STEL)
	14 mg/m³

	WEL STEL (OEL STEL)
	2 ppm

	Norway - Occupational Exposure Limits

	Grenseverdi (OEL TWA)
	7 mg/m³

	Grenseverdi (OEL TWA)
	1 ppm

	Korttidsverdi (OEL STEL)
	14 mg/m³ (value from the regulation)

	Korttidsverdi (OEL STEL)
	2 ppm (value from the regulation)

	Switzerland - Occupational Exposure Limits

	MAK (OEL TWA)
	7 mg/m³ (aerosol, vapour)

	MAK (OEL TWA)
	1 ppm (aerosol, vapour)

	KZGW (OEL STEL)
	14 mg/m³ (aerosol, vapour)

	KZGW (OEL STEL)
	2 ppm (aerosol, vapour)

	OEL chemical category
	Category 2 reproductive toxin

	USA - ACGIH - Occupational Exposure Limits

	ACGIH OEL TWA
	1 ppm (vapor)

	ACGIH OEL STEL
	2 ppm (vapor fraction)



	Alcohol C-10 (112-30-1)

	Bulgaria - Occupational Exposure Limits

	OEL TWA
	10 mg/m³

	Germany - Occupational Exposure Limits (TRGS 900)

	AGW (OEL TWA)
	66 mg/m³ (the risk of damage to the embryo or fetus can be excluded when AGW and BGW values are observed)

	AGW (OEL TWA)
	10 ppm (the risk of damage to the embryo or fetus can be excluded when AGW and BGW values are observed)

	Latvia - Occupational Exposure Limits

	OEL TWA
	10 mg/m³

	Lithuania - Occupational Exposure Limits

	IPRV (OEL TWA)
	10 mg/m³

	Romania - Occupational Exposure Limits

	OEL TWA
	100 mg/m³

	OEL TWA
	15 ppm

	OEL STEL
	200 mg/m³

	OEL STEL
	30 ppm

	Switzerland - Occupational Exposure Limits

	MAK (OEL TWA)
	66 mg/m³ (aerosol, vapour)

	MAK (OEL TWA)
	10 ppm (aerosol, vapour)

	KZGW (OEL STEL)
	66 mg/m³ (aerosol, vapour)

	KZGW (OEL STEL)
	10 ppm (aerosol, vapour)



	Benzyl acetate (140-11-4)

	Belgium - Occupational Exposure Limits

	OEL TWA
	62 mg/m³

	OEL TWA
	10 ppm

	Denmark - Occupational Exposure Limits

	OEL TWA
	61 mg/m³

	OEL TWA
	10 ppm

	OEL STEL
	122 mg/m³

	OEL STEL
	20 ppm

	Ireland - Occupational Exposure Limits

	OEL TWA
	10 ppm

	OEL STEL
	30 ppm (calculated)

	Latvia - Occupational Exposure Limits

	OEL TWA
	5 mg/m³

	Lithuania - Occupational Exposure Limits

	IPRV (OEL TWA)
	5 mg/m³

	Portugal - Occupational Exposure Limits

	OEL TWA
	10 ppm

	OEL chemical category
	A4 - Not Classifiable as a Human Carcinogen

	Romania - Occupational Exposure Limits

	OEL TWA
	50 mg/m³

	OEL TWA
	8 ppm

	OEL STEL
	80 mg/m³

	OEL STEL
	13 ppm

	Spain - Occupational Exposure Limits

	VLA-ED (OEL TWA)
	62 mg/m³

	VLA-ED (OEL TWA)
	10 ppm

	USA - ACGIH - Occupational Exposure Limits

	ACGIH OEL TWA
	10 ppm

	ACGIH chemical category
	Not Classifiable as a Human Carcinogen



	Caproic acid (142-62-1)

	Bulgaria - Occupational Exposure Limits

	OEL TWA
	5 mg/m³

	Latvia - Occupational Exposure Limits

	OEL TWA
	5 mg/m³

	Lithuania - Occupational Exposure Limits

	IPRV (OEL TWA)
	5 mg/m³



	ethanol, ethyl alcohol (64-17-5)

	Austria - Occupational Exposure Limits

	MAK (OEL TWA)
	1900 mg/m³

	MAK (OEL TWA)
	1000 ppm

	MAK (OEL STEL)
	3800 mg/m³

	MAK (OEL STEL)
	2000 ppm

	Belgium - Occupational Exposure Limits

	OEL TWA
	1907 mg/m³

	OEL TWA
	1000 ppm

	Bulgaria - Occupational Exposure Limits

	OEL TWA
	1000 mg/m³

	Croatia - Occupational Exposure Limits

	GVI (OEL TWA)
	1900 mg/m³

	GVI (OEL TWA)
	1000 ppm

	Czech Republic - Occupational Exposure Limits

	PEL (OEL TWA)
	1000 mg/m³

	Denmark - Occupational Exposure Limits

	OEL TWA
	1900 mg/m³

	OEL TWA
	1000 ppm

	OEL STEL
	3800 mg/m³

	OEL STEL
	2000 ppm

	Estonia - Occupational Exposure Limits

	OEL TWA
	1000 mg/m³

	OEL TWA
	500 ppm

	OEL STEL
	1900 mg/m³

	OEL STEL
	1000 ppm

	Finland - Occupational Exposure Limits

	HTP (OEL TWA)
	1900 mg/m³

	HTP (OEL TWA)
	1000 ppm

	HTP (OEL STEL)
	2500 mg/m³

	HTP (OEL STEL)
	1300 ppm

	France - Occupational Exposure Limits

	VME (OEL TWA)
	1900 mg/m³

	VME (OEL TWA)
	1000 ppm

	VLE (OEL C/STEL)
	9500 mg/m³

	VLE (OEL C/STEL)
	5000 ppm

	Germany - Occupational Exposure Limits (TRGS 900)

	AGW (OEL TWA)
	380 mg/m³ (the risk of damage to the embryo or fetus can be excluded when AGW and BGW values are observed)

	AGW (OEL TWA)
	200 ppm (the risk of damage to the embryo or fetus can be excluded when AGW and BGW values are observed)

	Greece - Occupational Exposure Limits

	OEL TWA
	1900 mg/m³

	OEL TWA
	1000 ppm

	Hungary - Occupational Exposure Limits

	AK (OEL TWA)
	1900 mg/m³

	CK (OEL STEL)
	3800 mg/m³

	Ireland - Occupational Exposure Limits

	OEL STEL
	1000 ppm

	Latvia - Occupational Exposure Limits

	OEL TWA
	1000 mg/m³

	Lithuania - Occupational Exposure Limits

	IPRV (OEL TWA)
	1000 mg/m³

	IPRV (OEL TWA)
	500 ppm

	TPRV (OEL STEL)
	1900 mg/m³

	TPRV (OEL STEL)
	1000 ppm

	Netherlands - Occupational Exposure Limits

	TGG-8u (OEL TWA)
	260 mg/m³

	TGG-8u (OEL TWA)
	137 ppm

	TGG-15min (OEL STEL)
	1900 mg/m³

	TGG-15min (OEL STEL)
	1000 ppm

	MAC chemical category
	skin notation

	Poland - Occupational Exposure Limits

	NDS (OEL TWA)
	1900 mg/m³

	Portugal - Occupational Exposure Limits

	OEL STEL
	1000 ppm

	OEL chemical category
	A3 - Confirmed Animal Carcinogen with Unknown Relevance to Humans

	Romania - Occupational Exposure Limits

	OEL TWA
	1900 mg/m³

	OEL TWA
	1000 ppm

	OEL STEL
	9500 mg/m³

	OEL STEL
	5000 ppm

	Slovakia - Occupational Exposure Limits

	NPHV (OEL TWA)
	960 mg/m³

	NPHV (OEL TWA)
	500 ppm

	NPHV (OEL C)
	1920 mg/m³

	Slovenia - Occupational Exposure Limits

	OEL TWA
	960 mg/m³

	OEL TWA
	500 ppm

	OEL STEL
	1920 mg/m³

	OEL STEL
	1000 ppm

	Spain - Occupational Exposure Limits

	VLA-EC (OEL STEL)
	1910 mg/m³

	VLA-EC (OEL STEL)
	1000 ppm

	Sweden - Occupational Exposure Limits

	NGV (OEL TWA)
	1000 mg/m³

	NGV (OEL TWA)
	500 ppm

	KGV (OEL STEL)
	1900 mg/m³

	KGV (OEL STEL)
	1000 ppm

	United Kingdom - Occupational Exposure Limits

	WEL TWA (OEL TWA)
	1920 mg/m³

	WEL TWA (OEL TWA)
	1000 ppm

	WEL STEL (OEL STEL)
	5760 mg/m³ (calculated)

	WEL STEL (OEL STEL)
	3000 ppm (calculated)

	Norway - Occupational Exposure Limits

	Grenseverdi (OEL TWA)
	950 mg/m³

	Grenseverdi (OEL TWA)
	500 ppm

	Korttidsverdi (OEL STEL)
	1187.5 mg/m³ (value calculated)

	Korttidsverdi (OEL STEL)
	625 ppm (value calculated)

	Switzerland - Occupational Exposure Limits

	MAK (OEL TWA)
	960 mg/m³

	MAK (OEL TWA)
	500 ppm

	KZGW (OEL STEL)
	1920 mg/m³

	KZGW (OEL STEL)
	1000 ppm

	USA - ACGIH - Occupational Exposure Limits

	ACGIH OEL STEL
	1000 ppm

	ACGIH chemical category
	Confirmed Animal Carcinogen with Unknown Relevance to Humans



	Aldehyde C-6 (66-25-1)

	Finland - Occupational Exposure Limits

	HTP (OEL STEL)
	42 mg/m³

	HTP (OEL STEL)
	10 ppm

	Poland - Occupational Exposure Limits

	NDS (OEL TWA)
	40 mg/m³

	NDSCh (OEL STEL)
	80 mg/m³



	Carbitol (111-90-0)

	Austria - Occupational Exposure Limits

	MAK (OEL TWA)
	35 mg/m³

	MAK (OEL TWA)
	6 ppm

	MAK (OEL STEL)
	140 mg/m³

	MAK (OEL STEL)
	24 ppm

	Estonia - Occupational Exposure Limits

	OEL TWA
	50.1 mg/m³

	OEL TWA
	10 ppm

	OEL chemical category
	skin notation

	Germany - Occupational Exposure Limits (TRGS 900)

	AGW (OEL TWA)
	35 mg/m³ (the risk of damage to the embryo or fetus can be excluded when AGW and BGW values are observed)

	AGW (OEL TWA)
	6 ppm (the risk of damage to the embryo or fetus can be excluded when AGW and BGW values are observed)

	Slovenia - Occupational Exposure Limits

	OEL TWA
	35 mg/m³

	OEL TWA
	6 ppm

	OEL STEL
	70 mg/m³

	OEL STEL
	12 ppm

	Sweden - Occupational Exposure Limits

	NGV (OEL TWA)
	80 mg/m³

	NGV (OEL TWA)
	15 ppm

	KGV (OEL STEL)
	170 mg/m³

	KGV (OEL STEL)
	30 ppm

	OEL chemical category
	skin notation

	Switzerland - Occupational Exposure Limits

	MAK (OEL TWA)
	50 mg/m³ (aerosol, inhalable dust, vapour)

	KZGW (OEL STEL)
	100 mg/m³ (aerosol, inhalable dust, vapour)


[bookmark: _Hlk54076527]8.1.2. Recommended monitoring procedures
No additional information available
[bookmark: _Hlk54076613]8.1.3. Air contaminants formed
No additional information available
[bookmark: _Hlk54076910]8.1.4. DNEL and PNEC
No additional information available
[bookmark: _Hlk54076968]8.1.5. Control banding
No additional information available
8.2. Exposure controls
8.2.1. Appropriate engineering controls
No additional information available

8.2.2. Personal protection equipment
	Personal protective equipment:

	Avoid all unnecessary exposure.

	Personal protective equipment symbol(s):

	[image: ]



8.2.2.1. Eye and face protection
	Eye protection:

	Chemical goggles or safety glasses



8.2.2.2. Skin protection
	Hand protection:

	Wear protective gloves.



8.2.2.3. Respiratory protection
	Respiratory protection:

	Wear appropriate mask



8.2.2.4. Thermal hazards
No additional information available

8.2.3. Environmental exposure controls
	Other information:

	Do not eat, drink or smoke during use.


SECTION 9: Physical and chemical properties
9.1. Information on basic physical and chemical properties
	Physical state
	:
	Liquid

	Color
	:
	Standard.

	Odor
	:
	characteristic.

	Odor threshold
	:
	Not available

	Melting point
	:
	Not available

	Freezing point
	:
	Not available

	Boiling point
	:
	Not available

	Flammability
	:
	Non flammable.

	Lower explosion limit
	:
	Not available

	Upper explosion limit
	:
	Not available

	Flash point
	:
	> 93 °C

	Auto-ignition temperature
	:
	Not available

	Decomposition temperature
	:
	Not available

	pH
	:
	Not available

	Viscosity, kinematic
	:
	Not available

	Solubility
	:
	Not available

	Partition coefficient n-octanol/water (Log Kow)
	:
	Not available

	Vapor pressure
	:
	Not available

	Vapor pressure at 50°C
	:
	Not available

	Density
	:
	Not available

	Relative density
	:
	Not available

	Relative vapor density at 20°C
	:
	Not available

	Particle characteristics
	:
	Not applicable


9.2. Other information
[bookmark: _Hlk54084650]9.2.1. Information with regard to physical hazard classes
No additional information available
9.2.2. Other safety characteristics
No additional information available
SECTION 10: Stability and reactivity
10.1. Reactivity
No additional information available
10.2. Chemical stability
Not established.
10.3. Possibility of hazardous reactions
Not established.
10.4. Conditions to avoid
Direct sunlight. Extremely high or low temperatures.
10.5. Incompatible materials
Strong acids. Strong bases.
10.6. Hazardous decomposition products
fume. Carbon monoxide. Carbon dioxide.
SECTION 11: Toxicological information
11.1. Information on hazard classes as defined in Regulation (EC) No 1272/2008
	Acute toxicity (oral)
	:
	Not classified

	Acute toxicity (dermal)
	:
	Not classified

	Acute toxicity (inhalation)
	:
	Not classified



	Diphenyl oxide (101-84-8)

	LD50 oral rat
	2450 mg/kg (Source: NLM_CIP)

	LD50 oral
	2830 mg/kg body weight

	LD50 dermal rabbit
	> 7940 mg/kg (Source: NLM_CIP)

	LC50 Inhalation - Rat (Dust/Mist)
	1.5 mg/l/4h



	Hexyl cinnamic aldehyde (101-86-0)

	LD50 oral rat
	3100 mg/kg (Source: NLM_CIP)

	LD50 oral
	3100 mg/kg body weight

	LD50 dermal rabbit
	> 3000 mg/kg (Source: EPA_HPV)

	LC50 Inhalation - Rat
	> 5 mg/l/4h



	Hydroxy (107-75-5)

	LD50 oral rat
	> 5 g/kg (Source: NLM_CIP)

	LD50 dermal rabbit
	> 2000 mg/kg (Source: ECHA_API)



	Alcohol C-10 (112-30-1)

	LD50 oral rat
	4720 mg/kg (Source: NZ_CCID)

	LD50 dermal rabbit
	3560 mg/kg (Source: NLM_CIP)



	Helional (1205-17-0)

	LD50 dermal rabbit
	> 2000 mg/kg (Source: ECHA_API)



	Amyl cinnamic aldehyde (122-40-7)

	LD50 oral rat
	3730 mg/kg (Source: CHEMVIEW)

	LD50 dermal rabbit
	> 2000 mg/kg (Source: CHEMVIEW)



	Benzyl acetate (140-11-4)

	LD50 oral rat
	2490 mg/kg (Source: JAPAN_GHS)

	LD50 oral
	2490 mg/kg body weight

	LD50 dermal rabbit
	> 5000 mg/kg (Source: JAPAN_GHS)



	Caproic acid (142-62-1)

	LD50 oral rat
	3 g/kg (Source: NLM_HSDB)

	LD50 oral
	4000 mg/kg body weight

	LD50 dermal rabbit
	630 mg/kg (Source: NLM_HSDB)



	ethanol, ethyl alcohol (64-17-5)

	LD50 oral rat
	7060 mg/kg (Source: NLM_CIP)

	LC50 Inhalation - Rat
	133.8 mg/l/4h



	Aldehyde C-6 (66-25-1)

	LD50 oral rat
	4890 mg/kg (Source: NLM_CIP)

	LD50 dermal rabbit
	> 8100 mg/kg (Source: ECHA_API)



	isoeugenol (97-54-1)

	LD50 oral rat
	1560 mg/kg (Source: NLM_CIP)

	LD50 oral
	1500 mg/kg body weight

	LD50 dermal
	1912 mg/kg body weight



	Citronellol Pure (106-22-9)

	LD50 oral rat
	3450 mg/kg (Source: NLM_CIP)

	LD50 oral
	3450 mg/kg body weight

	LD50 dermal rabbit
	2650 mg/kg (Source: EPA_HPV)

	LD50 dermal
	2650 mg/kg body weight



	Linalool (78-70-6)

	LD50 oral
	2790 mg/kg



	benzyl benzoate (120-51-4)

	LD50 oral rat
	500 mg/kg (Source: NLM_CIP)

	LD50 oral
	1160 mg/kg body weight

	LD50 dermal rabbit
	4000 mg/kg (Source: NLM_CIP)



	Carbitol (111-90-0)

	LD50 oral rat
	10502 mg/kg (Source: OECD_SIDS)

	LD50 dermal rabbit
	9143 mg/kg (Source: OECD_SIDS)

	LC50 Inhalation - Rat
	> 5240 mg/m³ (Exposure time: 4 h Source: NLM_CIP)



	Skin corrosion/irritation
	:
	Not classified

	Additional information
	:
	Based on available data, the classification criteria are not met



	Serious eye damage/irritation
	:
	Not classified

	Additional information
	:
	Based on available data, the classification criteria are not met



	Respiratory or skin sensitization
	:
	May cause an allergic skin reaction.

	Additional information
	:
	Based on available data, the classification criteria are not met



	Germ cell mutagenicity
	:
	Not classified

	Additional information
	:
	Based on available data, the classification criteria are not met



	Carcinogenicity
	:
	Not classified

	Additional information
	:
	Based on available data, the classification criteria are not met 



	Benzyl acetate (140-11-4)

	IARC group
	3 - Not classifiable



	isoeugenol (97-54-1)

	IARC group
	2B - Possibly carcinogenic to humans



	Reproductive toxicity
	:
	Not classified

	Additional information
	:
	Based on available data, the classification criteria are not met



	STOT-single exposure
	:
	Not classified

	Additional information
	:
	Based on available data, the classification criteria are not met



	isoeugenol (97-54-1)

	STOT-single exposure
	May cause respiratory irritation. 



	STOT-repeated exposure
	:
	Not classified

	Additional information
	:
	Based on available data, the classification criteria are not met



	Aspiration hazard
	:
	Not classified

	Additional information
	:
	Based on available data, the classification criteria are not met



	benzyl benzoate (120-51-4)

	Viscosity, kinematic
	7.456 mm²/s


[bookmark: _Hlk54089399]11.2. Information on other hazards
11.2.1. Endocrine disrupting properties
No additional information available
[bookmark: _Hlk54089489][bookmark: _Hlk54089553]11.2.2. Other information
	Potential Adverse human health effects and symptoms
	:
	Based on available data, the classification criteria are not met


SECTION 12: Ecological information
12.1. Toxicity
	Hazardous to the aquatic environment, short–term (acute)
	:
	Not classified

	Hazardous to the aquatic environment, long–term (chronic)
	:
	Not classified



	Alcohol C-10 (112-30-1)

	LC50 - Fish [1]
	2.2 – 2.5 mg/l (Exposure time: 96 h - Species: Pimephales promelas [flow-through] Source: EPA)

	LC50 - Fish [2]
	4.12 – 6.2 mg/l (Exposure time: 96 h - Species: Lepomis macrochirus [static] Source: EPA)

	EC50 - Crustacea [1]
	3 mg/l (Exposure time: 48 h - Species: Daphnia magna)



	Caproic acid (142-62-1)

	LC50 - Fish [1]
	306 – 334 mg/l (Exposure time: 96 h - Species: Pimephales promelas [flow-through] Source: EPA)

	LC50 - Fish [2]
	88 mg/l (Exposure time: 96 h - Species: Pimephales promelas [static] Source: EPA)



	ethanol, ethyl alcohol (64-17-5)

	LC50 - Fish [2]
	> 100 mg/l (Exposure time: 96 h - Species: Pimephales promelas [static] Source: EPA)

	EC50 - Crustacea [1]
	9268 – 14221 mg/l (Exposure time: 48 h - Species: Daphnia magna)

	EC50 - Crustacea [2]
	2 mg/l (Exposure time: 48 h - Species: Daphnia magna [Static])



	Aldehyde C-6 (66-25-1)

	LC50 - Fish [1]
	12 – 16.5 mg/l (Exposure time: 96 h - Species: Pimephales promelas [flow-through] Source: EPA)



	Linalool (78-70-6)

	EC50 96h - Algae [1]
	88.3 mg/l (Species: Desmodesmus subspicatus)



	benzyl benzoate (120-51-4)

	LC50 - Fish [1]
	2.32 mg/l (Exposure time: 96 h - Species: Danio rerio [semi-static] Source: ECHA)

	NOEC (chronic)
	0.168 mg/l



	Carbitol (111-90-0)

	LC50 - Fish [1]
	10000 mg/l (Exposure time: 96 h - Species: Lepomis macrochirus [static] Source: EPA)

	LC50 - Fish [2]
	19100 – 23900 mg/l (Exposure time: 96 h - Species: Lepomis macrochirus [flow-through] Source: EPA)

	EC50 - Crustacea [1]
	3940 – 4670 mg/l (Exposure time: 48 h - Species: Daphnia magna)


12.2. Persistence and degradability
	JAPANESE BAMBOO #EU47242F 5% in DPG 

	Persistence and degradability
	Not established.



	Diphenyl oxide (101-84-8)

	Persistence and degradability
	Rapidly degradable



	Hexyl cinnamic aldehyde (101-86-0)

	Persistence and degradability
	Rapidly degradable



	Hydroxy (107-75-5)

	Persistence and degradability
	Rapidly degradable



	Alcohol C-10 (112-30-1)

	Persistence and degradability
	Rapidly degradable



	Helional (1205-17-0)

	Persistence and degradability
	Rapidly degradable



	Amyl cinnamic aldehyde (122-40-7)

	Persistence and degradability
	Rapidly degradable



	Benzyl acetate (140-11-4)

	Persistence and degradability
	Rapidly degradable



	Caproic acid (142-62-1)

	Persistence and degradability
	Rapidly degradable



	ethanol, ethyl alcohol (64-17-5)

	Persistence and degradability
	Rapidly degradable



	Aldehyde C-6 (66-25-1)

	Persistence and degradability
	Rapidly degradable



	isoeugenol (97-54-1)

	Persistence and degradability
	Rapidly degradable



	Citronellol Pure (106-22-9)

	Persistence and degradability
	Rapidly degradable



	Bacdanol (28219-61-6)

	Persistence and degradability
	Rapidly degradable



	Undecavertol (81782-77-6)

	Persistence and degradability
	Rapidly degradable



	Linalool (78-70-6)

	Persistence and degradability
	Rapidly degradable



	benzyl benzoate (120-51-4)

	Persistence and degradability
	May cause long-term adverse effects in the environment.



	Carbitol (111-90-0)

	Persistence and degradability
	Rapidly degradable


12.3. Bioaccumulative potential
	JAPANESE BAMBOO #EU47242F 5% in DPG 

	Bioaccumulative potential
	Not established.



	Diphenyl oxide (101-84-8)

	BCF - Fish [1]
	(470 dimensionless)

	Partition coefficient n-octanol/water (Log Pow)
	4.21 (at 25 °C)



	Hydroxy (107-75-5)

	Partition coefficient n-octanol/water (Log Pow)
	1.68 (at 25 °C)



	Alcohol C-10 (112-30-1)

	Partition coefficient n-octanol/water (Log Pow)
	4.5 (at 25 °C (at pH 6)



	Helional (1205-17-0)

	Partition coefficient n-octanol/water (Log Pow)
	2.4 (at 25 °C)



	Amyl cinnamic aldehyde (122-40-7)

	Partition coefficient n-octanol/water (Log Pow)
	2.498 (at 25 °C (at pH 6.2)



	Benzyl acetate (140-11-4)

	Partition coefficient n-octanol/water (Log Pow)
	1.96 (at 25 °C (at pH 7)



	Caproic acid (142-62-1)

	Partition coefficient n-octanol/water (Log Pow)
	1.88



	ethanol, ethyl alcohol (64-17-5)

	Partition coefficient n-octanol/water (Log Pow)
	-0.35 (at 24 °C (at pH 7.4)



	Aldehyde C-6 (66-25-1)

	Partition coefficient n-octanol/water (Log Pow)
	2.3 (at 25 °C (at pH 5)



	Citronellol Pure (106-22-9)

	Partition coefficient n-octanol/water (Log Pow)
	3.41 (at 25 °C)



	Undecavertol (81782-77-6)

	Partition coefficient n-octanol/water (Log Pow)
	3.9 (at 30 °C (at pH 7)



	benzyl benzoate (120-51-4)

	Partition coefficient n-octanol/water (Log Pow)
	3.97 (at 25 °C)

	Bioaccumulative potential
	Not established.



	Carbitol (111-90-0)

	Partition coefficient n-octanol/water (Log Pow)
	-0.8


12.4. Mobility in soil
No additional information available
12.5. Results of PBT and vPvB assessment
No additional information available
12.6. Endocrine disrupting properties
[bookmark: _Hlk54090163]No additional information available
12.7. Other adverse effects
	Additional information
	:
	Avoid release to the environment.


SECTION 13: Disposal considerations
13.1. Waste treatment methods
	Product/Packaging disposal recommendations
	:
	Dispose in a safe manner in accordance with local/national regulations.

	Ecological information
	:
	Avoid release to the environment.


SECTION 14: Transport information
In accordance with ADR / IMDG / IATA / ADN / RID
	ADR
	IMDG
	IATA
	ADN
	RID

	14.1. UN number or ID number

	Not applicable
	Not applicable
	Not applicable
	Not applicable
	Not applicable

	14.2. UN proper shipping name

	Not applicable
	Not applicable
	Not applicable
	Not applicable
	Not applicable

	14.3. Transport hazard class(es)

	Not applicable
	Not applicable
	Not applicable
	Not applicable
	Not applicable

	14.4. Packing group

	Not applicable
	Not applicable
	Not applicable
	Not applicable
	Not applicable

	14.5. Environmental hazards

	Not applicable
	Not applicable
	Not applicable
	Not applicable
	Not applicable

	No supplementary information available


14.6. Special precautions for user
	Overland transport

	Not applicable



	Transport by sea

	Not applicable



	Air transport

	Not applicable



	Inland waterway transport

	Not applicable



	Rail transport

	Not applicable


14.7. Maritime transport in bulk according to IMO instruments
Not applicable
SECTION 15: Regulatory information
15.1. Safety, health and environmental regulations/legislation specific for the substance or mixture
15.1.1. EU-Regulations
REACH Annex XVII (Restriction List)
	EU restriction list (REACH Annex XVII)

	Reference code
	Applicable on
	Entry title or description

	3(a)
	ethanol, ethyl alcohol ; Aldehyde C-6
	Substances or mixtures fulfilling the criteria for any of the following hazard classes or categories set out in Annex I to Regulation (EC) No 1272/2008: Hazard classes 2.1 to 2.4, 2.6 and 2.7, 2.8 types A and B, 2.9, 2.10, 2.12, 2.13 categories 1 and 2, 2.14 categories 1 and 2, 2.15 types A to F

	3(b)
	JAPANESE BAMBOO #EU47242F 5% in DPG ; Hexyl cinnamic aldehyde ; Hydroxy ; Helional ; Amyl cinnamic aldehyde ; Caproic acid ; isoeugenol ; Citronellol Pure ; Bacdanol ; Linalool ; benzyl benzoate
	Substances or mixtures fulfilling the criteria for any of the following hazard classes or categories set out in Annex I to Regulation (EC) No 1272/2008: Hazard classes 3.1 to 3.6, 3.7 adverse effects on sexual function and fertility or on development, 3.8 effects other than narcotic effects, 3.9 and 3.10

	3(c)
	Hexyl cinnamic aldehyde ; Alcohol C-10 ; Helional ; Amyl cinnamic aldehyde ; Benzyl acetate ; Bacdanol ; Undecavertol ; benzyl benzoate
	Substances or mixtures fulfilling the criteria for any of the following hazard classes or categories set out in Annex I to Regulation (EC) No 1272/2008: Hazard class 4.1

	40.
	ethanol, ethyl alcohol ; Aldehyde C-6
	Substances classified as flammable gases category 1 or 2, flammable liquids categories 1, 2 or 3, flammable solids category 1 or 2, substances and mixtures which, in contact with water, emit flammable gases, category 1, 2 or 3, pyrophoric liquids category 1 or pyrophoric solids category 1, regardless of whether they appear in Part 3 of Annex VI to Regulation (EC) No 1272/2008 or not.


REACH Annex XIV (Authorisation List)
Contains no REACH Annex XIV substances.
REACH Candidate List (SVHC)
Contains no REACH candidate substance
PIC Regulation (Prior Informed Consent)
Contains no substance subject to Regulation (EU) No 649/2012 of the European Parliament and of the Council of 4 July 2012 concerning the export and import of hazardous chemicals.
POP Regulation (Persistent Organic Pollutants)
Contains no substance(s) subject to Regulation (EU) No 2019/1021 of the European Parliament and of the Council of 20 June 2019 on persistent organic pollutants
Ozone Regulation (1005/2009)
Contains no substance subject to REGULATION (EU) No 1005/2009 OF THE EUROPEAN PARLIAMENT AND OF THE COUNCIL of 16 September 2009 on substances that deplete the ozone layer.
Dual-Use Regulation (428/2009)
Contains no substance subject to the COUNCIL REGULATION (EC) No 428/2009 of 5 May 2009 setting up a Community regime for the control of exports, transfer, brokering and transit of dual-use items.
Explosives Precursors Regulation (2019/1148)
Contains no substance subject to Regulation (EU) 2019/1148 of the European Parliament and of the Council of 20 June 2019 on the marketing and use of explosives precursors.
Drug Precursors Regulation (273/2004)
Contains no substance subject to Regulation (EC) 273/2004 of the European Parliament and of the Council of 11 February 2004 on the manufacture and the placing on market of certain substances used in the illicit manufacture of narcotic drugs and psychotropic substances.
15.1.2. National regulations
	France

		Professional diseases

	Code
	Description

	RG 84
	Conditions caused by liquid organic solvents for professional use: saturated or unsaturated aliphatic or cyclic liquid hydrocarbons and mixtures thereof; liquid halogenated hydrocarbons; nitrated derivatives of aliphatic hydrocarbons; alcohols; glycols, glycol ethers; ketones; aldehydes; aliphatic and cyclic ethers, including tetrahydrofuran; esters; dimethylformamide and dimethylacetamine; acetonitrile and propionitrile; pyridine; dimethylsulfone and dimethylsulfoxide




	Germany

	Water hazard class (WGK)
	:
	WGK 1, slightly hazardous to water (Classification according to AwSV, Annex 1).

	Hazardous Incident Ordinance (12. BImSchV)
	:
	 Is not subject to the Hazardous Incident Ordinance (12. BImSchV)

	Netherlands

	ABM category
	:
	A(3) - hazardous for aquatic organisms, may have longterm hazardous effects in aquatic environment

	SZW-lijst van kankerverwekkende stoffen
	:
	Ethyl alcohol is listed

	SZW-lijst van mutagene stoffen
	:
	None of the components are listed

	SZW-lijst van reprotoxische stoffen – Borstvoeding
	:
	Ethyl alcohol is listed

	SZW-lijst van reprotoxische stoffen – Vruchtbaarheid
	:
	Ethyl alcohol is listed

	SZW-lijst van reprotoxische stoffen – Ontwikkeling
	:
	Ethyl alcohol is listed

	Denmark

	Classification remarks
	:
	Emergency management guidelines for the storage of flammable liquids must be followed

	Danish National Regulations
	:
	Young people below the age of 18 years are not allowed to use the product
Pregnant/breastfeeding women working with the product must not be in direct contact with the product


15.2. Chemical safety assessment
No chemical safety assessment has been carried out
SECTION 16: Other information
	Data sources
	:
	REGULATION (EC) No 1272/2008 OF THE EUROPEAN PARLIAMENT AND OF THE COUNCIL of 16 December 2008 on classification, labeling and packaging of substances and mixtures, amending and repealing Directives 67/548/EEC and 1999/45/EC, and amending Regulation (EC) No 1907/2006.

	Other information
	:
	None.



	Full text of H- and EUH-phrases:

	Acute Tox. 4 (Dermal)
	Acute toxicity (dermal), Category 4

	Acute Tox. 4 (Inhalation)
	Acute toxicity (inhalation) Category 4

	Acute Tox. 4 (Oral)
	Acute toxicity (oral) Category 4

	Aquatic Acute 1
	Hazardous to the aquatic environment – Acute Hazard Category 1

	Aquatic Chronic 1
	Hazardous to the aquatic environment – Chronic Hazard Category 1

	Aquatic Chronic 2
	Hazardous to the aquatic environment – Chronic Hazard Category 2

	Aquatic Chronic 3
	Hazardous to the aquatic environment – Chronic Hazard Category 3

	Carc. 2
	Carcinogenicity Category 2

	Eye Dam. 1
	Serious eye damage/eye irritation Category 1

	Eye Irrit. 2
	Serious eye damage/eye irritation, Category 2

	Flam. Liq. 2
	Flammable liquids Category 2

	Flam. Liq. 3
	Flammable liquids Category 3

	H225
	Highly flammable liquid and vapor.

	H226
	Flammable liquid and vapor.

	H302
	Harmful if swallowed.

	H312
	Harmful in contact with skin.

	H314
	Causes severe skin burns and eye damage.

	H315
	Causes skin irritation.

	H317
	May cause an allergic skin reaction.

	H318
	Causes serious eye damage.

	H319
	Causes serious eye irritation.

	H332
	Harmful if inhaled.

	H335
	May cause respiratory irritation.

	H351
	Suspected of causing cancer.

	H361
	Suspected of damaging fertility or the unborn child.

	H400
	Very toxic to aquatic life.

	H410
	Very toxic to aquatic life with long lasting effects.

	H411
	Toxic to aquatic life with long lasting effects.

	H412
	Harmful to aquatic life with long lasting effects.

	Repr. 2
	Reproductive toxicity Category 2

	Skin Corr. 1C
	Skin corrosion/irritation, Category 1, Sub-Category 1C

	Skin Irrit. 2
	Skin corrosion/irritation Category 2

	Skin Sens. 1
	Skin sensitization, Category 1

	Skin Sens. 1A
	Skin sensitization, Category 1A

	Skin Sens. 1B
	Skin sensitization, Category 1B

	STOT SE 3
	Specific target organ toxicity – Single exposure, Category 3, Respiratory tract irritation



	The classification complies with
	:
	ATP 12


Safety Data Sheet (SDS), EU
This information is based on our current knowledge and is intended to describe the product for the purposes of health, safety and environmental requirements only. It should not therefore be construed as guaranteeing any specific property of the product.
	
	
	

	6/25/2024 (Issue date)
	EN (English US)
	1/25



	
	
	

	6/25/2024 (Issue date)
	EN (English US)
	25/25



image1.png




image2.png
LGK 6.1D

LGK 6.1A

LGK 5.1A

LGK 5.1B

LGK 6.1B LGK 6.1C
LGK 8A LGK 8B
LGK 13 LGK 10-13





image3.png




