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SECTION 1: Identification of the substance/mixture and of the company/undertaking
1.1. Product identifier
	Product form
	:
	Mixture

	Product name
	:
	NEROLI SANTAL #EU55411F 10% in DPG

	Product code
	:
	EU55411F_10%

	Type of product
	:
	Perfumes, fragrances


1.2. Relevant identified uses of the substance or mixture and uses advised against
Relevant identified uses
	Industrial/Professional use spec
	:
	Industrial
For professional use only

	Use of the substance/mixture
	:
	Perfumes, fragrances

	Function or use category
	:
	Odour agents


1.3. Details of the supplier of the safety data sheet
No additional information available
1.4. Emergency telephone number
No additional information available
SECTION 2: Hazards identification
2.1. Classification of the substance or mixture
Classification according to Regulation (EC) No. 1272/2008 [CLP]
	Skin sensitisation, Category 1
	H317 
	

	Hazardous to the aquatic environment – Chronic Hazard, Category 3
	H412 
	


Full text of H- and EUH-statements: see section 16
Adverse physicochemical, human health and environmental effects
No additional information available
2.2. Label elements
Labelling according to Regulation (EC) No. 1272/2008 [CLP]
	Hazard pictograms (CLP)
	:
	[image: ]
	
	
	
	
	

	
	
	GHS07
	
	
	
	
	

	Signal word (CLP)
	:
	Warning

	Contains
	:
	1-(1,2,3,4,5,6,7,8-Octahydro-2,3,8,8-tetramethyl-2-naphthalenyl)ethanone; Carrot seed oil; Triplal (Vertocitral); Cinnamic aldehyde

	Hazard statements (CLP)
	:
	H317 - May cause an allergic skin reaction.
H412 - Harmful to aquatic life with long lasting effects.

	Precautionary statements (CLP)
	:
	P261 - Avoid breathing dust/fume/gas/mist/vapours/spray.
P272 - Contaminated work clothing should not be allowed out of the workplace.
P273 - Avoid release to the environment.
P280 - Wear protective gloves/protective clothing/eye protection/face protection/hearing protection.
P302+P352 - IF ON SKIN: Wash with plenty of water.
P321 - Specific treatment (see supplemental first aid instruction on this label).

	


2.3. Other hazards
	Contains no PBT and/or vPvB substances ≥ 0.1% assessed in accordance with REACH Annex XIII



	The mixture does not contain substance(s) included in the list established in accordance with Article 59(1) of REACH for having endocrine disrupting properties, or substance(s) are not identified as having endocrine disrupting properties in accordance with the criteria set out in Commission Delegated Regulation (EU) 2017/2100 or Commission Regulation (EU) 2018/605 at a concentration equal to or greater than 0,1 %



SECTION 3: Composition/information on ingredients
3.2. Mixtures
	Name
	Product identifier
	%
	Classification according to Regulation (EC) No. 1272/2008 [CLP]

	1-(1,2,3,4,5,6,7,8-Octahydro-2,3,8,8-tetramethyl-2-naphthalenyl)ethanone
	CAS-No.: 54464-57-2
EC-No.: 259-174-3
REACH-no: 01-2119489989-04
	0.98 – 1.96
	Skin Irrit. 2, H315
Skin Sens. 1, H317
Aquatic Chronic 1, H410

	Bis(2-ethylhexyl) adipate
substance with national workplace exposure limit(s) (PL)
	CAS-No.: 103-23-1
EC-No.: 203-090-1
REACH-no: 01-2119439699-19
	0.49 – 0.98
	Not classified

	Benzyl acetate
substance with national workplace exposure limit(s) (BE, DK, ES, IE, LT, LV, PT, RO)
	CAS-No.: 140-11-4
EC-No.: 205-399-7
REACH-no: 01-2119638272-42
	0.39 – 0.78
	Aquatic Chronic 3, H412

	Sandal Mysore Core
	CAS-No.: 28219-60-5
EC-No.: 248-907-2
	0.15 – 0.29
	Skin Irrit. 2, H315
Eye Irrit. 2, H319
Aquatic Acute 1, H400
Aquatic Chronic 1, H410

	Carrot seed oil
	CAS-No.: 8015-88-1
EC-No.: 616-965-1
	0.1 – 0.2
	Flam. Liq. 3, H226
Skin Irrit. 2, H315
Eye Irrit. 2, H319
Skin Sens. 1, H317
Asp. Tox. 1, H304
Aquatic Chronic 2, H411

	Triplal (Vertocitral)
	CAS-No.: 68039-49-6
EC-No.: 268-264-1
EC Index-No.: 605-043-00-4
	0.05 – 0.1
	Skin Irrit. 2, H315
Eye Irrit. 2, H319
Skin Sens. 1, H317
Aquatic Chronic 3, H412

	Cinnamic aldehyde
	CAS-No.: 104-55-2
EC-No.: 203-213-9
EC Index-No.: 606-155-00-6
REACH-no: 01-2119935242-45
	0.05 – 0.1
	Acute Tox. 4 (Dermal), H312
Skin Irrit. 2, H315
Eye Irrit. 2, H319
Skin Sens. 1A, H317
Aquatic Chronic 3, H412

	Diphenyl oxide
substance with national workplace exposure limit(s) (AT, BE, BG, CY, CZ, DE, DK, EE, ES, FI, FR, GB, GI, GR, HR, HU, IE, IT, LT, LU, LV, MT, NL, PL, PT, RO, SE, SI, SK, NO, CH, TR); substance with a Community workplace exposure limit
	CAS-No.: 101-84-8
EC-No.: 202-981-2
REACH-no: 01-2119472545-33
	0.01 – 0.02
	Eye Irrit. 2, H319
Aquatic Acute 1, H400
Aquatic Chronic 1, H410

	acetophenone
substance with national workplace exposure limit(s) (BE, BG, DK, ES, FI, HU, IE, LT, LV, PL, PT, RO)
	CAS-No.: 98-86-2
EC-No.: 202-708-7
EC Index-No.: 606-042-00-1
REACH-no: 01-2119533169-37
	0.01 – 0.02
	Acute Tox. 4 (Oral), H302
Eye Irrit. 2, H319

	1,2-Propanediol
substance with national workplace exposure limit(s) (GB, HR, IE, LT, LV, PL, NO)
	CAS-No.: 57-55-6
EC-No.: 200-338-0
REACH-no: 01-2119456809-23
	0.0048 – 0.0192
	Not classified

	Glycerine
substance with national workplace exposure limit(s) (BE, CZ, DE, EE, ES, FI, FR, GB, GR, HR, PL, PT, SI, SK, CH)
	CAS-No.: 56-81-5
EC-No.: 200-289-5
	0.00002 – 0.0001008
	Not classified

	2-phenoxyethanol
substance with national workplace exposure limit(s) (AT, DE, FI, PL, SI, CH)
	CAS-No.: 122-99-6
EC-No.: 204-589-7
EC Index-No.: 603-098-00-9
REACH-no: 01-2119488943-21
	≤ 0.0000001
	Acute Tox. 4 (Oral), H302
STOT SE 3, H335
Eye Dam. 1, H318



	Specific concentration limits:

	Name
	Product identifier
	Specific concentration limits (%)

	Cinnamic aldehyde
	CAS-No.: 104-55-2
EC-No.: 203-213-9
EC Index-No.: 606-155-00-6
REACH-no: 01-2119935242-45
	(0.001 < C < 0.01) EUH208
(0.01 ≤ C < 0.1) Skin Sens. 1; H317
(0.1 ≤ C < 100) Skin Sens. 1A; H317


Full text of H- and EUH-statements: see section 16

SECTION 4: First aid measures
4.1. Description of first aid measures
	First-aid measures general
	:
	Never give anything by mouth to an unconscious person. If you feel unwell, seek medical advice (show the label where possible).

	First-aid measures after inhalation
	:
	Allow affected person to breathe fresh air. Allow the victim to rest.

	First-aid measures after skin contact
	:
	Remove affected clothing and wash all exposed skin area with mild soap and water, followed by warm water rinse.

	First-aid measures after eye contact
	:
	Rinse immediately with plenty of water. Obtain medical attention if pain, blinking or redness persists.

	First-aid measures after ingestion
	:
	Rinse mouth. Do NOT induce vomiting. Obtain emergency medical attention.


4.2. Most important symptoms and effects, both acute and delayed
	Symptoms/effects
	:
	Not expected to present a significant hazard under anticipated conditions of normal use.


4.3. Indication of any immediate medical attention and special treatment needed
No additional information available
SECTION 5: Firefighting measures
5.1. Extinguishing media
	Suitable extinguishing media
	:
	Foam. Dry powder. Carbon dioxide. Water spray. Sand.

	Unsuitable extinguishing media
	:
	Do not use a heavy water stream.


5.2. Special hazards arising from the substance or mixture
No additional information available
5.3. Advice for firefighters
	Firefighting instructions
	:
	Use water spray or fog for cooling exposed containers. Exercise caution when fighting any chemical fire. Prevent fire fighting water from entering the environment.

	Protection during firefighting
	:
	Do not enter fire area without proper protective equipment, including respiratory protection.


SECTION 6: Accidental release measures
6.1. Personal precautions, protective equipment and emergency procedures
For non-emergency personnel
	Emergency procedures
	:
	Evacuate unnecessary personnel.


For emergency responders
	Protective equipment
	:
	Equip cleanup crew with proper protection.

	Emergency procedures
	:
	Ventilate area.


6.2. Environmental precautions
Prevent entry to sewers and public waters. Notify authorities if liquid enters sewers or public waters.
6.3. Methods and material for containment and cleaning up
	Methods for cleaning up
	:
	Soak up spills with inert solids, such as clay or diatomaceous earth as soon as possible. Collect spillage. Store away from other materials.


6.4. Reference to other sections
See Section 8. Exposure controls and personal protection.
SECTION 7: Handling and storage
7.1. Precautions for safe handling
	Precautions for safe handling
	:
	Wash hands and other exposed areas with mild soap and water before eating, drinking or smoking and when leaving work. Provide good ventilation in process area to prevent formation of vapour.


7.2. Conditions for safe storage, including any incompatibilities
	Storage conditions
	:
	Keep only in the original container in a cool, well ventilated place away from : Keep container closed when not in use.

	Incompatible products
	:
	Strong bases. Strong acids.

	Incompatible materials
	:
	Sources of ignition. Direct sunlight.

	Germany

	Storage class (LGK, TRGS 510)
	:
	LGK 12 - Non-combustible liquids

	Joint storage table
	:
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	Joint storage not permitted for
	:
	LGK 1, LGK 6.2, LGK 7

	Joint storage with restrictions permitted for
	:
	LGK 4.1A, LGK 4.3, LGK 5.1C

	Joint storage permitted for
	:
	LGK 2A, LGK 2B, LGK 3, LGK 4.1B, LGK 4.2, LGK 5.1A, LGK 5.1B, LGK 5.2, LGK 6.1A, LGK 6.1B, LGK 6.1C, LGK 6.1D, LGK 8A, LGK 8B, LGK 10, LGK 11, LGK 12, LGK 13, LGK 10-13

	Switzerland

	Storage class (LK)
	:
	LK 10/12 - Liquids


7.3. Specific end use(s)
No additional information available
SECTION 8: Exposure controls/personal protection
8.1. Control parameters
National occupational exposure and biological limit values

	Bis(2-ethylhexyl) adipate (103-23-1)

	Poland - Occupational Exposure Limits

	NDS (OEL TWA)
	400 mg/m³



	Benzyl acetate (140-11-4)

	Belgium - Occupational Exposure Limits

	OEL TWA
	62 mg/m³

	OEL TWA
	10 ppm

	Denmark - Occupational Exposure Limits

	OEL TWA
	61 mg/m³

	OEL TWA
	10 ppm

	OEL STEL
	122 mg/m³

	OEL STEL
	20 ppm

	Ireland - Occupational Exposure Limits

	OEL TWA
	10 ppm

	OEL STEL
	30 ppm (calculated)

	Latvia - Occupational Exposure Limits

	OEL TWA
	5 mg/m³

	Lithuania - Occupational Exposure Limits

	IPRV (OEL TWA)
	5 mg/m³

	Portugal - Occupational Exposure Limits

	OEL TWA
	10 ppm

	OEL chemical category
	A4 - Not Classifiable as a Human Carcinogen

	Romania - Occupational Exposure Limits

	OEL TWA
	50 mg/m³

	OEL TWA
	8 ppm

	OEL STEL
	80 mg/m³

	OEL STEL
	13 ppm

	Spain - Occupational Exposure Limits

	VLA-ED (OEL TWA)
	62 mg/m³

	VLA-ED (OEL TWA)
	10 ppm

	USA - ACGIH - Occupational Exposure Limits

	ACGIH® TLV® TWA
	10 ppm

	ACGIH® chemical category
	Not Classifiable as a Human Carcinogen



	Diphenyl oxide (101-84-8)

	EU - Indicative Occupational Exposure Limit (IOEL)

	IOEL TWA
	7 mg/m³

	IOEL TWA
	1 ppm

	IOEL STEL
	14 mg/m³

	IOEL STEL
	2 ppm

	Austria - Occupational Exposure Limits

	MAK (OEL TWA)
	7 mg/m³

	MAK (OEL TWA)
	1 ppm

	MAK (OEL STEL)
	14 mg/m³

	MAK (OEL STEL)
	2 ppm

	Belgium - Occupational Exposure Limits

	OEL TWA
	7 mg/m³ (vapor)

	OEL TWA
	1 ppm (vapor)

	OEL STEL
	14 mg/m³ (vapor)

	OEL STEL
	2 ppm (vapor)

	Bulgaria - Occupational Exposure Limits

	OEL TWA
	7 mg/m³

	OEL TWA
	1 ppm

	OEL STEL
	14 mg/m³

	OEL STEL
	2 ppm

	Croatia - Occupational Exposure Limits

	GVI (OEL TWA)
	7 mg/m³

	GVI (OEL TWA)
	1 ppm

	KGVI (OEL STEL)
	14 mg/m³

	KGVI (OEL STEL)
	2 ppm

	Cyprus - Occupational Exposure Limits

	OEL TWA
	7 mg/m³

	OEL TWA
	1 ppm

	OEL STEL
	14 mg/m³

	OEL STEL
	2 ppm

	Czech Republic - Occupational Exposure Limits

	PEL (OEL TWA)
	5 mg/m³

	Denmark - Occupational Exposure Limits

	OEL TWA
	7 mg/m³

	OEL TWA
	1 ppm

	OEL STEL
	14 mg/m³

	OEL STEL
	2 ppm

	Estonia - Occupational Exposure Limits

	OEL TWA
	7 mg/m³

	OEL TWA
	1 ppm

	OEL STEL
	14 mg/m³

	OEL STEL
	2 ppm

	Finland - Occupational Exposure Limits

	HTP (OEL TWA)
	7 mg/m³

	HTP (OEL TWA)
	1 ppm

	HTP (OEL STEL)
	14 mg/m³

	HTP (OEL STEL)
	2 ppm

	France - Occupational Exposure Limits

	VME (OEL TWA)
	7 mg/m³ (indicative limit)

	VME (OEL TWA)
	1 ppm (indicative limit)

	VLE (OEL C/STEL)
	14 mg/m³ (indicative limit)

	VLE (OEL C/STEL)
	2 ppm (indicative limit)

	Germany - Occupational Exposure Limits (TRGS 900)

	AGW (OEL TWA)
	7.1 mg/m³ (the risk of damage to the embryo or fetus can be excluded when AGW and BGW values are observed-vapor)

	AGW (OEL TWA)
	1 ppm (the risk of damage to the embryo or fetus can be excluded when AGW and BGW values are observed-vapor)

	Gibraltar - Occupational Exposure Limits

	OEL TWA
	7 mg/m³

	OEL TWA
	1 ppm

	OEL STEL
	14 mg/m³

	OEL STEL
	200 ppm

	Greece - Occupational Exposure Limits

	OEL TWA
	7 mg/m³

	OEL TWA
	1 ppm

	OEL STEL
	14 mg/m³

	OEL STEL
	2 ppm

	Hungary - Occupational Exposure Limits

	AK (OEL TWA)
	7 mg/m³

	CK (OEL STEL)
	14 mg/m³

	Ireland - Occupational Exposure Limits

	OEL TWA
	7 mg/m³ (vapour)

	OEL TWA
	1 ppm (vapour)

	OEL STEL
	14 mg/m³ (vapor)

	OEL STEL
	2 ppm (vapor)

	Italy - Occupational Exposure Limits

	OEL TWA
	7 mg/m³

	OEL TWA
	1 ppm

	Latvia - Occupational Exposure Limits

	OEL TWA
	7 mg/m³

	OEL TWA
	1 ppm

	Lithuania - Occupational Exposure Limits

	IPRV (OEL TWA)
	7 mg/m³

	IPRV (OEL TWA)
	1 ppm

	TPRV (OEL STEL)
	14 mg/m³

	TPRV (OEL STEL)
	2 ppm

	Luxembourg - Occupational Exposure Limits

	OEL TWA
	7 mg/m³

	OEL TWA
	1 ppm

	OEL STEL
	14 mg/m³

	OEL STEL
	2 ppm

	Malta - Occupational Exposure Limits

	OEL TWA
	7 mg/m³

	OEL TWA
	1 ppm

	OEL STEL
	14 mg/m³

	OEL STEL
	2 ppm

	Netherlands - Occupational Exposure Limits

	TGG-8u (OEL TWA)
	7 mg/m³

	TGG-8u (OEL TWA)
	1 ppm

	TGG-15min (OEL STEL)
	14 mg/m³

	TGG-15min (OEL STEL)
	2 ppm

	Poland - Occupational Exposure Limits

	NDS (OEL TWA)
	7 mg/m³

	NDSCh (OEL STEL)
	14 mg/m³

	Portugal - Occupational Exposure Limits

	OEL TWA
	7 mg/m³ (indicative limit value)

	OEL TWA
	1 ppm (indicative limit value-vapor)

	OEL STEL
	14 mg/m³ (indicative limit value)

	OEL STEL
	2 ppm (indicative limit value-vapor)

	Romania - Occupational Exposure Limits

	OEL TWA
	7 mg/m³

	OEL TWA
	1 ppm

	OEL STEL
	14 mg/m³

	OEL STEL
	2 ppm

	Slovakia - Occupational Exposure Limits

	NPHV (OEL TWA)
	7 mg/m³

	NPHV (OEL TWA)
	1 ppm

	NPHV (OEL C)
	14 mg/m³

	Slovenia - Occupational Exposure Limits

	OEL TWA
	7 mg/m³

	OEL TWA
	1 ppm

	OEL STEL
	14 mg/m³

	OEL STEL
	2 ppm

	Spain - Occupational Exposure Limits

	VLA-ED (OEL TWA)
	7.1 mg/m³ (vapor)

	VLA-ED (OEL TWA)
	1 ppm (vapor)

	VLA-EC (OEL STEL)
	14.2 mg/m³ (vapor)

	VLA-EC (OEL STEL)
	2 ppm (vapor)

	Sweden - Occupational Exposure Limits

	NGV (OEL TWA)
	7 mg/m³

	NGV (OEL TWA)
	1 ppm

	KGV (OEL STEL)
	14 mg/m³

	KGV (OEL STEL)
	2 ppm

	United Kingdom - Occupational Exposure Limits

	WEL TWA (OEL TWA)
	7 mg/m³

	WEL TWA (OEL TWA)
	1 ppm

	WEL STEL (OEL STEL)
	14 mg/m³

	WEL STEL (OEL STEL)
	2 ppm

	Norway - Occupational Exposure Limits

	Grenseverdi (OEL TWA)
	7 mg/m³

	Grenseverdi (OEL TWA)
	1 ppm

	Korttidsverdi (OEL STEL)
	14 mg/m³ (value from the regulation)

	Korttidsverdi (OEL STEL)
	2 ppm (value from the regulation)

	Switzerland - Occupational Exposure Limits

	MAK (OEL TWA)
	7 mg/m³ (aerosol, vapour)

	MAK (OEL TWA)
	1 ppm (aerosol, vapour)

	KZGW (OEL STEL)
	14 mg/m³ (aerosol, vapour)

	KZGW (OEL STEL)
	2 ppm (aerosol, vapour)

	OEL chemical category
	Category 2 reproductive toxin

	USA - ACGIH - Occupational Exposure Limits

	ACGIH® TLV® TWA
	1 ppm (vapor)

	ACGIH® TLV® STEL
	2 ppm (vapor fraction)



	1,2-Propanediol (57-55-6)

	Croatia - Occupational Exposure Limits

	GVI (OEL TWA)
	474 mg/m³ (total vapor and particles)
10 mg/m³ (particles)

	GVI (OEL TWA)
	150 ppm

	Ireland - Occupational Exposure Limits

	OEL TWA
	10 mg/m³ (particulate)
470 mg/m³ (total vapour and particulates)

	OEL TWA
	150 ppm (total vapour and particulates)

	OEL STEL
	1410 mg/m³ (calculated-particulates)
30 mg/m³ (calculated)

	OEL STEL
	450 ppm (calculated-total vapor and particulates)

	Latvia - Occupational Exposure Limits

	OEL TWA
	7 mg/m³

	Lithuania - Occupational Exposure Limits

	IPRV (OEL TWA)
	7 mg/m³

	Poland - Occupational Exposure Limits

	NDS (OEL TWA)
	100 mg/m³ (vapor and inhalable fraction)

	United Kingdom - Occupational Exposure Limits

	WEL TWA (OEL TWA)
	474 mg/m³ (total vapour and particulate)
10 mg/m³ (particulate)

	WEL TWA (OEL TWA)
	150 ppm (total vapour and particulate)

	WEL STEL (OEL STEL)
	1422 mg/m³ (calculated-total vapour and particulate)
30 mg/m³ (calculated-particulate)

	WEL STEL (OEL STEL)
	450 ppm (calculated-total vapour and particulate)

	Norway - Occupational Exposure Limits

	Grenseverdi (OEL TWA)
	79 mg/m³

	Grenseverdi (OEL TWA)
	25 ppm

	Korttidsverdi (OEL STEL)
	118.5 mg/m³ (value calculated)

	Korttidsverdi (OEL STEL)
	37.5 ppm (value calculated)



	Glycerine (56-81-5)

	Belgium - Occupational Exposure Limits

	OEL TWA
	10 mg/m³ (mist)

	Croatia - Occupational Exposure Limits

	GVI (OEL TWA)
	10 mg/m³

	Czech Republic - Occupational Exposure Limits

	PEL (OEL TWA)
	10 mg/m³

	Estonia - Occupational Exposure Limits

	OEL TWA
	10 mg/m³

	Finland - Occupational Exposure Limits

	HTP (OEL TWA)
	20 mg/m³

	France - Occupational Exposure Limits

	VME (OEL TWA)
	10 mg/m³ (aerosol)

	Germany - Occupational Exposure Limits (TRGS 900)

	AGW (OEL TWA)
	200 mg/m³ (the risk of damage to the embryo or fetus can be excluded when AGW and BGW values are observed-inhalable fraction)

	Greece - Occupational Exposure Limits

	OEL TWA
	10 mg/m³

	Poland - Occupational Exposure Limits

	NDS (OEL TWA)
	10 mg/m³ (inhalable fraction)

	Portugal - Occupational Exposure Limits

	OEL TWA
	10 mg/m³ (mist)

	Slovakia - Occupational Exposure Limits

	NPHV (OEL TWA)
	10 mg/m³

	Slovenia - Occupational Exposure Limits

	OEL TWA
	200 mg/m³ (inhalable fraction)

	OEL STEL
	400 mg/m³ (inhalable fraction)

	Spain - Occupational Exposure Limits

	VLA-ED (OEL TWA)
	10 mg/m³ (mist)

	United Kingdom - Occupational Exposure Limits

	WEL TWA (OEL TWA)
	10 mg/m³ (mist)

	WEL STEL (OEL STEL)
	30 mg/m³ (calculated-mist)

	Switzerland - Occupational Exposure Limits

	MAK (OEL TWA)
	50 mg/m³ (inhalable dust)

	KZGW (OEL STEL)
	100 mg/m³ (inhalable dust)



	2-phenoxyethanol (122-99-6)

	Austria - Occupational Exposure Limits

	MAK (OEL TWA)
	110 mg/m³

	MAK (OEL TWA)
	20 ppm

	MAK (OEL STEL)
	110 mg/m³

	MAK (OEL STEL)
	20 ppm

	OEL C
	110 mg/m³

	OEL C
	20 ppm

	Finland - Occupational Exposure Limits

	HTP (OEL TWA)
	110 mg/m³

	HTP (OEL TWA)
	20 ppm

	HTP (OEL STEL)
	290 mg/m³

	HTP (OEL STEL)
	50 ppm

	OEL chemical category
	Potential for cutaneous absorption

	Germany - Occupational Exposure Limits (TRGS 900)

	AGW (OEL TWA)
	5.7 mg/m³ (the risk of damage to the embryo or fetus can be excluded when AGW and BGW values are observed)

	AGW (OEL TWA)
	1 ppm (the risk of damage to the embryo or fetus can be excluded when AGW and BGW values are observed)

	Poland - Occupational Exposure Limits

	NDS (OEL TWA)
	230 mg/m³

	Slovenia - Occupational Exposure Limits

	OEL TWA
	5.7 mg/m³

	OEL TWA
	1 ppm

	OEL STEL
	5.7 mg/m³

	OEL STEL
	1 ppm

	Switzerland - Occupational Exposure Limits

	MAK (OEL TWA)
	110 mg/m³ (aerosol, vapour)

	MAK (OEL TWA)
	20 ppm (aerosol, vapour)

	KZGW (OEL STEL)
	110 mg/m³ (aerosol, vapour)

	KZGW (OEL STEL)
	20 ppm (aerosol, vapour)



	acetophenone (98-86-2)

	Belgium - Occupational Exposure Limits

	OEL TWA
	50 mg/m³

	OEL TWA
	10 ppm

	Bulgaria - Occupational Exposure Limits

	OEL TWA
	5 mg/m³

	Denmark - Occupational Exposure Limits

	OEL TWA
	49 mg/m³

	OEL TWA
	10 ppm

	OEL STEL
	98 mg/m³

	OEL STEL
	20 ppm

	Finland - Occupational Exposure Limits

	HTP (OEL TWA)
	25 mg/m³

	HTP (OEL TWA)
	5 ppm

	Hungary - Occupational Exposure Limits

	AK (OEL TWA)
	50 mg/m³

	Ireland - Occupational Exposure Limits

	OEL TWA
	49 mg/m³

	OEL TWA
	10 ppm

	OEL STEL
	147 mg/m³ (calculated)

	OEL STEL
	30 ppm (calculated)

	Latvia - Occupational Exposure Limits

	OEL TWA
	5 mg/m³

	Lithuania - Occupational Exposure Limits

	IPRV (OEL TWA)
	5 mg/m³

	OEL chemical category
	Skin notation

	Poland - Occupational Exposure Limits

	NDS (OEL TWA)
	50 mg/m³

	NDSCh (OEL STEL)
	100 mg/m³

	Portugal - Occupational Exposure Limits

	OEL TWA
	10 ppm

	Romania - Occupational Exposure Limits

	OEL TWA
	100 mg/m³

	OEL TWA
	20 ppm

	OEL STEL
	200 mg/m³

	OEL STEL
	41 ppm

	Spain - Occupational Exposure Limits

	VLA-ED (OEL TWA)
	50 mg/m³

	VLA-ED (OEL TWA)
	10 ppm

	USA - ACGIH - Occupational Exposure Limits

	ACGIH® TLV® TWA
	10 ppm


8.2. Exposure controls
Personal protection equipment
	Personal protective equipment:

	Avoid all unnecessary exposure.

	Personal protective equipment symbol(s):
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Eye and face protection
	Eye protection:

	Chemical goggles or safety glasses


Skin protection
	Hand protection:

	Wear protective gloves.


Respiratory protection
	Respiratory protection:

	Wear appropriate mask


Environmental exposure controls
	Other information:

	Do not eat, drink or smoke during use.


SECTION 9: Physical and chemical properties
9.1. Information on basic physical and chemical properties
	Physical state
	:
	Liquid

	Colour
	:
	Conforms to standard.

	Odour
	:
	characteristic.

	Odour threshold
	:
	Not available

	Melting point
	:
	Not available

	Freezing point
	:
	Not available

	Boiling point
	:
	Not available

	Flammability
	:
	Non flammable.

	Lower explosion limit
	:
	Not available

	Upper explosion limit
	:
	Not available

	Flash point
	:
	> 93 °C

	Auto-ignition temperature
	:
	Not available

	Decomposition temperature
	:
	Not available

	pH
	:
	Not available

	Viscosity, kinematic
	:
	Not available

	Solubility
	:
	Not available

	Partition coefficient n-octanol/water (Log Kow)
	:
	Not available

	Vapour pressure
	:
	Not available

	Vapour pressure at 50°C
	:
	Not available

	Density
	:
	Not available

	Relative density
	:
	Not available

	Relative vapour density at 20°C
	:
	Not available

	Particle characteristics
	:
	Not applicable


9.2. Other information
No additional information available
SECTION 10: Stability and reactivity
10.1. Reactivity
No additional information available
10.2. Chemical stability
Not established.
10.3. Possibility of hazardous reactions
Not established.
10.4. Conditions to avoid
Direct sunlight. Extremely high or low temperatures.
10.5. Incompatible materials
Strong acids. Strong bases.
10.6. Hazardous decomposition products
fume. Carbon monoxide. Carbon dioxide.
SECTION 11: Toxicological information
11.1. Information on hazard classes as defined in Regulation (EC) No 1272/2008
	Acute toxicity (oral)
	:
	Not classified

	Acute toxicity (dermal)
	:
	Not classified

	Acute toxicity (inhalation)
	:
	Not classified



	Bis(2-ethylhexyl) adipate (103-23-1)

	LD50 oral rat
	5600 mg/kg (Source: NLM_CIP)

	LD50 dermal rabbit
	8410 mg/kg (Source: NLM_CIP)

	LC50 Inhalation - Rat
	> 5.7 mg/l/4h



	Benzyl acetate (140-11-4)

	LD50 oral rat
	2490 mg/kg (Source: JAPAN_GHS)

	LD50 oral
	2490 mg/kg

	LD50 dermal rabbit
	> 5000 mg/kg (Source: JAPAN_GHS)



	Triplal (Vertocitral) (68039-49-6)

	LD50 oral
	2330 mg/kg



	Cinnamic aldehyde (104-55-2)

	LD50 oral rat
	2220 mg/kg (Source: NLM_CIP)

	LD50 oral
	2220 mg/kg

	LD50 dermal rabbit
	1260 mg/kg (Source: EPA_HPV)

	LD50 dermal
	1260 mg/kg



	Diphenyl oxide (101-84-8)

	LD50 oral rat
	2450 mg/kg (Source: NLM_CIP)

	LD50 oral
	2830 mg/kg

	LD50 dermal rabbit
	> 7940 mg/kg (Source: NLM_CIP)



	1,2-Propanediol (57-55-6)

	LD50 oral rat
	20 g/kg (Source: NLM_CIP)

	LD50 dermal rabbit
	20800 mg/kg (Source: NLM_CIP)



	Glycerine (56-81-5)

	LD50 oral rat
	27200 mg/kg (Source: ECHA_API)

	LD50 dermal rabbit
	> 10 g/kg (Source: NLM_CIP)

	LC50 Inhalation - Rat
	> 5.85 mg/l/4h



	2-phenoxyethanol (122-99-6)

	LD50 oral rat
	1850 mg/kg (Source: EU_CLH)

	LD50 oral
	1394 mg/kg

	LD50 dermal rabbit
	5 ml/kg (Source: NLM_CIP)

	LC50 Inhalation - Rat
	> 0.057 mg/l (Exposure time: 8 h Source: EU_CLH)



	acetophenone (98-86-2)

	LD50 oral rat
	2081 mg/kg (Source: ECHA_API)

	LD50 dermal rat
	3300 mg/kg (Source: ECHA_API)

	LC50 Inhalation - Rat
	> 2.13 mg/l (Exposure time: 8 h Source: CHEMVIEW)



	Skin corrosion/irritation
	:
	Not classified

	Additional information
	:
	Based on available data, the classification criteria are not met



	Serious eye damage/irritation
	:
	Not classified

	Additional information
	:
	Based on available data, the classification criteria are not met



	Respiratory or skin sensitisation
	:
	May cause an allergic skin reaction.

	Additional information
	:
	Based on available data, the classification criteria are not met



	Germ cell mutagenicity
	:
	Not classified

	Additional information
	:
	Based on available data, the classification criteria are not met



	Carcinogenicity
	:
	Not classified

	Additional information
	:
	Based on available data, the classification criteria are not met 



	Bis(2-ethylhexyl) adipate (103-23-1)

	IARC group
	3 - Not classifiable



	Benzyl acetate (140-11-4)

	IARC group
	3 - Not classifiable



	Reproductive toxicity
	:
	Not classified

	Additional information
	:
	Based on available data, the classification criteria are not met



	STOT-single exposure
	:
	Not classified

	Additional information
	:
	Based on available data, the classification criteria are not met



	2-phenoxyethanol (122-99-6)

	STOT-single exposure
	May cause respiratory irritation. 



	STOT-repeated exposure
	:
	Not classified

	Additional information
	:
	Based on available data, the classification criteria are not met



	Aspiration hazard
	:
	Not classified

	Additional information
	:
	Based on available data, the classification criteria are not met


[bookmark: _Hlk54089399]11.2. Information on other hazards
Other information
	Potential adverse human health effects and symptoms
	:
	Based on available data, the classification criteria are not met


SECTION 12: Ecological information
12.1. Toxicity
	Hazardous to the aquatic environment, short–term (acute)
	:
	Not classified

	Hazardous to the aquatic environment, long–term (chronic)
	:
	Harmful to aquatic life with long lasting effects.



	Bis(2-ethylhexyl) adipate (103-23-1)

	LC50 - Fish [1]
	0.48 – 0.85 mg/l (Exposure time: 96 h - Species: Lepomis macrochirus [static] Source: EPA)

	LC50 - Fish [2]
	0.48 – 0.85 mg/l (Exposure time: 96 h - Species: Oncorhynchus mykiss [static] Source: EPA)

	EC50 - Crustacea [1]
	> 1.6 mg/l (Exposure time: 48 h - Species: Daphnia magna)

	EC50 72h - Algae [1]
	> 500 mg/l (Species: Desmodesmus subspicatus)



	1,2-Propanediol (57-55-6)

	LC50 - Fish [1]
	51600 mg/l (Exposure time: 96 h - Species: Oncorhynchus mykiss [static] Source: IUCLID)

	LC50 - Fish [2]
	41 – 47 ml/l (Exposure time: 96 h - Species: Oncorhynchus mykiss [static] Source: EPA)

	EC50 - Crustacea [1]
	> 1000 mg/l (Exposure time: 48 h - Species: Daphnia magna [Static])

	EC50 96h - Algae [1]
	19000 mg/l (Species: Pseudokirchneriella subcapitata)



	Glycerine (56-81-5)

	LC50 - Fish [1]
	54 g/l (Exposure time: 96 h -ECHA db)



	2-phenoxyethanol (122-99-6)

	LC50 - Fish [1]
	337 – 352 mg/l (Exposure time: 96 h - Species: Pimephales promelas [flow-through] Source: EPA)

	LC50 - Fish [2]
	366 mg/l (Exposure time: 96 h - Species: Pimephales promelas [static] Source: IUCLID)

	EC50 - Crustacea [1]
	> 500 mg/l (Exposure time: 48 h - Species: Daphnia magna)

	EC50 72h - Algae [1]
	> 500 mg/l (Species: Desmodesmus subspicatus)



	acetophenone (98-86-2)

	LC50 - Fish [1]
	162 mg/l (Exposure time: 96 h - Species: Pimephales promelas [flow-through] Source: EPA)

	LC50 - Fish [2]
	155 mg/l (Exposure time: 96 h - Species: Pimephales promelas [static] Source: EPA)


12.2. Persistence and degradability
	NEROLI SANTAL #EU55411F 10% in DPG 

	Persistence and degradability
	Not established.



	1-(1,2,3,4,5,6,7,8-Octahydro-2,3,8,8-tetramethyl-2-naphthalenyl)ethanone (54464-57-2)

	Persistence and degradability
	Rapidly degradable



	Bis(2-ethylhexyl) adipate (103-23-1)

	Persistence and degradability
	Rapidly degradable



	Benzyl acetate (140-11-4)

	Persistence and degradability
	Rapidly degradable



	Sandal Mysore Core (28219-60-5)

	Persistence and degradability
	Rapidly degradable



	Carrot seed oil (8015-88-1)

	Persistence and degradability
	Rapidly degradable



	Triplal (Vertocitral) (68039-49-6)

	Persistence and degradability
	Rapidly degradable



	Cinnamic aldehyde (104-55-2)

	Persistence and degradability
	Rapidly degradable



	Diphenyl oxide (101-84-8)

	Persistence and degradability
	Rapidly degradable



	1,2-Propanediol (57-55-6)

	Persistence and degradability
	Rapidly degradable



	Glycerine (56-81-5)

	Persistence and degradability
	Rapidly degradable



	2-phenoxyethanol (122-99-6)

	Persistence and degradability
	Rapidly degradable



	acetophenone (98-86-2)

	Persistence and degradability
	Rapidly degradable


12.3. Bioaccumulative potential
	NEROLI SANTAL #EU55411F 10% in DPG 

	Bioaccumulative potential
	Not established.



	1-(1,2,3,4,5,6,7,8-Octahydro-2,3,8,8-tetramethyl-2-naphthalenyl)ethanone (54464-57-2)

	Partition coefficient n-octanol/water (Log Pow)
	5.65 (at 30°C)



	Bis(2-ethylhexyl) adipate (103-23-1)

	BCF - Fish [1]
	(27 dimensionless)

	Partition coefficient n-octanol/water (Log Pow)
	8.94 (at 25 °C)



	Benzyl acetate (140-11-4)

	Partition coefficient n-octanol/water (Log Pow)
	1.96 (at 25 °C (at pH 7)



	Sandal Mysore Core (28219-60-5)

	Partition coefficient n-octanol/water (Log Pow)
	3.8



	Triplal (Vertocitral) (68039-49-6)

	Partition coefficient n-octanol/water (Log Pow)
	2.6



	Cinnamic aldehyde (104-55-2)

	Partition coefficient n-octanol/water (Log Pow)
	2.1065 (at 25 °C)



	Diphenyl oxide (101-84-8)

	BCF - Fish [1]
	(470 dimensionless)

	Partition coefficient n-octanol/water (Log Pow)
	4.21 (at 25 °C)



	1,2-Propanediol (57-55-6)

	BCF - Fish [1]
	(1 dimensionless)

	Partition coefficient n-octanol/water (Log Pow)
	-1.07 (at 20.5 °C (at pH >=6.2-<=6.4)



	Glycerine (56-81-5)

	BCF - Fish [1]
	(no bioaccumulation)

	Partition coefficient n-octanol/water (Log Pow)
	-1.75 (at 25 °C (at pH 7.4)



	2-phenoxyethanol (122-99-6)

	Partition coefficient n-octanol/water (Log Pow)
	1.107



	acetophenone (98-86-2)

	Partition coefficient n-octanol/water (Log Pow)
	1.63 – 1.65


12.4. Mobility in soil
No additional information available
12.5. Results of PBT and vPvB assessment
No additional information available
12.6. Endocrine disrupting properties
[bookmark: _Hlk54090163]No additional information available
12.7. Other adverse effects
	NEROLI SANTAL #EU55411F 10% in DPG 

	Other information
	Avoid release to the environment.


SECTION 13: Disposal considerations
13.1. Waste treatment methods
	Product/Packaging disposal recommendations
	:
	Dispose in a safe manner in accordance with local/national regulations.

	Ecological waste information
	:
	Avoid release to the environment.

	HP Code
	:
	HP14 - “Ecotoxic:” waste which presents or may present immediate or delayed risks for one or more sectors of the environment


SECTION 14: Transport information
In accordance with ADR / IMDG / IATA / ADN / RID
	ADR
	IMDG
	IATA
	ADN
	RID

	14.1. UN number or ID number

	Not applicable
	Not applicable
	Not applicable
	Not applicable
	Not applicable

	14.2. UN proper shipping name

	Not applicable
	Not applicable
	Not applicable
	Not applicable
	Not applicable

	14.3. Transport hazard class(es)

	Not applicable
	Not applicable
	Not applicable
	Not applicable
	Not applicable

	14.4. Packing group

	Not applicable
	Not applicable
	Not applicable
	Not applicable
	Not applicable

	14.5. Environmental hazards

	Not applicable
	Not applicable
	Not applicable
	Not applicable
	Not applicable

	No supplementary information available


14.6. Special precautions for user
	Overland transport

	Not applicable



	Transport by sea

	Not applicable



	Air transport

	Not applicable



	Inland waterway transport

	Not applicable



	Rail transport

	Not applicable


14.7. Maritime transport in bulk according to IMO instruments
Not applicable
SECTION 15: Regulatory information
15.1. Safety, health and environmental regulations/legislation specific for the substance or mixture
EU-Regulations
REACH Annex XVII (Restriction List)
	EU restriction list (REACH Annex XVII)

	Reference code
	Applicable on
	Entry title or description

	3(a)
	Carrot seed oil
	Substances or mixtures fulfilling the criteria for any of the following hazard classes or categories set out in Annex I to Regulation (EC) No 1272/2008: Hazard classes 2.1 to 2.4, 2.6 and 2.7, 2.8 types A and B, 2.9, 2.10, 2.12, 2.13 categories 1 and 2, 2.14 categories 1 and 2, 2.15 types A to F

	3(b)
	NEROLI SANTAL #EU55411F 10% in DPG ; 1-(1,2,3,4,5,6,7,8-Octahydro-2,3,8,8-tetramethyl-2-naphthalenyl)ethanone ; Sandal Mysore Core ; Carrot seed oil ; Triplal (Vertocitral) ; Cinnamic aldehyde ; Phenoxyethanol ; Acetophenone
	Substances or mixtures fulfilling the criteria for any of the following hazard classes or categories set out in Annex I to Regulation (EC) No 1272/2008: Hazard classes 3.1 to 3.6, 3.7 adverse effects on sexual function and fertility or on development, 3.8 effects other than narcotic effects, 3.9 and 3.10

	3(c)
	NEROLI SANTAL #EU55411F 10% in DPG ; 1-(1,2,3,4,5,6,7,8-Octahydro-2,3,8,8-tetramethyl-2-naphthalenyl)ethanone ; Benzyl acetate ; Sandal Mysore Core ; Carrot seed oil ; Triplal (Vertocitral) ; Cinnamic aldehyde
	Substances or mixtures fulfilling the criteria for any of the following hazard classes or categories set out in Annex I to Regulation (EC) No 1272/2008: Hazard class 4.1


REACH Annex XIV (Authorisation List)
Contains no substance(s) listed on REACH Annex XIV (Authorisation List)
REACH Candidate List (SVHC)
Contains no substance(s) listed on the REACH Candidate List
PIC Regulation (Prior Informed Consent)
Contains no substance(s) listed on the PIC list (Regulation EU 649/2012 concerning the export and import of hazardous chemicals)
POP Regulation (Persistent Organic Pollutants)
Contains no substance(s) listed on the POP list (Regulation EU 2019/1021 on persistent organic pollutants)
Ozone Regulation (2024/590)
Contains no substance(s) listed on the Ozone Depletion list (Regulation EU 2024/590 on substances that deplete the ozone layer)
Council Regulation (EC) for the control of dual-use items
Contains no substance subject to the COUNCIL REGULATION (EC) for the control of dual-use items
Explosives Precursors Regulation (EU 2019/1148)
Contains no substance(s) listed on the Explosives Precursors list (Regulation EU 2019/1148 on the marketing and use of explosives precursors)
Drug Precursors Regulation (EC 273/2004)
Contains no substance(s) listed on the Drug Precursors list (Regulation EC 273/2004 on the manufacture and the placing on market of certain substances used in the illicit manufacture of narcotic drugs and psychotropic substances)
National regulations
	Austria

	Toxic Substances Ordinance 2000
	:
	Is not subject to the Toxic Substances Ordinance 2000.

	France

		Occupational diseases

	Code
	Description

	RG 84
	Conditions caused by liquid organic solvents for professional use: saturated or unsaturated aliphatic or cyclic liquid hydrocarbons and mixtures thereof; liquid halogenated hydrocarbons; nitrated derivatives of aliphatic hydrocarbons; alcohols; glycols, glycol ethers; ketones; aldehydes; aliphatic and cyclic ethers, including tetrahydrofuran; esters; dimethylformamide and dimethylacetamine; acetonitrile and propionitrile; pyridine; dimethylsulfone and dimethylsulfoxide




	Germany

	VOC ordinance (ChemVOCFarbV)
	:
	

	

	Water hazard class (WGK)
	:
	WGK 2, Significantly hazardous to water (Classification according to AwSV, Annex 1).

	List of sensitizing substances (TRGS 907)
	:
	Contains sensitizing substances according TRGS 907.

	Major Accidents Ordinance (12. BImSchV)
	:
	Is not subject to the Major Accidents Ordinance (12. BImSchV)

	Netherlands

	ABM category
	:
	A(3) - hazardous for aquatic organisms, may have longterm hazardous effects in aquatic environment

	SZW-lijst van kankerverwekkende stoffen
	:
	Triplal (Vertocitral) is listed

	SZW-lijst van mutagene stoffen
	:
	Triplal (Vertocitral) is listed

	SZW-lijst van reprotoxische stoffen – Borstvoeding
	:
	None of the components are listed

	SZW-lijst van reprotoxische stoffen – Vruchtbaarheid
	:
	None of the components are listed

	SZW-lijst van reprotoxische stoffen – Ontwikkeling
	:
	None of the components are listed

	Denmark

	Classification remarks
	:
	Emergency management guidelines for the storage of flammable liquids must be followed

	Danish National Regulations
	:
	Young people below the age of 18 years are not allowed to use the product
Pregnant/breastfeeding women working with the product must not be in direct contact with the product

	Poland

	Polish National Regulations
	:
	Act of 25 February 2011 on chemical substances and their mixtures (J. o L. No. 63, item 322 as amended; consolidated text J. o L. 2019, item 1225).
Act of 14 December 2012 on waste (J. o L. 2013, item 322 as amended; consolidated text J. o L. 2020, item 797).
The announcement of Marshal of the Sejm of the Republic of Poland dated 19 October 2016 concerning the consolidated text announcement of the decree on the management of packaging and packaging waste (J. o L. 2016, item 1863 as amended).
Decree of the Minister of Environment of 14 December 2014 on the catalogue of waste (J. o L. 2014, item 1923).
Act of 19 August 2011 on the Carriage of Dangerous Goods (J. o L. 2011 No. 227, item 1367 as amended; consolidated text J. o L. 2020, item 154).
Regulation of the Minister of Family, Labour and Social Policy of 12 June 2018 on the highest permissible concentration and intensity of noxious agents for health at work environment (J. o L. item 1286 as amended).
The announcement of Minister of Health dated 9 September 2016 concerning the consolidated text announcement of the decree of the Minister of Health of 30 December 2004 on health and safety at work related to exposure to chemical agents at work (J. o L. of 16 September 2016, item 1488)
Regulation of the Minister of Health of 2 February 2011 on tests and measurements of the noxious agents for health at work environment (J. o L. No. 33, item 166 as amended).
Regulation of the Minister of Environment of 9 December 2003 on particularly hazardous substances to the environment (J. o L. No. 217, item 2141).
ADR Agreement: Government Statement of 13 March 2023 on the entry into force of amendments to Annexes A and B to the Agreement concerning the International Carriage of Dangerous Goods by Road (ADR), signed in Geneva on 30 September 1957 (J. o. L. 2023, item 891)
Regulation of the Minister of Health of 25 August 2015 on the method of marking places, pipelines, and containers and tanks used for storing or containing hazardous substances or hazardous mixtures (J.o.L. 2015, item 1368 as ammended)


15.2. Chemical safety assessment
No chemical safety assessment has been carried out
SECTION 16: Other information
	Data sources
	:
	REGULATION (EC) No 1272/2008 OF THE EUROPEAN PARLIAMENT AND OF THE COUNCIL of 16 December 2008 on classification, labelling and packaging of substances and mixtures, amending and repealing Directives 67/548/EEC and 1999/45/EC, and amending Regulation (EC) No 1907/2006.

	Other information
	:
	None.



	Full text of H- and EUH-statements:

	Acute Tox. 4 (Dermal)
	Acute toxicity (dermal), Category 4

	Acute Tox. 4 (Oral)
	Acute toxicity (oral), Category 4

	Aquatic Acute 1
	Hazardous to the aquatic environment – Acute Hazard, Category 1

	Aquatic Chronic 1
	Hazardous to the aquatic environment – Chronic Hazard, Category 1

	Aquatic Chronic 2
	Hazardous to the aquatic environment – Chronic Hazard, Category 2

	Aquatic Chronic 3
	Hazardous to the aquatic environment – Chronic Hazard, Category 3

	Asp. Tox. 1
	Aspiration hazard, Category 1

	EUH208
	Contains {0|message≤name of sensitising substance>|fieldvalue=_SENSITIZER_COMPONENTS}. May produce an allergic reaction.

	Eye Dam. 1
	Serious eye damage/eye irritation, Category 1

	Eye Irrit. 2
	Serious eye damage/eye irritation, Category 2

	Flam. Liq. 3
	Flammable liquids, Category 3

	Skin Irrit. 2
	Skin corrosion/irritation, Category 2

	Skin Sens. 1
	Skin sensitisation, Category 1

	Skin Sens. 1A
	Skin sensitisation, category 1A

	STOT SE 3
	Specific target organ toxicity – Single exposure, Category 3, Respiratory tract irritation

	H226
	Flammable liquid and vapour.

	H302
	Harmful if swallowed.

	H304
	May be fatal if swallowed and enters airways.

	H312
	Harmful in contact with skin.

	H315
	Causes skin irritation.

	H317
	May cause an allergic skin reaction.

	H318
	Causes serious eye damage.

	H319
	Causes serious eye irritation.

	H335
	May cause respiratory irritation.

	H400
	Very toxic to aquatic life.

	H410
	Very toxic to aquatic life with long lasting effects.

	H411
	Toxic to aquatic life with long lasting effects.

	H412
	Harmful to aquatic life with long lasting effects.



	The classification complies with
	:
	ATP 12


Safety Data Sheet (SDS), EU
This information is based on our current knowledge and is intended to describe the product for the purposes of health, safety and environmental requirements only. It should not therefore be construed as guaranteeing any specific property of the product.
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